RADLAN-QOS-SERV DEFINITIONS ::= BEGIN

-- Version:    7.39_10_00
-- Date:       31 May 2005
--
-- 22-Dec-2003 Add scalar rlQosServMibAction.
-- 12-Jan-2004 Change the index to name table to be read-write and
--             add rlQosServMibAction value 'noImportPolicy'.
-- 26-Jan-2004 Split Template's and FCE's TCP and UDP port fields onto
--             sperate ones.
-- 18-Jan-2005 RevitalM
--             1. Merge Template's and FCE's TCP and UDP port fields into one field for both profiles.
--             2. Add two service types: committedBoundBW and trust.
-- 25-Jan-2005 LiorM
--             1. Add VPT, Ethertype,ICMP code , ICMP type , IGMP Type and TCP flags to template and FCE
-- 20-Feb-2005 GalitV
--             1. Add rlQosServFceVptMask, rlQosServFceTcpFlagsMask
-- 29-May-2005 RevitalM
--             1. Change default value of rlQosServFceEtherType to 1501 (=minimum value for etherType)

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32,
    IpAddress                                   FROM SNMPv2-SMI
    InterfaceIndex                              FROM IF-MIB
    RowStatus, TruthValue                       FROM RADLAN-SNMPv2
    TEXTUAL-CONVENTION, DisplayString,
    MacAddress                                  FROM SNMPv2-TC
    PortList                                    FROM Q-BRIDGE-MIB
    rnd                                         FROM RADLAN-MIB;

rlQosServ MODULE-IDENTITY
      LAST-UPDATED "200308280024Z"  -- August 28, 2003
      ORGANIZATION "Radlan Computer Communication Ltd."
      CONTACT-INFO
              "radlan.com"
      DESCRIPTION
              "The MIB module describes the private MIB for QOS service mode."
      REVISION     "200310280024Z"  -- October 28, 2003
      DESCRIPTION
              "Initial revision"
      ::= { rnd 99 }

RlQosServServiceStatus ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of service statuses"
    SYNTAX  INTEGER {
        active(1),
        suspended(2)
    }

RlQosServNamedTableId  ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Specifies one of the named tables Id"
    SYNTAX INTEGER {
        fcl(1),
        fce(2),
        profile(3)
    }


 -- QoS Template Table

rlQosServTemplateTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServTemplateEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies classification template information.
         Currently this table will contain exactly one entry."
    ::= { rlQosServ 1 }

rlQosServTemplateEntry OBJECT-TYPE
    SYNTAX RlQosServTemplateEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The entry of this table describes all classifier fields.
         The index is sequential integer represent by rlQosServTemplateEntry."
    INDEX { rlQosServTemplateIndex }
    ::= { rlQosServTemplateTable 1 }

RlQosServTemplateEntry::= SEQUENCE {
    rlQosServTemplateIndex                  INTEGER,
    rlQosServTemplateDestMac                TruthValue,
    rlQosServTemplateDestMacMask            MacAddress,
    rlQosServTemplateSrcMac                 TruthValue,
    rlQosServTemplateSrcMacMask             MacAddress,
    rlQosServTemplateVlan                   TruthValue,
    rlQosServTemplateDestIp                 TruthValue,
    rlQosServTemplateDestIpMask             IpAddress,
    rlQosServTemplateSrcIp                  TruthValue,
    rlQosServTemplateSrcIpMask              IpAddress,
    rlQosServTemplateIpProtocol             TruthValue,
    rlQosServTemplateSrcPort                TruthValue,
    rlQosServTemplateDestPort               TruthValue,
    rlQosServTemplateTos                    TruthValue,
    rlQosServTemplateVpt                    TruthValue,
    rlQosServTemplateEtherType              TruthValue,
    rlQosServTemplateTcpFlags               TruthValue,
    rlQosServTemplateIcmpType               TruthValue,
    rlQosServTemplateIcmpCode               TruthValue,
    rlQosServTemplateIgmpType               TruthValue
}

rlQosServTemplateIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary index for the template table."
    ::= { rlQosServTemplateEntry 1 }

rlQosServTemplateDestMac OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the destination Mac field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 2 }

rlQosServTemplateDestMacMask OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Destination Mac address mask. It may specify any byte (not bit),
         within the Mac address, for classification, designated by 0."
--    DEFVAL { '000000000000'H }
    ::= { rlQosServTemplateEntry 3 }

rlQosServTemplateSrcMac OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the source Mac field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 4 }

rlQosServTemplateSrcMacMask OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Source Mac address mask. It may specify any byte (not bit),
         within the Mac address, for classification, designated by 0."
--    DEFVAL { '000000000000'H }
    ::= { rlQosServTemplateEntry 5 }

rlQosServTemplateVlan OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Vlan field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 6 }

rlQosServTemplateDestIp OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the destination Ip field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 7 }

rlQosServTemplateDestIpMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Destination Ip address mask. It may specify any byte (not bit),
         within the Ip address, for classification, designated by 0."
    DEFVAL { '00000000'H }
    ::= { rlQosServTemplateEntry 8 }

rlQosServTemplateSrcIp OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the source Ip field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 9 }

rlQosServTemplateSrcIpMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Source Ip address mask. It may specify any byte (not bit),
         within the Ip address, for classification, designated by 0."
    DEFVAL { '00000000'H }
    ::= { rlQosServTemplateEntry 10 }

rlQosServTemplateIpProtocol OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Ip protocol field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 11 }

rlQosServTemplateSrcPort OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Tcp/Udp source port field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 12 }

rlQosServTemplateDestPort OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Tcp/Udp destination port field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 13 }

rlQosServTemplateTos OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Tos field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 14 }

rlQosServTemplateVpt OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the VPT field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 15 }

rlQosServTemplateEtherType OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Ether Type field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 16 }

rlQosServTemplateTcpFlags OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Tcp flags (Control Bits) field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 17 }

rlQosServTemplateIcmpType OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Icmp type field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 18 }

rlQosServTemplateIcmpCode OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Icmp code field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 19 }

rlQosServTemplateIgmpType OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Include the Igmp type field as a template classifier."
    DEFVAL { false }
    ::= { rlQosServTemplateEntry 20 }

-- QoS FCL (Flow Classification List) table

rlQosServFclTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServFclEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies FCL table information"
    ::= { rlQosServ 2 }

rlQosServFclEntry OBJECT-TYPE
    SYNTAX RlQosServFclEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one Flow Classification List with
         It's Flow Classification Element.
         The information includes the FCL index and reference to a FCE index.
         The indices are the Fcl index represent by rlQosServFclIndex and the
         Fce index represent by rlQosServFclFceIndex."
    INDEX { rlQosServFclIndex,
            rlQosServFclFcePriority }
    ::= { rlQosServFclTable 1 }

RlQosServFclEntry::= SEQUENCE {
    rlQosServFclIndex           INTEGER,
    rlQosServFclFcePriority     INTEGER,
    rlQosServFclFceIndex        INTEGER,
    rlQosServFclStatus          RowStatus
}

rlQosServFclIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary index for the FCL table. Value '0' is invalid."
    ::= { rlQosServFclEntry 1 }

rlQosServFclFcePriority OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Priority of the FCE within the FCL."
    ::= { rlQosServFclEntry 2 }

rlQosServFclFceIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "A reference to the FCE index."
    ::= { rlQosServFclEntry 3 }

rlQosServFclStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosServFclEntry 4 }


-- QoS FCE (Flow Classification Element) table

rlQosServFceTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServFceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies FCE table information"
    ::= { rlQosServ 3 }

rlQosServFceEntry OBJECT-TYPE
    SYNTAX RlQosServFceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one Flow Classifier Element.
         The information includes ACE index and a combination of all the other
         classifications, as depicted in the selection field.
         Classifiers are Mac and Ip source and destination addresses, Vlan,
         Ip protocol, TCP & UDP source and destination ports, Dscp and Ip
         precedence values.
         The index is a sequential integer represent by rlQosServFceIndex."
    INDEX { rlQosServFceIndex }
    ::= { rlQosServFceTable 1 }

RlQosServFceEntry::= SEQUENCE {
    rlQosServFceIndex               INTEGER,
    rlQosServFceErrorCode           INTEGER,
    rlQosServFceSelection           BITS,
    rlQosServFceDestMac             MacAddress,
    rlQosServFceDestMacMask         MacAddress,
    rlQosServFceSrcMac              MacAddress,
    rlQosServFceSrcMacMask          MacAddress,
    rlQosServFceVlan                INTEGER,
    rlQosServFceVlanMask            INTEGER,
    rlQosServFceDestIp              IpAddress,
    rlQosServFceDestIpMask          IpAddress,
    rlQosServFceSrcIp               IpAddress,
    rlQosServFceSrcIpMask           IpAddress,
    rlQosServFceIpProtocol          INTEGER,
    rlQosServFceDestPort            INTEGER,
    rlQosServFceDestPortMask        INTEGER,
    rlQosServFceSrcPort             INTEGER,
    rlQosServFceSrcPortMask         INTEGER,
    rlQosServFceDscp                INTEGER,
    rlQosServFceIpPrecedence        INTEGER,
    rlQosServFceVpt                 INTEGER,
    rlQosServFceVptMask             INTEGER,
    rlQosServFceEtherType           INTEGER,
    rlQosServFceTcpFlags            INTEGER,
    rlQosServFceTcpFlagsMask        INTEGER,
    rlQosServFceIcmpType            INTEGER,
    rlQosServFceIcmpCode            INTEGER,
    rlQosServFceIgmpType            INTEGER,
    rlQosServFceStatus              RowStatus
}

rlQosServFceIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary incremental Index for the Fce table."
    ::= { rlQosServFceEntry 1 }

rlQosServFceErrorCode OBJECT-TYPE
    SYNTAX INTEGER {
         noError(1),
         noTemplate(2)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Fce error code."
    DEFVAL { noError }
    ::= { rlQosServFceEntry 2 }

rlQosServFceSelection OBJECT-TYPE
    SYNTAX BITS {
         macDestAddr(0),
         macSrcAddr(1),
         vlan(2),
         ipDestAddr(3),
         ipSrcAddr(4),
         ipProtocol(5),
         destPort(6),
         srcPort(7),
         dscp(8),
         ipPrecedence(9),
         vpt(10),
         etherType(11),
         tcpFlags(12),
         icmpType(13),
         icmpCode(14),
         igmpType(15)
         }

    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Flow Classification Elements selection."
    ::= { rlQosServFceEntry 3 }

rlQosServFceDestMac OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the destination Mac address to compare with."
--    DEFVAL { '000000000000'H }
    ::= { rlQosServFceEntry 4 }

rlQosServFceDestMacMask OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the destination Mac address mask to compare with.
         It may specify any byte (not bit), designated by 0."
--    DEFVAL { '000000000000'H }
    ::= { rlQosServFceEntry 5 }

rlQosServFceSrcMac OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the source Mac address to compare with."
--    DEFVAL { '000000000000'H }
    ::= { rlQosServFceEntry 6 }

rlQosServFceSrcMacMask OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the source Mac address mask to compare.
         It may specify any byte (not bit), designated by 0."
--    DEFVAL { '000000000000'H }
    ::= { rlQosServFceEntry 7 }

rlQosServFceVlan OBJECT-TYPE
    SYNTAX INTEGER(0..4095)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Vlan to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 8 }

rlQosServFceVlanMask OBJECT-TYPE
    SYNTAX INTEGER(0..4095)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates 12-bits Vlan bits to compare.
         It may specify any byte (not bit), designated by 0."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 9 }

rlQosServFceDestIp OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the destination Ip address to compare with."
    DEFVAL { '00000000'H }
    ::= { rlQosServFceEntry 10 }

rlQosServFceDestIpMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the destination Ip address mask to compare.
         It may specify any byte (not bit), designated by 0."
    DEFVAL { '00000000'H }
    ::= { rlQosServFceEntry 11 }

rlQosServFceSrcIp OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the source Ip address to compare with."
    DEFVAL { '00000000'H }
    ::= { rlQosServFceEntry 12 }

rlQosServFceSrcIpMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the source Ip address mask to compare.
         It may specify any byte (not bit), designated by 0."
    DEFVAL { '00000000'H }
    ::= { rlQosServFceEntry 13 }

rlQosServFceIpProtocol OBJECT-TYPE
    SYNTAX INTEGER(0..255)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Ip protocol to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 14 }

rlQosServFceDestPort OBJECT-TYPE
    SYNTAX INTEGER(0..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the TCP/UDP destination port to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 15 }

rlQosServFceDestPortMask OBJECT-TYPE
    SYNTAX INTEGER(0..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates 16-bits TCP/UDP destination port bits to compare.
         It may specify any byte (not bit), designated by 0."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 16 }

rlQosServFceSrcPort OBJECT-TYPE
    SYNTAX INTEGER(0..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the TCP/UDP source port to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 17 }

rlQosServFceSrcPortMask OBJECT-TYPE
    SYNTAX INTEGER(0..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates 16-bits TCP/UDP source port bits to compare.
         It may specify any byte (not bit), designated by 0."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 18 }

rlQosServFceDscp OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Destination Mac address to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 19 }

rlQosServFceIpPrecedence OBJECT-TYPE
    SYNTAX INTEGER(0..7)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Ip precedence to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 20 }

rlQosServFceVpt OBJECT-TYPE
    SYNTAX INTEGER(0..7)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the VPT to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 21 }

rlQosServFceVptMask OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the VPT mask to compare with.
         It may specify any bit, designated by 0."
--    DEFVAL { 0 }
    ::= { rlQosServFceEntry 22 }

rlQosServFceEtherType OBJECT-TYPE
    SYNTAX INTEGER(1501..65536)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicate the Ether Type to compare with."
    DEFVAL { 1501 }
    ::= { rlQosServFceEntry 23 }

rlQosServFceTcpFlags OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Tcp Flags field to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 24 }

    rlQosServFceTcpFlagsMask OBJECT-TYPE
    SYNTAX INTEGER(0..63)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Tcp Flags field to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 25 }

rlQosServFceIcmpType OBJECT-TYPE
    SYNTAX INTEGER(0..255)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Icmp type to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 26 }

    rlQosServFceIcmpCode OBJECT-TYPE
    SYNTAX INTEGER(0..255)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Icmp code to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 27 }

rlQosServFceIgmpType OBJECT-TYPE
    SYNTAX INTEGER(0..255)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Indicates the Igmp type to compare with."
    DEFVAL { 0 }
    ::= { rlQosServFceEntry 28 }

rlQosServFceStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of this table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosServFceEntry 29 }


-- QoS profile table

rlQosServProfileTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies (service) profile table information"
    ::= { rlQosServ 4 }

rlQosServProfileEntry OBJECT-TYPE
    SYNTAX RlQosServProfileEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one service profile element.
         The information includes: Profile name, type and various numeric
         parameters associated with the profile's service types.
         The index is sequential integer represent by rlQosServProfileIndex."
    INDEX { rlQosServProfileIndex }
    ::= { rlQosServProfileTable 1 }

RlQosServProfileEntry::= SEQUENCE {
    rlQosServProfileIndex               INTEGER,
    rlQosServProfileType                INTEGER,
    rlQosServProfileServiceType         INTEGER,
    rlQosServProfileIngressBurstSize    Unsigned32,
    rlQosServProfileMaxBandwidth        Unsigned32,
    rlQosServProfileMinBandwidth        Unsigned32,
    rlQosServProfileMaxDelay            Unsigned32,
    rlQosServProfileStatus              RowStatus
    }

rlQosServProfileIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary index for the profile table."
    ::= { rlQosServProfileEntry 1 }

rlQosServProfileType OBJECT-TYPE
    SYNTAX INTEGER {
        regular(1),
        aggregate(2)
    }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Profile's type"
    DEFVAL{ regular }
    ::= { rlQosServProfileEntry 2 }

rlQosServProfileServiceType OBJECT-TYPE
    SYNTAX INTEGER {
        bestEffort(1),
        minDelay(2),
        committedDelay(3),
        minMaxBandwidth(4),
        committedBoundBandwidth(5),
        rateLimit(6),
        trustCos(7),
        trustDscp(8),
        trust(9),
        drop(10),
        dropAndDisablePort(11)

    }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Profile's service type."
    DEFVAL{ bestEffort }
    ::= { rlQosServProfileEntry 3 }

rlQosServProfileIngressBurstSize OBJECT-TYPE
    SYNTAX Unsigned32(0..1000000)
    UNITS   "bytes"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Profile's Ingress Burst Size, used only by the 'rate limit' service."
    DEFVAL{ 3000 }
    ::= { rlQosServProfileEntry 4 }

rlQosServProfileMaxBandwidth OBJECT-TYPE
    SYNTAX Unsigned32(0..10000000)
    UNITS   "bytes"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Profile's Max Bandwidth, used by the 'min delay', committed delay'
         'min max bandwidth' and committed Bound Bandwidth'services.
         Value 0 is used only as default value, and is invalid otherwise."
    DEFVAL{ 0 }
    ::= { rlQosServProfileEntry 5 }

rlQosServProfileMinBandwidth OBJECT-TYPE
    SYNTAX Unsigned32(0..10000000)
    UNITS   "bytes"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Profile's Min Bandwidth, used only by the 'min max bandwidth'
         service.
         Value 0 is used only as default value, and is invalid otherwise."
    DEFVAL{ 0 }
    ::= { rlQosServProfileEntry 6 }

rlQosServProfileMaxDelay  OBJECT-TYPE
    SYNTAX Unsigned32
    UNITS "milliseconds"
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Profile's Max Delay, used only by the 'committed delay' service.
         Value 0 is used only as default value, and is invalid otherwise."
    DEFVAL{ 0 }
    ::= { rlQosServProfileEntry 7 }

rlQosServProfileStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosServProfileEntry 8 }


-- QoS service table

rlQosServServiceTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServServiceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies service table information."
    ::= { rlQosServ 5 }

rlQosServServiceEntry OBJECT-TYPE
    SYNTAX RlQosServServiceEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one service profile element.
        The information includes: service's index, priority, pointers to
        associated profile and Fcl, operational and administrative statuses,
        ingress and egress interface lists, and two operational parameter
        values associated with a service type, as defined in the profile table.
        The index is sequential integer represent by rlQosServServiceIndex."
    INDEX { rlQosServServiceIndex }
    ::= { rlQosServServiceTable 1 }

RlQosServServiceEntry::= SEQUENCE {
    rlQosServServiceIndex               INTEGER,
    rlQosServServicePriority            Unsigned32,
    rlQosServServiceProfilePointer      INTEGER,
    rlQosServServiceFclPointer          INTEGER,
    rlQosServServiceInIfList            PortList,
    rlQosServServiceOutIfList           PortList,
    rlQosServServiceScaledOutIfList     PortList,
    rlQosServServiceProfileParamOper    Unsigned32,
    rlQosServServiceStatusOper          RlQosServServiceStatus,
    rlQosServServiceStatusAdmin         RlQosServServiceStatus,
    rlQosServServiceStatus              RowStatus
}

rlQosServServiceIndex OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An arbitrary index for the service table."
    ::= { rlQosServServiceEntry 1 }

rlQosServServicePriority OBJECT-TYPE
    SYNTAX Unsigned32(1..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Service's priority."
    ::= { rlQosServServiceEntry 2 }

rlQosServServiceProfilePointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Pointer to attached profile entry."
    ::= { rlQosServServiceEntry 3 }

rlQosServServiceFclPointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Pointer to attached FCL entry."
    ::= { rlQosServServiceEntry 4 }

rlQosServServiceInIfList OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Ingress interface list associated with this service entry."
    ::= { rlQosServServiceEntry 5 }

rlQosServServiceOutIfList OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Egress interface list associated with this service entry."
    ::= { rlQosServServiceEntry 6 }

rlQosServServiceScaledOutIfList OBJECT-TYPE
    SYNTAX PortList
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Egress scaled interface list associated with this service entry."
    ::= { rlQosServServiceEntry 7 }

rlQosServServiceProfileParamOper OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "If the service type specified in a profile associated with this entry
         has a parameter, this object instance specifies the parameter's
         operative value.
         This value will be different from the value defined in the associated
         profile only in case of scaling out, otherwise value 0 is used."
    ::= { rlQosServServiceEntry 8 }

rlQosServServiceStatusOper  OBJECT-TYPE
    SYNTAX RlQosServServiceStatus
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Operational value of the service status."
    ::= { rlQosServServiceEntry 9 }

rlQosServServiceStatusAdmin  OBJECT-TYPE
    SYNTAX RlQosServServiceStatus
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Administrative value of the service status."
    DEFVAL{ suspended }
    ::= { rlQosServServiceEntry 10 }

rlQosServServiceStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosServServiceEntry 11 }


-- QoS service priority table

rlQosServServicePriorityTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServServicePriorityEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies service priority table information."
    ::= { rlQosServ 6 }

rlQosServServicePriorityEntry OBJECT-TYPE
    SYNTAX RlQosServServicePriorityEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table maps a priority to a service.
        The information includes: service's priority and the service index
        in the service table.
        The index is sequential integer represent by
        rlQosServServicePriorityIndex."
    INDEX { rlQosServServicePriorityIndex }
    ::= { rlQosServServicePriorityTable 1 }

RlQosServServicePriorityEntry::= SEQUENCE {
    rlQosServServicePriorityIndex       INTEGER,
    rlQosServServicePriorityPointer     INTEGER
}

rlQosServServicePriorityIndex OBJECT-TYPE
    SYNTAX INTEGER(1..65535)
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The service priority."
    ::= { rlQosServServicePriorityEntry 1 }

rlQosServServicePriorityPointer OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The index of the service associated with this priority in the service
         table."
    ::= { rlQosServServicePriorityEntry 2 }


--  QoS service type DSCP and VPT default mapping

rlQosServServiceDefaultMappingTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServServiceDefaultMappingEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies service priority table information."
    ::= { rlQosServ 7 }

rlQosServServiceDefaultMappingEntry OBJECT-TYPE
    SYNTAX RlQosServServiceDefaultMappingEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table describes one service priority entry.
        The information includes: service's priority, a pointer to its
        corresponding index in the service table.
        The index is sequential integer represent by
        rlQosServServicePriorityIndex."
    INDEX { rlQosServServiceDefaultMappingType }
    ::= { rlQosServServiceDefaultMappingTable 1 }

RlQosServServiceDefaultMappingEntry::= SEQUENCE {
    rlQosServServiceDefaultMappingType      INTEGER,
    rlQosServServiceDefaultMappingDscp      INTEGER,
    rlQosServServiceDefaultMappingVpt       INTEGER
}

rlQosServServiceDefaultMappingType OBJECT-TYPE
    SYNTAX INTEGER {
        bestEffort(1),
        minDelay(2),
        committedDelay(3),
        minMaxBandwidth(4),
        committedBoundBandwidth(5),
        rateLimit(6),
        trustDscp(7)
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Service type for the default mapping.
         'Trust DSCP' service type is absent since no default mapping
         is possible for it."
    ::= { rlQosServServiceDefaultMappingEntry 1 }

rlQosServServiceDefaultMappingDscp OBJECT-TYPE
    SYNTAX INTEGER (0..64)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "DSCP default mapping value.
         A value of 64 means no DSCP default mapping is done."
    ::= { rlQosServServiceDefaultMappingEntry 2 }

rlQosServServiceDefaultMappingVpt OBJECT-TYPE
    SYNTAX INTEGER (0..8)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Vpt default mapping value.
         A value of 9 means no VPT default mapping is done."
    ::= { rlQosServServiceDefaultMappingEntry 3 }

--  QoS scaling error table

rlQosServScalingErrorTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServScalingErrorEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "This table specifies scaling error table"
    ::= { rlQosServ 8 }

rlQosServScalingErrorEntry OBJECT-TYPE
    SYNTAX RlQosServScalingErrorEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Each entry in this table specifies for each interface its scaling
        error, if such indeed exists."
    INDEX { rlQosServScalingErrorIfIndex }
    ::= { rlQosServScalingErrorTable 1 }

RlQosServScalingErrorEntry::= SEQUENCE {
        rlQosServScalingErrorIfIndex        InterfaceIndex,
        rlQosServScalingErrorReason         INTEGER
}

rlQosServScalingErrorIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The interface index."
    ::= { rlQosServScalingErrorEntry 1 }

rlQosServScalingErrorReason OBJECT-TYPE
    SYNTAX INTEGER {
        changeSpeed-10000to1000(1),
        changeSpeed-10000to100(2),
        changeSpeed-10000to10(3),
        changeSpeed-1000to100(4),
        changeSpeed-1000to10(5),
        changeSpeed-100to10(6),
        changeSpeed-10to100(7),
        changeSpeed-10to1000(8),
        changeSpeed-10to10000(9),
        changeSpeed-100to1000(10),
        changeSpeed-100to10000(11),
        changeSpeed-1000to10000(12)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Scaling error reason."
    ::= { rlQosServScalingErrorEntry 2 }

-- QoS free sequential table

rlQosServFreeSequentialTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServFreeSequentialEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table is used to get free indices of tables to create
         new entries, and next free priorities.
         The algorithm for free indexes depends on table types:
         Fcl table        - first free index.
         Fce table        - first free index.
         Service table    - first free index.
         Service priority - last used priority + priority-delta.

         The priority-delta is used to supply QoS MIB user easy new priority
         insert entry capabilities.
         Values of these deltas depend on the MIB implementation.
         The 'Get and Increment' approach is used in all cases."
    ::= { rlQosServ 9 }

rlQosServFreeSequentialEntry OBJECT-TYPE
    SYNTAX RlQosServFreeSequentialEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The entry is used to get free index for particular table."
    INDEX  { rlQosServFreeSequentialId }
    ::= { rlQosServFreeSequentialTable 1 }

RlQosServFreeSequentialEntry ::= SEQUENCE  {
    rlQosServFreeSequentialId           INTEGER,
    rlQosServFreeSequentialValue        INTEGER
}

rlQosServFreeSequentialId OBJECT-TYPE
    SYNTAX INTEGER {
        fcl(1),
        fce(2),
        profile(3),
        service(4),
        priorityService(5)
    }
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Identification of the sequential, for which free indices or priority
         are retrieved."
    ::= { rlQosServFreeSequentialEntry 1 }

rlQosServFreeSequentialValue OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The free index for the table or service priority.
         Returned '0' means no free entries/priority."
    ::= { rlQosServFreeSequentialEntry 2 }

-- QoS name to index table

rlQosServNameToIndexTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServNameToIndexEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table is used to get specific table(s) indices from the name."
    ::= { rlQosServ 10 }

rlQosServNameToIndexEntry OBJECT-TYPE
    SYNTAX  RlQosServNameToIndexEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The entry is used to get index form particular name and table type."
    INDEX  {  rlQosServNameToIndexTableId,
              rlQosServNameToIndexName}
    ::= { rlQosServNameToIndexTable 1 }

RlQosServNameToIndexEntry ::= SEQUENCE  {
    rlQosServNameToIndexTableId      RlQosServNamedTableId,
    rlQosServNameToIndexName         DisplayString,
    rlQosServNameToIndexValue        INTEGER,
    rlQosServNameToIndexStatus       RowStatus
}

rlQosServNameToIndexTableId OBJECT-TYPE
    SYNTAX RlQosServNamedTableId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Identification of the table, for which the index is retrieved."
    ::= { rlQosServNameToIndexEntry 1 }

rlQosServNameToIndexName OBJECT-TYPE
    SYNTAX DisplayString(SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Name of the table's entry"
    ::= { rlQosServNameToIndexEntry 2 }

rlQosServNameToIndexValue OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The index of the table. Value '0' is invalid."
    ::= { rlQosServNameToIndexEntry 3 }

rlQosServNameToIndexStatus OBJECT-TYPE
    SYNTAX RowStatus
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
       "The status of a table entry.
        It is used to delete/Add an entry from this table."
    ::= { rlQosServNameToIndexEntry 4 }

-- QoS index to name table

rlQosServIndexToNameTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RlQosServIndexToNameEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table is used to get specific table(s) name from indices.
         It is a read-write table for internal (CDB) purpose only and is not to
         set by outside users."
    ::= { rlQosServ 11 }

rlQosServIndexToNameEntry OBJECT-TYPE
    SYNTAX  RlQosServIndexToNameEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The entry is used to get name form particular index and table type."
    INDEX  {  rlQosServIndexToNameTableId,
              rlQosServIndexToNameIndex}
    ::= { rlQosServIndexToNameTable 1 }

RlQosServIndexToNameEntry ::= SEQUENCE  {
    rlQosServIndexToNameTableId      RlQosServNamedTableId,
    rlQosServIndexToNameIndex        INTEGER,
    rlQosServIndexToNameValue        DisplayString
}

rlQosServIndexToNameTableId OBJECT-TYPE
    SYNTAX RlQosServNamedTableId
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Identification of the table, for which the name is retrieved."
    ::= { rlQosServIndexToNameEntry 1 }

rlQosServIndexToNameIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The index of the table. Value '0' is invalid."
    ::= { rlQosServIndexToNameEntry 2 }

rlQosServIndexToNameValue OBJECT-TYPE
    SYNTAX DisplayString(SIZE(1..32))
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Name of the table's entry"
    ::= { rlQosServIndexToNameEntry 3 }

-- QoS Mib version

rlQosServMibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 1.
         1 - original version.
         2- "
    ::= { rlQosServ 12 }

-- QoS Mib action

rlQosServMibAction OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        importPolicy(2),
        noImportPolicy(3),
        flatServicePriorities(4)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Actions to be performed by QoS service mode MIB."
    DEFVAL { none }
    ::= { rlQosServ 13 }

END
