ALCATEL-IND1-VRRP3-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        NOTIFICATION-TYPE, Counter32, 
        Integer32                           FROM SNMPv2-SMI

        RowStatus, MacAddress,
        TruthValue, TimeStamp               FROM SNMPv2-TC

        MODULE-COMPLIANCE, OBJECT-GROUP,
        NOTIFICATION-GROUP                  FROM SNMPv2-CONF
	softentIND1Vrrp                     FROM ALCATEL-IND1-BASE
        ifIndex                             FROM IF-MIB
        InetAddressType, InetAddress        FROM INET-ADDRESS-MIB

	VrId                                FROM VRRP-MIB;


alcatelIND1VRRP3MIB MODULE-IDENTITY
    LAST-UPDATED "200704030000Z"
    ORGANIZATION "Alcatel-Lucent"
    CONTACT-INFO
        "Please consult with Customer Service to ensure the most appropriate
         version of this document is used with the products in question:

                    Alcatel-Lucent, Enterprise Solutions Division
                   (Formerly Alcatel Internetworking, Incorporated)
                           26801 West Agoura Road
                        Agoura Hills, CA  91301-5122
                          United States Of America

        Telephone:               North America  +1 800 995 2696
                                 Latin America  +1 877 919 9526
                                 Europe         +31 23 556 0100
                                 Asia           +65 394 7933
                                 All Other      +1 818 878 4507

        Electronic Mail:         support@ind.alcatel.com
        World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
        File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

    DESCRIPTION
        "This module describes an authoritative enterprise-specific Simple
         Network Management Protocol (SNMP) Management Information Base (MIB):

             Proprietary VRRP MIB definitions for simultaneous 
             support of IPv4 and IPv6 protocols.

         The right to make changes in specification and other information
         contained in this document without prior notice is reserved.

         No liability shall be assumed for any incidental, indirect, special,
	       or consequential damages whatsoever arising from or related to this
         document or the information contained herein.

         Vendors, end-users, and other interested parties are granted
         non-exclusive license to use this specification in connection with
         management of the products for which it is intended to be used.

                     Copyright (C) 1995-2007 Alcatel-Lucent
                         ALL RIGHTS RESERVED WORLDWIDE"

    REVISION "200704030000Z"    -- 02 April 2007
    DESCRIPTION "The latest version of this MIB Module."

    ::= { softentIND1Vrrp 2 }



--
--  VRRP MIB Groups
--

alaVrrp3Operations  OBJECT IDENTIFIER ::= { alcatelIND1VRRP3MIB 1 }
alaVrrp3Statistics  OBJECT IDENTIFIER ::= { alcatelIND1VRRP3MIB 2 }
alaVrrp3Conformance OBJECT IDENTIFIER ::= { alcatelIND1VRRP3MIB 3 }

--
--  Start of MIB objects
--

alaVrrp3NotificationCntl  OBJECT-TYPE
    SYNTAX       INTEGER {
        enabled     (1),
        disabled    (2)
    }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates whether the VRRP-enabled router will generate
         SNMP traps for events defined in this MIB. 'Enabled'
         results in SNMP traps; 'disabled', no traps are sent."
    DEFVAL { enabled }
    ::= { alaVrrp3Operations 1 }

--
--  VRRP Operations Table
--

alaVrrp3OperTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF AlaVrrp3OperEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Unified Operations table for a VRRP router which
         consists of a sequence (i.e., one or more conceptual
         rows) of 'alaVrrp3OperEntry' items."
    ::= { alaVrrp3Operations 2 }

alaVrrp3OperEntry OBJECT-TYPE
    SYNTAX       AlaVrrp3OperEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "An entry in the alaVrrp3OperTable containing the
         operational characteristics of a virtual router. On a
         VRRP router, a given virtual router is identified by a
         combination of the IP version, VRID, and ifIndex.

         Note that rows in this table can be distinguished on a
         Multi-stacked device running both VRRP over IPv4 and
         IPv6 interfaces.

         Rows in the table cannot be modified unless the value
         of 'alaVrrp3OperAdminState' is 'disabled' and the
         'alaVrrp3OperState' has transitioned to
         'initialize'"

    INDEX    { alaVrrp3OperIpVersion, alaVrrp3OperVrId, 
               ifIndex }
    ::= { alaVrrp3OperTable 1 }

AlaVrrp3OperEntry ::=
    SEQUENCE {
        alaVrrp3OperIpVersion
            INTEGER,
        alaVrrp3OperVrId
            VrId,
        alaVrrp3OperVirtualMacAddr
            MacAddress,
        alaVrrp3OperState
            INTEGER,
        alaVrrp3OperAdminState
            INTEGER,
        alaVrrp3OperPriority
            Integer32,
        alaVrrp3OperVersion
            INTEGER,
        alaVrrp3OperIpAddrCount
            Integer32,
        alaVrrp3OperMasterIpAddrType
            InetAddressType,
        alaVrrp3OperMasterIpAddr
            InetAddress,
        alaVrrp3OperPrimaryIpAddrType
            InetAddressType,
        alaVrrp3OperPrimaryIpAddr
            InetAddress,
        alaVrrp3OperAdvInterval
            Integer32,
        alaVrrp3OperPreemptMode
            TruthValue,
        alaVrrp3OperAcceptMode
            TruthValue,
        alaVrrp3OperUpTime
            TimeStamp,
        alaVrrp3OperRowStatus
            RowStatus
    }

alaVrrp3OperIpVersion OBJECT-TYPE
    SYNTAX       INTEGER {
        ipv4     (1),
        ipv6     (2)
    }
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "This object contains the IP version on which this VRRP
         instance is running."
    ::= { alaVrrp3OperEntry 1 }

alaVrrp3OperVrId OBJECT-TYPE
    SYNTAX       VrId
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "This object contains the Virtual Router Identifier
         (VRID)."
    ::= { alaVrrp3OperEntry 2 }

alaVrrp3OperVirtualMacAddr OBJECT-TYPE
    SYNTAX       MacAddress
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The virtual MAC address of the virtual router.
         Although this object can be derived from the
         'alaVrrp3OperVrId' object, it is defined so that it
         is easily obtainable by a management application and
         can be included in VRRP-related SNMP traps."
    ::= { alaVrrp3OperEntry 3 }

alaVrrp3OperState OBJECT-TYPE
    SYNTAX       INTEGER {
        initialize   (1),
        backup       (2),
        master       (3)
    }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The current state of the virtual router. This object
         has three defined values:

         - `initialize', which indicates that the
           virtual router is waiting for a startup event.

         - `backup', which indicates the virtual router is
           monitoring the availability of the master router.

         - `master', which indicates that the virtual router
           is forwarding packets for IP addresses that are
           associated with this router.

         Setting the `alaVrrp3OperAdminState' object (below)
         Initiates transitions in the value of this object."
    ::= { alaVrrp3OperEntry 4 }

alaVrrp3OperAdminState OBJECT-TYPE
    SYNTAX       INTEGER {
        up       (1),
        down     (2)
    }
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "This object will enable/disable the virtual router
         function. Setting the value to `up', will transition
         the state of the virtual router from `initialize' to
         `backup' or `master', depending on the value of
         `alaVrrp3OperPriority'.

         Setting the value to `down', will transition the
         router from `master' or `backup' to `initialize'. State
         transitions may not be immediate; they sometimes depend
         on other factors, such as the interface (IF) state.

         The `alaVrrp3OperAdminState' object must be set to
         `down' prior to modifying the other read-create objects
         in the conceptual row. The value of the
         alaVrrp3OperRowStatus' object (below) must be
         `active', signifying that the conceptual row is valid
         (i.e., the objects are correctly set), in order for
         this object to be set to `up'."
    DEFVAL    { down }
    ::= { alaVrrp3OperEntry 5 }

alaVrrp3OperPriority OBJECT-TYPE
    SYNTAX       Integer32 (0..255)
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "This object specifies the priority to be used for the
         virtual router master election process. Higher values
         imply higher priority.

         A priority of '0', although not settable, is sent by
         the master router to indicate that this router has
         ceased to participate in VRRP and a backup virtual
         router should transition to become a new master.

         A priority of 255 is used for the router that owns the
         associated IP address(es)."
    DEFVAL       { 100 }
    ::= { alaVrrp3OperEntry 6 }

alaVrrp3OperVersion OBJECT-TYPE
    SYNTAX       INTEGER {
        vrrpv2   (1),
        vrrpv3   (2)
    }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "This object contains the VRRP version this VRRP
         instance is running."
    ::= { alaVrrp3OperEntry 7 }

alaVrrp3OperIpAddrCount OBJECT-TYPE
    SYNTAX       Integer32 (0..255)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The number of IP addresses associated with this
         virtual router. This number is equal to the number
         of rows in the alaVrrp3AssoIpAddrTable that
         correspond to a given combination of IP version, 
         VRID, and ifIndex."
    ::= { alaVrrp3OperEntry 8 }

alaVrrp3OperMasterIpAddrType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "This specifies the type of
         alaVrrp3OperMasterIpAddr in this row."
    ::= { alaVrrp3OperEntry 9 }

alaVrrp3OperMasterIpAddr OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The master router's real (primary for vrrp over IPv4)
         IP address. This is the IP address listed as the
         source in the advertisement last received by this
         virtual router.  For IPv6, a link local address."
    ::= { alaVrrp3OperEntry 10 }

alaVrrp3OperPrimaryIpAddrType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "This specifies the the type of
         alaVrrp3OperPrimaryIpAddr in this row."
    ::= { alaVrrp3OperEntry 11 }

alaVrrp3OperPrimaryIpAddr OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "For VRRP over IPv6 this is the link local address 
         for a given ifIndex.  For VRRP over IPv4, in the 
         case where there is more than one IP address for
         a given `ifIndex', this object is used to
         specify the IP address that will become the
         alaVrrp3OperMasterIpAddr', should the virtual router
         transition from backup to master."
    DEFVAL       { '00000000'H } -- 0.0.0.0 or ::
    ::= { alaVrrp3OperEntry 12 }

alaVrrp3OperAdvInterval OBJECT-TYPE
    SYNTAX       Integer32 (1..4095)
    UNITS        "centiseconds"
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The time interval, in centiseconds, between sending
         advertisement messages. Only the master router sends
         VRRP advertisements."
    DEFVAL       { 100 }
    ::= { alaVrrp3OperEntry 13 }

alaVrrp3OperPreemptMode OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "Controls whether a higher priority virtual router will
         preempt a lower priority master."
    DEFVAL       { true }
    ::= { alaVrrp3OperEntry 14 }

alaVrrp3OperAcceptMode OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "Controls whether a virtual router in the master state
         will accept packets addressed to the address owner's 
         IPv6 address as its own it it is not the IP address 
         owner.
         This is required only for rows indicating VRRP over IPv6.
         This object can be sparse and should not be implemented
         for rows indicating VRRP for Ipv4."
    DEFVAL       { true }
    ::= { alaVrrp3OperEntry 15 }

alaVrrp3OperUpTime OBJECT-TYPE
    SYNTAX       TimeStamp
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "This is the value of the `sysUpTime' object when this
         virtual router (i.e., the `alaVrrp3OperState') transitioned
         out of `initialized'."
    ::= { alaVrrp3OperEntry 16 }

alaVrrp3OperRowStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The row status variable, used in accordance to
         installation and removal conventions for conceptual
         rows. The rowstatus of a currently active row in the
         alaVrrp3OperTable is constrained by the operational
         state of the corresponding virtual router.
         When `alaVrrp3OperRowStatus' is set to active(1), no
         other objects in the conceptual row, with the exception
         of `alaVrrp3OperAdminState', can be modified. Prior
         to setting the `alaVrrp3OperRowStatus' object from
         `active' to a different value, the
         `alaVrrp3OperAdminState' object must be set to
         `down' and the `alaVrrp3OperState' object be transitioned
         to `initialize'.

         To create a row in this table, a manager sets this
         object to either createAndGo(4) or createAndWait(5).
         Until instances of all corresponding columns are
         appropriately configured, the value of the
         corresponding instance of the `alaVrrp3OperRowStatus'
         column will be read as notReady(3).
         In particular, a newly created row cannot be made
         active(1) until (minimally) the corresponding instance
         of `alaVrrp3OperVrId' has been set and there is at
         least one active row in the `alaVrrp3AssoIpAddrTable'
         defining an associated IP address for the virtual
         router."
    ::= { alaVrrp3OperEntry 17 }

--
--  VRRP Associated Address Table
--

alaVrrp3AssoIpAddrTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF AlaVrrp3AssoIpAddrEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The table of addresses associated with this 
         virtual router."
    ::= { alaVrrp3Operations 3 }

alaVrrp3AssoIpAddrEntry OBJECT-TYPE
    SYNTAX       AlaVrrp3AssoIpAddrEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "An entry in the table contains an IP address that is
         associated with a virtual router. The number of rows
         for a given IP version, VrId, and ifIndex will equal 
         the number of IP addresses associated (e.g., backed
         up) by the virtual router (equivalent to
         'alaVrrp3OperIpAddrCount').

         Rows in the table cannot be modified unless the value
         of `alaVrrp3OperAdminState' is `disabled' and the
         `alaVrrp3OperState' has transitioned to`initialize'."

    INDEX    { alaVrrp3OperIpVersion, alaVrrp3OperVrId, ifIndex, 
               alaVrrp3AssoIpAddrType, alaVrrp3AssoIpAddr }
    ::= { alaVrrp3AssoIpAddrTable 1 }

AlaVrrp3AssoIpAddrEntry ::=
    SEQUENCE {
        alaVrrp3AssoIpAddrType
            InetAddressType,
        alaVrrp3AssoIpAddr
            InetAddress,
        alaVrrp3AssoIpAddrRowStatus
            RowStatus
    }

alaVrrp3AssoIpAddrType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The IP addresses type of alaVrrp3AssoIpAddr in this
         row."
    ::= { alaVrrp3AssoIpAddrEntry 1 }

alaVrrp3AssoIpAddr OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The assigned IP addresses that a virtual router is
         responsible for backing up."
    ::= { alaVrrp3AssoIpAddrEntry 2 }

alaVrrp3AssoIpAddrRowStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The row status variable, used according to
         installation and removal conventions for conceptual
         rows. Setting this object to active(1) or
         createAndGo(4) results in the addition of an associated
         address for a virtual router.

         Destroying the entry or setting it to notInService(2)
         removes the associated address from the virtual router.
         The use of other values is implementation-dependent."
    ::= { alaVrrp3AssoIpAddrEntry 3 }

--
--  VRRP Router Statistics
--

alaVrrp3RouterChecksumErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP packets received with an
         invalid VRRP checksum value."
    ::= { alaVrrp3Statistics 1 }

alaVrrp3RouterVersionErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP packets received with an
         unknown or unsupported version number."
    ::= { alaVrrp3Statistics 2 }

alaVrrp3RouterVrIdErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP packets received with an
         invalid VRID for this virtual router."
    ::= { alaVrrp3Statistics 3 }

--
--  VRRP Router Statistics Table
--

alaVrrp3RouterStatsTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF AlaVRRP3RouterStatsEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Table of virtual router statistics."
    ::= { alaVrrp3Statistics 4 }

alaVrrp3RouterStatsEntry OBJECT-TYPE
    SYNTAX       AlaVRRP3RouterStatsEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "An entry in the table, containing statistics
         information about a given virtual router."
    INDEX    { alaVrrp3OperIpVersion, alaVrrp3OperVrId, 
               ifIndex }
    ::= { alaVrrp3RouterStatsTable 1 }

AlaVRRP3RouterStatsEntry ::=
    SEQUENCE {
        alaVrrp3StatsBecomeMaster
            Counter32,
        alaVrrp3StatsAdvertiseRcvd
            Counter32,
        alaVrrp3StatsAdvIntervalErrors
            Counter32,
        alaVrrp3StatsIpTtlErrors
            Counter32,
        alaVrrp3StatsPriZeroPktsRcvd
            Counter32,
        alaVrrp3StatsPriZeroPktsSent
            Counter32,
        alaVrrp3StatsInvldTypePktsRcvd
            Counter32,
        alaVrrp3StatsAddressListErrors
            Counter32,
        alaVrrp3StatsInvldAuthType
            Counter32,
        alaVrrp3StatsPacketLengthErrors
            Counter32
    }


alaVrrp3StatsBecomeMaster OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of times that this virtual router's
         state has transitioned to MASTER."
    ::= { alaVrrp3RouterStatsEntry 1 }

alaVrrp3StatsAdvertiseRcvd OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP advertisements received by
         this virtual router."
    ::= { alaVrrp3RouterStatsEntry 2 }

alaVrrp3StatsAdvIntervalErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP advertisement packets
         received for which the advertisement interval is
         different than the one configured for the local virtual
         router."
    ::= { alaVrrp3RouterStatsEntry 3 }

alaVrrp3StatsIpTtlErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP packets received by the
         virtual router with IP TTL (Time-To-Live) not equal to
         255. It also indicates the number of VRRPv3 packets
         received by the virtual router with IPv6 hop limit not
         equal to 255."
    ::= { alaVrrp3RouterStatsEntry 4 }

alaVrrp3StatsPriZeroPktsRcvd OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP packets received by the
         virtual router with a priority of '0'."
    ::= { alaVrrp3RouterStatsEntry 5 }

alaVrrp3StatsPriZeroPktsSent OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of VRRP packets sent by the virtual
         router with a priority of '0'."
    ::= { alaVrrp3RouterStatsEntry 6 }

alaVrrp3StatsInvldTypePktsRcvd OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The number of VRRP packets received by the virtual
         router with an invalid value in the 'type' field."
    ::= { alaVrrp3RouterStatsEntry 7 }

alaVrrp3StatsAddressListErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of packets received for which the
         address list does not match the locally configured list
         for the virtual router."
    ::= { alaVrrp3RouterStatsEntry 8 }

alaVrrp3StatsInvldAuthType OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of packets received with 'Auth Type'
         not equal to Authentication Type 0, No Authentication.
         This is required only for rows indicating VRRP over IPv4.
         This object can be sparse and should not be implemented
         for rows indicating VRRP for Ipv6."
    ::= { alaVrrp3RouterStatsEntry 9 }

alaVrrp3StatsPacketLengthErrors OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total number of packets received with a packet
         length less than the length of the VRRP header."
    ::= { alaVrrp3RouterStatsEntry 10 }

--
--   Trap Definitions
--

alaVrrp3Notifications   OBJECT IDENTIFIER ::= { alcatelIND1VRRP3MIB 0 }

---
--- Objects used in the traps
---

alaVrrp3TrapNewMasterReason OBJECT-TYPE
    SYNTAX        INTEGER {
        priority         (0),
        preempted        (1),
        masterNoResponse (2)
    }
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "This indicates the reason for NewMaster trap.
         Used by alaVrrp3TrapNewMaster trap."
    ::= { alaVrrp3Operations 4 }

alaVrrp3TrapProtoErrReason OBJECT-TYPE
    SYNTAX        INTEGER {
        hopLimitError (0),
        versionError  (1),
        checksumError (2),
        vridError     (3)
    }
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "This indicates the reason for protocol error trap.
         Used by alaVrrp3TrapProtoError trap."
    ::= { alaVrrp3Operations 5 }


alaVrrp3TrapNewMaster NOTIFICATION-TYPE
    OBJECTS      { alaVrrp3OperMasterIpAddrType,
                   alaVrrp3OperMasterIpAddr,
                   alaVrrp3TrapNewMasterReason
                 }
    STATUS       current
    DESCRIPTION
        "The newMaster trap indicates that the sending agent
         has transitioned to 'Master' state."
    ::= { alaVrrp3Notifications 1 }

alaVrrp3TrapProtoError NOTIFICATION-TYPE
    OBJECTS      { alaVrrp3TrapProtoErrReason
                 }
    STATUS       current
    DESCRIPTION
        "The error trap indicates that the sending agent has
         encountered the protocol error indicated by
         ErrorReason."
    ::= { alaVrrp3Notifications 2 }


--
--  Conformance Information
--

alaVrrp3MIBCompliances  OBJECT IDENTIFIER ::= { alaVrrp3Conformance 1 }
alaVrrp3MIBGroups       OBJECT IDENTIFIER ::= { alaVrrp3Conformance 2 }

--
-- Compliance Statements
--


alaVrrp3MIBCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
	"The compliance statement for switches with Alcatel VRRP and
	implementing ALCATEL-IND1-VRRP3-MIB."

    MODULE -- this module
    MANDATORY-GROUPS  {
        alaVrrp3OperGroup,
        alaVrrp3StatsGroup,
        alaVrrp3TrapInfoGroup,
        alaVrrp3NotificationsGroup
    }

    OBJECT        alaVrrp3OperPriority
    WRITE-SYNTAX  Integer32 (1..255)
    DESCRIPTION  "SETable values are from 1 to 255."
    ::= { alaVrrp3MIBCompliances 1 }

--
-- Conformance Groups
--

alaVrrp3OperGroup   OBJECT-GROUP
    OBJECTS  {
        alaVrrp3NotificationCntl,
        alaVrrp3OperVirtualMacAddr,
        alaVrrp3OperState,
        alaVrrp3OperAdminState,
        alaVrrp3OperPriority,
        alaVrrp3OperVersion,
        alaVrrp3OperIpAddrCount,
        alaVrrp3OperMasterIpAddrType,
        alaVrrp3OperMasterIpAddr,
        alaVrrp3OperPrimaryIpAddrType,
        alaVrrp3OperPrimaryIpAddr,
        alaVrrp3OperAdvInterval,
        alaVrrp3OperPreemptMode,
        alaVrrp3OperAcceptMode,
        alaVrrp3OperUpTime,
        alaVrrp3OperRowStatus,
        alaVrrp3AssoIpAddrRowStatus
    }
    STATUS current
    DESCRIPTION
	"A collection of objects to support management of Alcatel VRRP."
    ::= { alaVrrp3MIBGroups 1 }

alaVrrp3StatsGroup  OBJECT-GROUP
    OBJECTS  {
        alaVrrp3RouterChecksumErrors,
        alaVrrp3RouterVersionErrors,
        alaVrrp3RouterVrIdErrors,
        alaVrrp3StatsBecomeMaster,
        alaVrrp3StatsAdvertiseRcvd,
        alaVrrp3StatsAdvIntervalErrors,
        alaVrrp3StatsPriZeroPktsRcvd,
        alaVrrp3StatsPriZeroPktsSent,
        alaVrrp3StatsInvldTypePktsRcvd,
        alaVrrp3StatsInvldAuthType,
        alaVrrp3StatsIpTtlErrors,
        alaVrrp3StatsAddressListErrors,
        alaVrrp3StatsPacketLengthErrors
    }
    STATUS current
    DESCRIPTION
	"A collection of objects to support management of Alcatel VRRP."
    ::= { alaVrrp3MIBGroups 2 }

alaVrrp3TrapInfoGroup  OBJECT-GROUP
    OBJECTS  {
        alaVrrp3TrapNewMasterReason,
        alaVrrp3TrapProtoErrReason
    }
    STATUS current
    DESCRIPTION
	"A collection of objects to support management of Alcatel VRRP."
    ::= { alaVrrp3MIBGroups 3 }

alaVrrp3NotificationsGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
        alaVrrp3TrapNewMaster,
        alaVrrp3TrapProtoError
    }
    STATUS current
    DESCRIPTION
	"A collection of objects to support management of Alcatel VRRP."
    ::= { alaVrrp3MIBGroups 4 }

END

