ALCATEL-IND1-VLAN-MGR-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		DisplayString, RowStatus, TEXTUAL-CONVENTION	FROM SNMPv2-TC
		MODULE-IDENTITY, OBJECT-IDENTITY,
		OBJECT-TYPE, IpAddress, Unsigned32				FROM SNMPv2-SMI
		MODULE-COMPLIANCE, OBJECT-GROUP          		FROM SNMPv2-CONF
		softentIND1VlanMgt								FROM ALCATEL-IND1-BASE;


	alcatelIND1VLANMgrMIB MODULE-IDENTITY
		LAST-UPDATED "200704030000Z"
		ORGANIZATION "Alcatel-Lucent"
		CONTACT-INFO
            "Please consult with Customer Service to ensure the most appropriate
             version of this document is used with the products in question:

                        Alcatel-Lucent, Enterprise Solutions Division
                       (Formerly Alcatel Internetworking, Incorporated)
                               26801 West Agoura Road
                            Agoura Hills, CA  91301-5122
                              United States Of America

            Telephone:               North America  +1 800 995 2696
                                     Latin America  +1 877 919 9526
                                     Europe         +31 23 556 0100
                                     Asia           +65 394 7933
                                     All Other      +1 818 878 4507

            Electronic Mail:         support@ind.alcatel.com
            World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
            File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

		DESCRIPTION
			"This module describes an authoritative enterprise-specific Simple
             Network Management Protocol (SNMP) Management Information Base (MIB):

                 For the Birds Of Prey Product Line
                 Vlan Manager for the distribution of vlan configuration information,
				 including the association between vlans and ports.

             The right to make changes in specification and other information
             contained in this document without prior notice is reserved.

             No liability shall be assumed for any incidental, indirect, special, or
             consequential damages whatsoever arising from or related to this
             document or the information contained herein.

             Vendors, end-users, and other interested parties are granted
             non-exclusive license to use this specification in connection with
             management of the products for which it is intended to be used.

                         Copyright (C) 1995-2007 Alcatel-Lucent
                             ALL RIGHTS RESERVED WORLDWIDE"

		REVISION      "200704030000Z"
        DESCRIPTION
            "The latest version of this MIB Module."
		::= { softentIND1VlanMgt 1}

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	IpxNetworkAddress ::= TEXTUAL-CONVENTION
		DISPLAY-HINT "x"
		STATUS current
		DESCRIPTION
			"Textual convention for ipx network address.
			 This is an unsigned integer (32 bits) that should be
			 represented as a hexedecimal value."
		SYNTAX Unsigned32

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	alcatelIND1VLANMgrMIBObjects OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Manager
            Subsystem Managed Objects."
        ::= { alcatelIND1VLANMgrMIB 1 }


    alcatelIND1VLANMgrMIBConformance OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Manager
            Subsystem Conformance Information."
        ::= { alcatelIND1VLANMgrMIB 2 }


    alcatelIND1VLANMgrMIBGroups OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Manager
            Subsystem Units Of Conformance."
        ::= { alcatelIND1VLANMgrMIBConformance 1 }


    alcatelIND1VLANMgrMIBCompliances OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Manager
            Subsystem Compliance Statements."
        ::= { alcatelIND1VLANMgrMIBConformance 2 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	vlanMgrVlan  OBJECT IDENTIFIER ::= { alcatelIND1VLANMgrMIBObjects 1 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	vlanTable  OBJECT-TYPE
	    SYNTAX  SEQUENCE OF VlanEntry
	    MAX-ACCESS  not-accessible
	    STATUS  current
	    DESCRIPTION
		 "A list of Virtual LAN instances in this device."
	    ::= { vlanMgrVlan 1 }

	vlanEntry  OBJECT-TYPE
	    SYNTAX  VlanEntry
	    MAX-ACCESS  not-accessible
	    STATUS  current
	    DESCRIPTION
		 "A VLAN entry."
	    INDEX { vlanNumber }
	    ::= { vlanTable 1 }

	VlanEntry ::= SEQUENCE {
		vlanNumber
			INTEGER,
	    vlanDescription
			DisplayString,
	    vlanAdmStatus
			INTEGER,
	    vlanOperStatus
			INTEGER,
		vlanStatus
			RowStatus,
		vlanStpStatus
        	INTEGER,
		vlanAuthentStatus
			INTEGER,
		vlanVoiceStatus
			INTEGER,
		vlanIpAddress
			IpAddress,
		vlanIpMask
			IpAddress,
		vlanIpEncap
			INTEGER,
		vlanIpForward
			INTEGER,
		vlanIpStatus
			INTEGER,
		vlanIpxNet
			IpxNetworkAddress,
		vlanIpxEncap
			INTEGER,
		vlanIpxRipSapMode
			INTEGER,
		vlanIpxDelayTicks
			INTEGER,
		vlanIpxStatus
			INTEGER,
		vlanTagMobilePortStatus
			INTEGER,
		vlanPortMacStatus
			INTEGER,
		vlanLocalProxyArp
			INTEGER,
		vlanMtu
                        INTEGER,
                vlan1x1StpStatus
        		INTEGER,
		vlanflatStpStatus
        		INTEGER,
        	vlanHABandwidth
    	                INTEGER,
                vlanSvlanTrafficType
                        INTEGER,
                vlanSvlanPriority
        		INTEGER,
                vlanMacLearningControlStatus          
                        INTEGER
	}

	vlanNumber  OBJECT-TYPE
	    SYNTAX  INTEGER (1..4094)
	    MAX-ACCESS  read-write
	    STATUS  current
	    DESCRIPTION
		 "The VLAN number identifying this instance. Valid
		  range from 1 to 4094."
	    ::= { vlanEntry 1 }

	vlanDescription  OBJECT-TYPE
	    SYNTAX  DisplayString (SIZE (0..32))
	    MAX-ACCESS  read-write
	    STATUS  current
	    DESCRIPTION
		 "Textual description of the VLAN instance."
	    ::= { vlanEntry 2 }

	vlanAdmStatus  OBJECT-TYPE
	    SYNTAX  INTEGER {
	    	enabled(1),
	    	disabled(2)
	    }
	    MAX-ACCESS  read-write
	    STATUS  current
	    DESCRIPTION
		"The administrative status which can be set by
		 configuration. Disable(1) will disable ALL vports
		 that are connected to this VLAN, enable(2) will enable
		 ALL ports on this VLAN, delete(3) will detach and
		 delete the ports/routers AND remove the VLAN."
		 DEFVAL { enabled }
		::= { vlanEntry 3 }

	vlanOperStatus  OBJECT-TYPE
		SYNTAX  INTEGER {
			active(1),
			inactive(2)
		}
		MAX-ACCESS  read-only
		STATUS  current
		DESCRIPTION
			"Provide operating status of a particular VLAN environment."
		::= { vlanEntry 4 }

	 vlanStatus  OBJECT-TYPE
	 	SYNTAX  RowStatus
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
			"Row status to control creation/deletion of vlans."
		::= { vlanEntry 5 }

	vlanStpStatus  OBJECT-TYPE
		SYNTAX  INTEGER {
			enabled(1),
			disabled(2)
		}
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
		"Indicates status of spanning tree for the current VLAN."
		DEFVAL { enabled }
		::= { vlanEntry 6 }

	vlanAuthentStatus OBJECT-TYPE
		SYNTAX  INTEGER {
			enabled(1),
			disabled(2)
		}
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
		"Indicates status of authentication for the current VLAN."
		DEFVAL { disabled }
		::= { vlanEntry 7 }


	vlanVoiceStatus OBJECT-TYPE
		SYNTAX  INTEGER {
			enabled(1),
			disabled(2)
		}
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
		"Indicates status of voice usage for the current VLAN."
		DEFVAL { disabled }
		::= { vlanEntry 8 }


	vlanIpAddress  OBJECT-TYPE
		SYNTAX  IpAddress
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
			"IP address of the VLAN's virtual router port.
			 Note:  a vlan does not necessarily have an ip address.
			 Setting one requires that the ip address be set, and optionally the
			 following since they have defaults:  ip mask, ip encap, ip forward.
			 Then setting vlanIpStatus to add will create the ip router port
			 for the given vlan (the index)."
		 ::= { vlanEntry 9 }

	vlanIpMask OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Subnetwork mask for VLAN IP Address.
			 Default is class level mask for the ip address."
		::= { vlanEntry 10 }

	vlanIpEncap OBJECT-TYPE
		SYNTAX INTEGER {
			ethernet2 (1),
			snap (2),
			notApplicable(3)
		}
		MAX-ACCESS read-write
	    STATUS current
		DESCRIPTION
		"VLAN's IP router port encapsulation.
		 Not applicable when there is no ip router port."
		DEFVAL { ethernet2 }
		::= { vlanEntry 11 }

	vlanIpForward OBJECT-TYPE
		SYNTAX INTEGER {
			enable(1),
			disable(2),
			notApplicable(3)
		}
		MAX-ACCESS read-write
	    STATUS current
		DESCRIPTION
		"VLAN's IP router port ip frame forwarding (disabled = ip host only).
		 Not applicable when there is no ip router port."
		DEFVAL { enable }
		::= { vlanEntry 12 }

	vlanIpStatus OBJECT-TYPE
		SYNTAX INTEGER {
			add(1),
			delete(2)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"Provides ability to add and remove the VLAN ip address."
		::= { vlanEntry 13 }

	vlanIpxNet OBJECT-TYPE
		SYNTAX IpxNetworkAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"IPX network address.
		 Note:  a vlan does not necessarily have an ipx net number.
		 Setting one requires that the ipx net be set, and optionally the
		 ipx encap, ipx rip-sap mode, and delay ticks (all have defaults).
		 Then the vlanIpxStatus should be set to add to create the
		 ipx router port."
		::= { vlanEntry 14 }

	vlanIpxEncap OBJECT-TYPE
		SYNTAX INTEGER {
			ethernet2 (1),
			novellraw (2),
			llc (3),
			snap (4),
			notApplicable(5)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"IPX of frame enapsulation of IPX VLAN router port.
		 Not applicable when there is no ipx router port."
		DEFVAL { ethernet2 }
		::= { vlanEntry 15 }

	vlanIpxRipSapMode OBJECT-TYPE
		SYNTAX INTEGER {
			riponly (1),
			ripsap (2),
			triggered (3),
			inactive(4),
			notApplicable(5)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"IPX advertisement mode.
		 Not applicable when there is no ipx router port."
		DEFVAL { ripsap }
		::= { vlanEntry 16 }

	vlanIpxDelayTicks OBJECT-TYPE
		SYNTAX INTEGER (0..65535)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"Tick metric to use for supporting IPX routing decisions."
		DEFVAL { 0 }
		::= {vlanEntry 17 }

	vlanIpxStatus OBJECT-TYPE
		SYNTAX INTEGER {
			add(1),
			delete(2)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"Provides ability to add and remove the VLAN ipx network node."
		::= { vlanEntry 18 }

	vlanTagMobilePortStatus OBJECT-TYPE
                SYNTAX INTEGER {
                        enable(1),
                        disable(2)
                }
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                "When enabled for a VLAN, a mobile port will be moved to the
		 VLAN based on the tag."
                ::= { vlanEntry 19 }

	vlanPortMacStatus OBJECT-TYPE
		SYNTAX INTEGER {
			enable(1),
			disable(2)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"When enabled for a VLAN, it will be considered a special VLAN not
		 affected by the ordinary vlan commands except the command to
		 delete a VLAN"
		::= { vlanEntry 20 }

	vlanLocalProxyArp OBJECT-TYPE
     		SYNTAX INTEGER {
       			enable(1),
       			disable(2)
     		}
     		MAX-ACCESS read-write
     		STATUS current
     		DESCRIPTION
       		"When enabled for a VLAN, local proxy ARP processing happens on this=
 		 VLAN."
     		::= { vlanEntry 21 }

	vlanMtu  OBJECT-TYPE
                SYNTAX  INTEGER (1280..9198)
                MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                 "Maximum transmission unit i.e. the maximum size of packet that this
                  vlan can handle. It ranges from 1280 to 9198."
                ::= { vlanEntry 22 }

	vlan1x1StpStatus  OBJECT-TYPE
		SYNTAX  INTEGER {
			enabled(1),
			disabled(2)
		}
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
		"Indicates status of 1x1 spanning tree for the current VLAN."
		DEFVAL { enabled }
		::= { vlanEntry  23}

	vlanflatStpStatus  OBJECT-TYPE
		SYNTAX  INTEGER {
			enabled(1),
			disabled(2)
		}
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
		"Indicates status of flat spanning tree for the current VLAN."
		DEFVAL { enabled }
		::= { vlanEntry  24}

	vlanHABandwidth OBJECT-TYPE
                SYNTAX  INTEGER (0..50)
                MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                "Bandwidth of flood queue allocated by Q-driver for High Availability
		 vlans. The value ranges from 1 to 50 Mega bits per second."
                ::= { vlanEntry 25 }

        vlanSvlanTrafficType OBJECT-TYPE
                        SYNTAX  INTEGER {
                                notApplicable(0),
                                customer(1),
                                provider(2),
                                multicastEnterprise(3),
                                multicastVlanStacking(4),
                                eServiceCustomer(6),
                                eServiceManagement(7),
                                eServiceMulticastVlanStacking(8)
                        }
                MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                "The created SVLAN is desired for carrying customer or
                provider traffic, default is customer. When creating
                standard Vlans the value should be notApplicable"
		        DEFVAL { 0 }
                ::= { vlanEntry 26 }

   	vlanSvlanPriority OBJECT-TYPE
                SYNTAX  INTEGER (-1..7)
                MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                "All traffic getting mapped to this Svlan should be either
                priority mapped or mapped to a specific priority 0-7, default
                is priority 0. For standard Vlans the value should be -1"
		        DEFVAL { 0 }
                ::= { vlanEntry 27 }
        vlanMacLearningControlStatus   OBJECT-TYPE
                SYNTAX          INTEGER{
                                      enabled (1),
                                      disabled (2)
                                       }
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION
                "Status of Mac Learning on a vlan"
                        DEFVAL { enabled }
                ::= { vlanEntry 28 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	vlanMgrVpa  OBJECT IDENTIFIER ::= { alcatelIND1VLANMgrMIBObjects 2 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	vpaTable  OBJECT-TYPE
	    SYNTAX  SEQUENCE OF VpaEntry
	    MAX-ACCESS  not-accessible
	    STATUS  current
	    DESCRIPTION
		 "A list of Virtual LAN instances in this device."
	    ::= { vlanMgrVpa 1 }

	vpaEntry  OBJECT-TYPE
	    SYNTAX  VpaEntry
	    MAX-ACCESS  not-accessible
	    STATUS  current
	    DESCRIPTION
		 "A VLAN-Port Association (VPA) entry."
	    INDEX { vpaVlanNumber, vpaIfIndex }
	    ::= { vpaTable 1 }

	VpaEntry ::= SEQUENCE {
		vpaVlanNumber
			INTEGER,
		vpaIfIndex
			Unsigned32,
		vpaType
			INTEGER,
		vpaState
			INTEGER,
		vpaStatus
			RowStatus,
		vpaPortMacType
			INTEGER
	}

	vpaVlanNumber  OBJECT-TYPE
		SYNTAX  INTEGER (1..4094)
		MAX-ACCESS  read-write
	    STATUS  current
	    DESCRIPTION
		 "The VLAN number component of this instance. Valid
		  range from 1 to 4094."
	    ::= { vpaEntry 1 }

	vpaIfIndex  OBJECT-TYPE
		SYNTAX  Unsigned32 (1001..4294967295)
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
		"The ifIndex component of this instance."
		::= {vpaEntry 2 }

        vpaType  OBJECT-TYPE
                SYNTAX  INTEGER {
                        cfgDefault(1),
                        qTagged(2),
                        mobile(3),
                        mirrored(4),
                        svlan(6),
                        dynamic(7)
                }
                MAX-ACCESS  read-only
                STATUS  current
                DESCRIPTION
                "The type of this vpa.  Two are statically configured:
                 configured default VPA and qTagged VPA. The mirrored
                 is an internal type set for mirrored ports and the
                 rest are dynamic vlan's
     
                 1. cfgDefault - Default vlan VPA Type
                 2. qTagged    - The qTagged vlan VPA Type
                 3. mobile     - The vpa is dynamically created according
                                 to rules/policies.
                 4. mirrored   - Set internally when the vpa created is on
              	                 a mirrored port.
                 6. slvan      - Service vlan vpa's which are created.
                 7. dynamic    - Created by dynamic GVRP or MVRP Protocol."

                ::= { vpaEntry 3 }

	vpaState  OBJECT-TYPE
		SYNTAX  INTEGER {
			inactive(1),
			blocking(2),
			forwarding(3),
			filtering(4)
		}
		MAX-ACCESS  read-only
		STATUS  current
		DESCRIPTION
		"The state of this vpa:
			1. inactive   - link down
			2. blocking   - link up, forwarding down
			3. forwarding - link up, forwarding up, sources learned normally
			4. filtering  - link up, forwarding up, sources filtered."
		::= { vpaEntry 4 }

	vpaStatus  OBJECT-TYPE
		SYNTAX  RowStatus
		MAX-ACCESS  read-write
		STATUS  current
		DESCRIPTION
		"This is used to create or delete staticPrimary VPAs (default vlans
		 on a port ).  Creation replaces the existing staticPrimary VPA
		 while deletion replaces the existing VPA so that the vlan number
		 is 1 for the given port.  Of course the corresponding vlan and
		 port must exist."
		 ::= { vpaEntry 5 }

	vpaPortMacType OBJECT-TYPE
		SYNTAX INTEGER {
			ingress(1),
			egress(2),
			inapplicable(3)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"Value of this field will decide whether the port represented by vpaIfIndex is a ingress port or egress port. This fiels is applicable only for portMac vlans"
		::= { vpaEntry 6 }



-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	vlanMgrVlanSet  OBJECT IDENTIFIER ::= { alcatelIND1VLANMgrMIBObjects 3 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

	vlanSetVlanCount  OBJECT-TYPE
	    SYNTAX  INTEGER (1..4094)
	    MAX-ACCESS  read-only
	    STATUS  current
	    DESCRIPTION
		 "Count of existing VLANs on switch."
	    ::= { vlanMgrVlanSet 1 }

	vlanSetVlanRouterCount  OBJECT-TYPE
	    SYNTAX  INTEGER (0..4094)
	    MAX-ACCESS  read-only
	    STATUS  current
	    DESCRIPTION
		 "Count of VLANs on switch with at least one router port configured."
	    ::= { vlanMgrVlanSet 2 }

	vlanSetIpRouterCount  OBJECT-TYPE
	    SYNTAX  INTEGER (0..4094)
	    MAX-ACCESS  read-only
	    STATUS  current
	    DESCRIPTION
		 "Count of VLANs on switch with IP router port configured."
	    ::= { vlanMgrVlanSet 3 }

	vlanSetIpxRouterCount  OBJECT-TYPE
	    SYNTAX  INTEGER (0..256)
	    MAX-ACCESS  read-only
	    STATUS  current
	    DESCRIPTION
		 "Count of VLANs on switch with IPX router port configured."
	    ::= { vlanMgrVlanSet 4 }

	vlanSetMultiRtrMacStatus  OBJECT-TYPE
	    SYNTAX  INTEGER {
			enable(1),
			disable(2)
		}
	    MAX-ACCESS  read-write
	    STATUS  current
	    DESCRIPTION
		 "Controls whether unique mac assigned to each vlan
		  with router port (limit 64)."
		DEFVAL { disable }
	    ::= { vlanMgrVlanSet 5 }

--YP
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

        vlanMgrHAPort  OBJECT IDENTIFIER ::= { alcatelIND1VLANMgrMIBObjects 4 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

        vlanHAPortTable     OBJECT-TYPE
                SYNTAX  SEQUENCE OF VlanHAPortEntry
                MAX-ACCESS  not-accessible
                STATUS  current
                DESCRIPTION
                        "A list of Port To HA vlan binding."
                ::= { vlanMgrHAPort 1 }

        vlanHAPortEntry     OBJECT-TYPE
                SYNTAX  VlanHAPortEntry
                MAX-ACCESS  not-accessible
                STATUS  current
                DESCRIPTION
                        "Port To HA vlan binding entry."
                INDEX { vlanHAPortVlanId, vlanHAPortIfIndex, vlanHAPortType }
                ::= { vlanHAPortTable 1 }


        VlanHAPortEntry ::= SEQUENCE {
                vlanHAPortVlanId         INTEGER,
                vlanHAPortIfIndex        Unsigned32,
		vlanHAPortType		 INTEGER,
                vlanHAPortRowStatus      RowStatus
                }

        vlanHAPortVlanId            OBJECT-TYPE
                SYNTAX  INTEGER (1..4094)
                MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                "The vlan Id in which this port is a HA port"
                ::= { vlanHAPortEntry 1 }


        vlanHAPortIfIndex   OBJECT-TYPE
                SYNTAX  Unsigned32
                MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                "This port is associated with a HA vlan."
                ::= { vlanHAPortEntry 2 }

	vlanHAPortType	  OBJECT-TYPE
		SYNTAX INTEGER {
                        ingress(1),
                        egress(2)
                }
		MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                "Value of this field will decide whether the port represented by vlanHAPortIfIndex is a ingress port or egress port."
		::= { vlanHAPortEntry 3 }

        vlanHAPortRowStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-write
                STATUS  current
                DESCRIPTION
                "This indicate whether to add or delete the ifIndex"
                ::= { vlanHAPortEntry 4 }





-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- COMPLIANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

    alcatelIND1VLANMgrMIBCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
            "Compliance statement for
             VLAN Manager."
        MODULE
            MANDATORY-GROUPS
            {
                vlanMgrVlanGroup,
                vlanMgrVpaGroup,
				vlanMgrVlanSetGroup
            }

        ::= { alcatelIND1VLANMgrMIBCompliances 1 }


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- UNITS OF CONFORMANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

    vlanMgrVlanGroup OBJECT-GROUP
        OBJECTS
        {
			vlanNumber,		   -- vlan table
	    	vlanDescription,
	    	vlanAdmStatus,
	    	vlanOperStatus,
			vlanStatus,
			vlan1x1StpStatus,
			vlanflatStpStatus,
			vlanStpStatus,
			vlanAuthentStatus,
			vlanVoiceStatus,
			vlanIpAddress,
			vlanIpMask,
			vlanIpEncap,
			vlanIpForward,
			vlanIpStatus,
			vlanIpxNet,
			vlanIpxEncap,
			vlanIpxRipSapMode,
			vlanIpxDelayTicks,
			vlanIpxStatus
        }
        STATUS  current
        DESCRIPTION
            "Collection of objects for management of Vlan Manager VLANs."
        ::= { alcatelIND1VLANMgrMIBGroups 1 }


    vlanMgrVpaGroup OBJECT-GROUP
        OBJECTS
        {
			vpaVlanNumber,		  -- vpa table
			vpaIfIndex,
			vpaType,
			vpaState,
			vpaStatus
        }
        STATUS  current
        DESCRIPTION
            "Collection of objects for management of Vlan Manager VPAs."
        ::= { alcatelIND1VLANMgrMIBGroups 2 }

	vlanMgrVlanSetGroup OBJECT-GROUP
		OBJECTS
		{
		   vlanSetVlanCount,
		   vlanSetVlanRouterCount,
		   vlanSetIpRouterCount,
		   vlanSetIpxRouterCount,
		   vlanSetMultiRtrMacStatus
		}
		STATUS current
		DESCRIPTION
			"Collection of objects for Vlan Manager global properties."
		::= { alcatelIND1VLANMgrMIBGroups 3 }

	END

