TRIPPLITE-MIB DEFINITIONS ::= BEGIN

IMPORTS
  DisplayString,
  TruthValue,
  TimeStamp,
  TimeInterval,
  DateAndTime,
  AutonomousType,
  VariablePointer,
  RowStatus
    FROM SNMPv2-TC
  OBJECT-GROUP,
  NOTIFICATION-GROUP
    FROM SNMPv2-CONF
  MODULE-IDENTITY,
  OBJECT-IDENTITY,
  OBJECT-TYPE,
  NOTIFICATION-TYPE,
  Gauge32,
  Integer32,
  enterprises,
  IpAddress
    FROM SNMPv2-SMI
  PositiveInteger,
  NonNegativeInteger
    FROM UPS-MIB;

tripplite MODULE-IDENTITY
  LAST-UPDATED "200904270000Z"
  ORGANIZATION "Tripplite Inc"
  CONTACT-INFO
    "Mike Delgroso
    Tripplite, Inc.
    1111 W. 35th St.
    Chicago, IL 60609"
  DESCRIPTION
    "This MIB module defines MIB objects which provide mechanisms for
    remote management capabilities of Tripplite PowerAlert and related
    software."
  REVISION "200904270000Z"
  DESCRIPTION
    "Added tlUpsAlarmOutputCurrentChanged well known alarm trap"
  REVISION "200810140000Z"
  DESCRIPTION
    "Added tlUpsOutletCurrentTable and tlUpsOutletPowerTable to publish load-specific variables"
  REVISION "200809250000Z"
  DESCRIPTION
    "Added tlUpsOutletGroupTable."
  REVISION "200802010000Z"
  DESCRIPTION
	"V1 trap decode support."
  REVISION "200711300000Z"
  DESCRIPTION
	"Changed tlUpsAlarmTime to int to match implementation, same for tlUpsAlarmDescr to string"
  REVISION "200711290000Z"
  DESCRIPTION
	"Changed tlUpsConfigBattReplDate and tlUpsTestDate from integer back to string."
  REVISION "200708260000Z"
  DESCRIPTION
    "Migrated changes from 12.04.0034, which included Load -> Outlet."
  REVISION "200702280000Z"
  DESCRIPTION
    "Renamed Load to Outlet. Cleaned up MIB compilation errors."
  REVISION "200612120000Z"
  DESCRIPTION
    "Changed tlUpsConfigBattReplDate and tlUpsTestDate from string to integer."
  REVISION "200612060000Z"
  DESCRIPTION
    "Implement tlUpsOutletTable."
  REVISION "200606200000Z"
  DESCRIPTION
    "Implemented tlUpsAlarmTable to coincide with upsAlarmTable, but
    all for additional variables."
  REVISION "200507130000Z"
  DESCRIPTION
    "Modifications to bring MIB into compliance.  Changed OID name from
    upsLoadNumLoads to tlUpsLoadNumLoads."
  REVISION "200305160000Z"
  DESCRIPTION
    "Initial release, for PowerAlert Version 12."
  ::= { enterprises 850 }


--------------------------------------------------------------------------
-- Enumerations
--------------------------------------------------------------------------

tlEnumerations OBJECT IDENTIFIER  ::= { tripplite 2 }

tlOperatingSystems OBJECT IDENTIFIER ::= { tlEnumerations 1 }

hpux9 OBJECT IDENTIFIER   ::= { tlOperatingSystems 1 }

sunos4 OBJECT IDENTIFIER  ::= { tlOperatingSystems 2 }

solaris OBJECT IDENTIFIER   ::= { tlOperatingSystems 3 }

osf OBJECT IDENTIFIER   ::= { tlOperatingSystems 4 }

ultrix OBJECT IDENTIFIER  ::= { tlOperatingSystems 5 }

hpux10 OBJECT IDENTIFIER  ::= { tlOperatingSystems 6 }

netbsd1 OBJECT IDENTIFIER   ::= { tlOperatingSystems 7 }

freebsd OBJECT IDENTIFIER   ::= { tlOperatingSystems 8 }

irix OBJECT IDENTIFIER  ::= { tlOperatingSystems 9 }

linux OBJECT IDENTIFIER   ::= { tlOperatingSystems 10 }

bsdi OBJECT IDENTIFIER  ::= { tlOperatingSystems 11 }

openbsd OBJECT IDENTIFIER   ::= { tlOperatingSystems 12 }

win32 OBJECT IDENTIFIER   ::= { tlOperatingSystems 13 }

hpux11 OBJECT IDENTIFIER  ::= { tlOperatingSystems 14 }

win9x OBJECT IDENTIFIER   ::= { tlOperatingSystems 50 }

winnt OBJECT IDENTIFIER   ::= { tlOperatingSystems 51 }

solspark OBJECT IDENTIFIER  ::= { tlOperatingSystems 52 }

solintel OBJECT IDENTIFIER  ::= { tlOperatingSystems 53 }

aix OBJECT IDENTIFIER   ::= { tlOperatingSystems 54 }

sco OBJECT IDENTIFIER   ::= { tlOperatingSystems 55 }

osx OBJECT IDENTIFIER   ::= { tlOperatingSystems 56 }

unknown OBJECT IDENTIFIER   ::= { tlOperatingSystems 255 }


--------------------------------------------------------------------------
-- UPS Device
--------------------------------------------------------------------------

tlUPS OBJECT IDENTIFIER   ::= { tripplite 100 }

tlUpsObjects OBJECT IDENTIFIER  ::= { tlUPS 1 }

tlUpsIdent OBJECT IDENTIFIER  ::= { tlUpsObjects 1 }

tlUpsIdentUpsSoftwareChecksum OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "A checksum for the UPS fostware."
  ::= { tlUpsIdent 1 }

tlUpsIdentSerialNum OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "Serial number for the UPS."
  ::= { tlUpsIdent 2 }

tlUpsIdentID OBJECT-TYPE
  SYNTAX Integer32 (0..65535)
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "A user-supplied ID for the UPS."
  ::= { tlUpsIdent 3 }

tlUpsSnmpCardSerialNum OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "Serial number for the UPS."
  ::= { tlUpsIdent 4 }


tlUpsBattery OBJECT IDENTIFIER  ::= { tlUpsObjects 2 }

tlUpsBatteryAge OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The age of the battery, in the format YYYYMMDD.  This is equal to
    the current date minus tlConfigBattReplDate."
  ::= { tlUpsBattery 1 }


tlUpsTemperatureF OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The temperature of the battery, in Farenheight degrees.  This is
    calculated from upsBatteryTemperature, which is in Celsius degrees."
  ::= { tlUpsBattery 2 }


tlUpsInput OBJECT IDENTIFIER  ::= { tlUpsObjects 3 }

tlUpsOutput OBJECT IDENTIFIER   ::= { tlUpsObjects 4 }

tlUpsBypass OBJECT IDENTIFIER   ::= { tlUpsObjects 5 }

tlUpsAlarm OBJECT IDENTIFIER  ::= { tlUpsObjects 6 }

tlUpsAlarmsPresent OBJECT-TYPE
  SYNTAX Gauge32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The present number of active alarm conditions."
  ::= { tlUpsAlarm 1 }
  
tlUpsAlarmTable OBJECT-TYPE
  SYNTAX SEQUENCE OF TlUpsAlarmEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "A list of alarm table entries."
  ::= { tlUpsAlarm 2 }
  
tlUpsAlarmEntry OBJECT-TYPE
  SYNTAX TlUpsAlarmEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "An entry containing information applicable to a particular alarm."
  INDEX { tlUpsAlarmId }
  ::= { tlUpsAlarmTable 1 }
    
TlUpsAlarmEntry ::= SEQUENCE {
  tlUpsAlarmId         PositiveInteger,
  tlUpsAlarmDescr      AutonomousType,
  tlUpsAlarmTime       TimeStamp,
  tlUpsAlarmDetail     DisplayString,
  tlUpsAlarmDeviceId   PositiveInteger,
  tlUpsAlarmDeviceName DisplayString,
  tlUpsAlarmLocation   DisplayString,
  tlUpsAlarmGroup      INTEGER,
  tlUpsAlarmIp         IpAddress,
  tlUpsAlarmMac        DisplayString
}

tlUpsAlarmId OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "A unique identifier for an alarm condition."
  ::= { tlUpsAlarmEntry 1 }
  
tlUpsAlarmDescr OBJECT-TYPE
  SYNTAX STRING
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "A description of the alarm condition."
  ::= { tlUpsAlarmEntry 2 }
  
tlUpsAlarmTime OBJECT-TYPE
  SYNTAX INTEGER
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The value of sysUpTime when the alarm condition was detected."
  ::= { tlUpsAlarmEntry 3 }
  
tlUpsAlarmDetail OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "A textual description of the alarm condition."
  ::= { tlUpsAlarmEntry 4 }
  
tlUpsAlarmDeviceId OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "A numeric identifier for the device on which the alarm is active."
  ::= { tlUpsAlarmEntry 5 }
  
tlUpsAlarmDeviceName OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "A string identifier for the device on which the alarm is active."
  ::= { tlUpsAlarmEntry 6 }
  
tlUpsAlarmLocation OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The location of the device on which the alarm is active."
  ::= { tlUpsAlarmEntry 7 }
  
tlUpsAlarmGroup OBJECT-TYPE
  SYNTAX INTEGER {
      critical(1),
      warning(2),
      info(3),
      status(4),
      offline(5),
      custom(6) }
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The category/group of this alarm."
  ::= { tlUpsAlarmEntry 8 }

tlUpsAlarmIp OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The originating IP address associated with this alarm."
  ::= { tlUpsAlarmEntry 9 }

tlUpsAlarmMac OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The originating mac address associated with this alarm."
  ::= { tlUpsAlarmEntry 10 }

tlUpsWellKnownAlarms OBJECT IDENTIFIER  ::= { tlUpsAlarm 3 }

tlUpsAlarmPrimaryPowerOutage OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "The primary power source is not present."
    ::= { tlUpsWellKnownAlarms 1 }

tlUpsAlarmSecondaryPowerOutage OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "The secondary power source is not present."
    ::= { tlUpsWellKnownAlarms 2 }
    
tlUpsAlarmLoadLevelAboveThreshold OBJECT-IDENTITY
  STATUS current
  DESCRIPTION
    "The load level is above the designated threshold."
  ::= { tlUpsWellKnownAlarms 3 }

tlUpsAlarmOutputCurrentChanged OBJECT_IDENTITY
  STATUS current
  DESCRIPTION
    "The output current changed from its last known value."
  ::= { tlUpsWellKnownAlarms 4 }

tlUpsAlarmDevName OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS deprecated
  DESCRIPTION
    "The name of the device, tlDevName, corresponding to the device that is
    associated with this alarm."
  ::= { tlUpsAlarm 7 }

tlUpsAlarmDevLocation OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS deprecated
  DESCRIPTION
    "The location of the device, tlDevLocation, corresponding to the device
    that is associated with this alarm."
  ::= { tlUpsAlarm 8 }

tlUpsAlarmCategory OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS deprecated
  DESCRIPTION
    "The category, tlDevEvtCategory, of this alarm."
  ::= { tlUpsAlarm 9 }



tlUpsTest OBJECT IDENTIFIER   ::= { tlUpsObjects 7 }

tlUpsTestDate OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The date of the last self-test run on the ups, in the
    format YYYYMMDD."
  ::= { tlUpsTest 1 }

tlUpsTestResultsDetail OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "Result of the last self-test run on the ups."
  ::= { tlUpsTest 2 }

tlUpsControl OBJECT IDENTIFIER  ::= { tlUpsObjects 8 }

tlUpsWatchdogSupported OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "Indicates whether or not this UPS supports a watchdog reboot."
  ::= { tlUpsControl 1 }


tlUpsWatchdogSecsBeforeReboot OBJECT-TYPE
  SYNTAX NonNegativeInteger
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The maximum number of seconds that can expire between polls that
    the engine makes to the UPS for data.  If this time runs out, then
    the UPS will cycle its outputs.  Set this to zero to turns disable
    this feature."
  ::= { tlUpsControl 2 }

tlUpsWellKnownControls OBJECT IDENTIFIER  ::= { tlUpsControl 3 }

tlUpsControlSelfTest OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "Set to TRUE to initiate Self Test"
  ::= { tlUpsWellKnownControls 1 }
  
tlUpsControlRamp OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "Set to TRUE to initiate Ramp"
  ::= { tlUpsWellKnownControls 2 }
  
tlUpsControlShed OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "Set to TRUE to initiate Shed"
  ::= { tlUpsWellKnownControls 3 }
  
tlUpsControlUpsOn OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "Set to TRUE to turn UPS on"
  ::= { tlUpsWellKnownControls 4 }

tlUpsControlUpsOff OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "Set to TRUE to turn UPS off"
  ::= { tlUpsWellKnownControls 5 }
  
tlUpsConfig OBJECT IDENTIFIER   ::= { tlUpsObjects 9 }

tlUpsConfigBattReplDate OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The date on which the battery was last replaced, in the format
    YYYYMMDD."
  ::= { tlUpsConfig 1 }

tlUpsConfigTftpGetAddr OBJECT-TYPE
  SYNTAX IpAddress
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The IP address of the TFTP server you wish to acquire a config ini file from, non persistent, 0.0.0.0 when empty"
  ::= { tlUpsConfig 2 }

tlUpsConfigTftpGetAcction OBJECT-TYPE
  SYNTAX INTEGER {
      get(1),
      getting(2),
      idle(3) }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "setting this entry to get(1) will start a down load from the specified address, during the download this entry
    will read getting(2), when finished, the card will reboot to the new ini supplied parms. At all other times this 
    entry will read idle(3)"
  ::= { tlUpsConfig 3 }


tlUpsOutlet OBJECT IDENTIFIER   ::= { tlUpsObjects 10 }

tlUpsOutletNumOutlets OBJECT-TYPE
  SYNTAX NonNegativeInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The number of available Outlets in this device."
  ::= { tlUpsOutlet 1 }

tlUpsOutletTable OBJECT-TYPE
  SYNTAX SEQUENCE OF TlUpsOutletEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "A list of all device Outlets for all devices."
  ::= { tlUpsOutlet 2 }

tlUpsOutletEntry OBJECT-TYPE
  SYNTAX TlUpsOutletEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "An entry containing Outlet information applicable to a particular
    device managed by this agent."
  INDEX {
    tlUpsOutletIndex }
  ::= { tlUpsOutletTable 1 }

TlUpsOutletEntry ::= SEQUENCE {
  tlUpsOutletIndex        PositiveInteger,
  tlUpsOutletState        INTEGER,
  tlUpsOutletType         Integer32,
  tlUpsOutletControl      INTEGER,
  tlUpsOutletName         DisplayString,
  tlUpsOutletRampAction   INTEGER,
  tlUpsOutletRampDataType INTEGER,
  tlUpsOutletRampData     Integer32,
  tlUpsOutletShedAction   INTEGER,
  tlUpsOutletShedDataType INTEGER,
  tlUpsOutletShedData     Integer32,
  tlUpsOutletGroupNdx     Integer32 }

tlUpsOutletIndex OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "This is the index number of this Outlet for the device
    indicated by tlDeviceIndex."
  ::= { tlUpsOutletEntry 1 }

tlUpsOutletState OBJECT-TYPE
  SYNTAX INTEGER {
      unknown(0),
      off(1),
      on(2) }
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The current state of the Outlet."
  ::= { tlUpsOutletEntry 2 }

tlUpsOutletType OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "This is a bit field that indicates the type of this Outlet.

    Bit   Display
     0    Battery Protected
     1    Controllable
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    "
  ::= { tlUpsOutletEntry 3 }

tlUpsOutletControl OBJECT-TYPE
  SYNTAX INTEGER {
      turnOff(1),
      turnOn(2),
      cycle(3) }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "Controls the state of the Outlet."
  ::= { tlUpsOutletEntry 4 }

tlUpsOutletName OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "A string identifying the devices attached to the
    output(s) of the device."
  ::= { tlUpsOutletEntry 5 }


tlUpsOutletRampAction OBJECT-TYPE
  SYNTAX INTEGER {
      remainOff(0),
      turnOnAfterDelay(1)
   }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The ramp action to take on the Outlet."
  ::= { tlUpsOutletEntry 6 }

tlUpsOutletRampDataType OBJECT-TYPE
  SYNTAX INTEGER {
      delayInSeconds(0)
   }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The type of data associated with ramp action."
  ::= { tlUpsOutletEntry 7 }

tlUpsOutletRampData OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The data value associated with type of ramp data."
  ::= { tlUpsOutletEntry 8 }

tlUpsOutletShedAction OBJECT-TYPE
  SYNTAX INTEGER {
      remainOn(0),
      turnOffAfterDelay(1)
   }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The shed action to take on the Outlet."
  ::= { tlUpsOutletEntry 9 }

tlUpsOutletShedDataType OBJECT-TYPE
  SYNTAX INTEGER {
      delayInSeconds(0)
   }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The type of data associated with shed action."
  ::= { tlUpsOutletEntry 10 }

tlUpsOutletShedData OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The data value associated with type of shed data."
  ::= { tlUpsOutletEntry 11 }

tlUpsOutletGroupNdx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "tlUpsOutletGroupIndex of corresponding outlet group, or 0 if ungrouped."
  ::= { tlUpsOutletEntry 12 }


tlUpsOutletCurrentTable OBJECT-TYPE
  SYNTAX SEQUENCE OF TlUpsOutletCurrentEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "A list of load currents."
  ::= { tlUpsOutlet 3 }
  
tlUpsOutletCurrentEntry OBJECT-TYPE
  SYNTAX TlUpsOutletCurrentEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "An entry containing Outlet current information applicable to a particular
    device managed by this agent."
  INDEX {
    tlUpsOutletCurrentIndex }
  ::= { tlUpsOutletCurrentTable 1 }

TlUpsOutletCurrentEntry ::= SEQUENCE {
  tlUpsOutletCurrentIndex      PositiveInteger,
  tlUpsOutletCurrentValue      PositiveInteger }

tlUpsOutletCurrentIndex OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "This is the index number of this Outlet."
  ::= { tlUpsOutletCurrentEntry 1 }

tlUpsOutletCurrentValue OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The value of this outlet's current, represented as 0.1A"
  ::= { tlUpsOutletCurrentEntry 2 }


tlUpsOutletPowerTable OBJECT-TYPE
  SYNTAX SEQUENCE OF TlUpsOutletPowerEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "A list of load power."
  ::= { tlUpsOutlet 4 }
  
tlUpsOutletPowerEntry OBJECT-TYPE
  SYNTAX TlUpsOutletPowerEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "An entry containing Outlet power information applicable to a particular
    device managed by this agent."
  INDEX {
    tlUpsOutletPowerIndex }
  ::= { tlUpsOutletPowerTable 1 }

TlUpsOutletPowerEntry ::= SEQUENCE {
  tlUpsOutletPowerIndex      PositiveInteger,
  tlUpsOutletPowerValue      PositiveInteger }

tlUpsOutletPowerIndex OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "This is the index number of this Outlet."
  ::= { tlUpsOutletPowerEntry 1 }

tlUpsOutletPowerValue OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The value of this outlet's power in watts."
  ::= { tlUpsOutletPowerEntry 2 }


tlUpsOutletGroup OBJECT IDENTIFIER   ::= { tlUpsObjects 11 }

tlUpsOutletNumOutletGroups OBJECT-TYPE
  SYNTAX NonNegativeInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The number of available Outlet Groups in this device."
  ::= { tlUpsOutletGroup 1 }

tlUpsOutletGroupTable OBJECT-TYPE
  SYNTAX SEQUENCE OF TlUpsOutletGroupEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "A list of device outlet group entries. The number of entries is
    given by the value of tlUpsOutletNumOutletGroups."
  ::= { tlUpsOutletGroup 2 }
  
tlUpsOutletGroupEntry OBJECT-TYPE
  SYNTAX TlUpsOutletGroupEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "An entry containing outlet group information applicable
     to a particular device managed by this agent"
  INDEX { tlUpsOutletGroupIndex }
  ::= { tlUpsOutletGroupTable 1 }

TlUpsOutletGroupEntry ::= SEQUENCE {
  tlUpsOutletGroupIndex     PositiveInteger,
  tlUpsOutletGroupUnused	Integer32,
  tlUpsOutletGroupName      DisplayString,
  tlUpsOutletGroupDesc      DisplayString,
  tlUpsOutletGroupState     INTEGER,
  tlUpsOutletGroupControl   INTEGER }

tlUpsOutletGroupIndex OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "This is the index number of this load group for the device."
  ::= { tlUpsOutletGroupEntry 1 }

tlUpsOutletGroupUnused OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "Unused placeholder"
  ::= { tlUpsOutletGroupEntry 2 }

tlUpsOutletGroupName OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The name of this outlet group."
  ::= { tlUpsOutletGroupEntry 3 }

tlUpsOutletGroupDesc OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "A description for this outlet group."
  ::= { tlUpsOutletGroupEntry 4 }

tlUpsOutletGroupState OBJECT-TYPE
  SYNTAX INTEGER {
      unknown(0),
      off(1),
      on(2),
      mixed(3) }
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The current state of the outlet group."
  ::= { tlUpsOutletGroupEntry 5 }

tlUpsOutletGroupControl OBJECT-TYPE
  SYNTAX INTEGER {
      turnOff(1),
      turnOn(2),
      cycle(3) }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "Controls the state of every outlet associated with the group."
  ::= { tlUpsOutletGroupEntry 6 }


tlUpsTraps              OBJECT IDENTIFIER ::= { tlUPS 2 }

tlUpsTrapAlarmEntryAddedV1 TRAP-TYPE
    ENTERPRISE tlUpsTraps
    VARIABLES { tlUpsAlarmId, tlUpsAlarmDescr, tlUpsAlarmDetail, tlUpsAlarmDeviceId,
                tlUpsAlarmDeviceName, tlUpsAlarmLocation, tlUpsAlarmGroup }
    DESCRIPTION
            "This trap is sent each time an alarm is inserted into
            to the alarm table."
    --#SUMMARY "UPS Alarm: %s - %s."
    --#ARGUMENTS {6, 2}
    --#SEVERITY WARNING
 ::= 3

tlUpsTrapAlarmEntryAdded NOTIFICATION-TYPE
    OBJECTS { tlUpsAlarmId, tlUpsAlarmDescr, tlUpsAlarmDetail, tlUpsAlarmDeviceId,
              tlUpsAlarmDeviceName, tlUpsAlarmLocation, tlUpsAlarmGroup }
    STATUS  current
    DESCRIPTION
            "This trap is sent each time an alarm is inserted into
            to the alarm table."
    --#SUMMARY "UPS Alarm: %s - %s."
    --#ARGUMENTS {6, 2}
    --#SEVERITY WARNING
    ::= { tlUpsTraps 3 }

tlUpsTrapAlarmEntryRemovedV1 TRAP-TYPE
    ENTERPRISE tlUpsTraps
    VARIABLES { tlUpsAlarmId, tlUpsAlarmDescr, tlUpsAlarmDetail, tlUpsAlarmDeviceId,
                tlUpsAlarmDeviceName, tlUpsAlarmLocation, tlUpsAlarmGroup }
    DESCRIPTION
            "This trap is sent each time an alarm is removed from
            the alarm table."
    --#SUMMARY "UPS Alarm: %s - %s."
    --#ARGUMENTS {6, 2}
    --#SEVERITY WARNING
 ::= 4

tlUpsTrapAlarmEntryRemoved NOTIFICATION-TYPE
    OBJECTS { tlUpsAlarmId, tlUpsAlarmDescr, tlUpsAlarmDetail, tlUpsAlarmDeviceId,
              tlUpsAlarmDeviceName, tlUpsAlarmLocation, tlUpsAlarmGroup }
    STATUS  current
    DESCRIPTION
            "This trap is sent each time an alarm is removed from
            the alarm table."
    --#SUMMARY "UPS Alarm: %s - %s."
    --#ARGUMENTS {6, 2}
    --#SEVERITY WARNING
    ::= { tlUpsTraps 4 }


--------------------------------------------------------------------------
-- EnviroSense Device
--------------------------------------------------------------------------

tlEnviroSense OBJECT IDENTIFIER   ::= { tripplite 101 }

tlEnvEnvironment OBJECT IDENTIFIER   ::= { tlEnviroSense 1 }

tlEnvTemperatureData OBJECT IDENTIFIER   ::= { tlEnvEnvironment 1 }

tlEnvTemperatureC OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The ambient temperature (C)."
  ::= { tlEnvTemperatureData 1 }

tlEnvTemperatureF OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The ambient temperature (F)."
  ::= { tlEnvTemperatureData 2 }

tlEnvTemperatureLowLimit OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The lower alarm limit for ambient temperature (F)."
  ::= { tlEnvTemperatureData 3 }

tlEnvTemperatureHighLimit OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The upper alarm limit for ambient temperature (F)."
  ::= { tlEnvTemperatureData 4 }

tlEnvTemperatureInAlarm OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "Indicates whether or not temperature is in alarm."
  ::= { tlEnvTemperatureData 5 }

tlEnvHumidityData OBJECT IDENTIFIER   ::= { tlEnvEnvironment 2 }

tlEnvHumidity OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The ambient humidity (%)."
  ::= { tlEnvHumidityData 1 }

tlEnvHumidityLowLimit OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The lower alarm limit for ambient humidity (%)."
  ::= { tlEnvHumidityData 2 }

tlEnvHumidityHighLimit OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The upper alarm limit for ambient humidity (%)."
  ::= { tlEnvHumidityData 3 }

tlEnvHumidityInAlarm OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "Indicates whether or not humidity is in alarm."
  ::= { tlEnvHumidityData 4 }

tlEnvContacts OBJECT IDENTIFIER  ::= { tlEnviroSense 2 }

tlEnvContactTable OBJECT-TYPE
  SYNTAX SEQUENCE OF TlEnvContactEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "A table of contacts."
  ::= { tlEnvContacts 1 }

tlEnvContactEntry OBJECT-TYPE
  SYNTAX TlEnvContactEntry
  MAX-ACCESS not-accessible
  STATUS current
  DESCRIPTION
    "An entry containing information applicable to a particular contact."
  INDEX {
    tlEnvContactIndex }
  ::= { tlEnvContactTable 1 }

TlEnvContactEntry ::= SEQUENCE {
  tlEnvContactIndex    PositiveInteger,
  tlEnvContactName     DisplayString,
  tlEnvContactStatus   INTEGER,
  tlEnvContactConfig   INTEGER }

tlEnvContactIndex OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The table row index for the contact."
  ::= { tlEnvContactEntry 1 }

tlEnvContactName OBJECT-TYPE
  SYNTAX DisplayString
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The name or description of the contact."
  ::= { tlEnvContactEntry 2 }

tlEnvContactStatus OBJECT-TYPE
  SYNTAX INTEGER {
      normal(0),
      alarm(1) }
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
    "The current status of the contact."
  ::= { tlEnvContactEntry 3 }

tlEnvContactConfig OBJECT-TYPE
  SYNTAX INTEGER {
      normallyOpen(0),
      normallyClosed(1) }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The configuration of the contact."
  ::= { tlEnvContactEntry 4 }


--------------------------------------------------------------------------
-- KVM over IP Device
--------------------------------------------------------------------------

-- this is a 3rd party MIB structure located at { tripplite 102 }

--------------------------------------------------------------------------
-- Conformance definitions
--------------------------------------------------------------------------

tlConformance OBJECT IDENTIFIER   ::= { tripplite 20 }

tlCompliances OBJECT IDENTIFIER   ::= { tlConformance 1 }

tlGroups OBJECT IDENTIFIER  ::= { tlConformance 2 }

tlSubsetGroups OBJECT IDENTIFIER  ::= { tlGroups 1 }

tlBasicGroups OBJECT IDENTIFIER   ::= { tlGroups 2 }

tlFullGroups OBJECT IDENTIFIER  ::= { tlGroups 3 }


tlV11Groups OBJECT IDENTIFIER  ::= { tlGroups 4 }

tlDeprecatedV11Group OBJECT-GROUP
  OBJECTS {
    upsTrapCode,
    upsTrapDescription }
  STATUS obsolete
  DESCRIPTION
    "The tlDeprecatedV11Group defines objects which were used by
    Sinetica SNMP cards on Tripplite UPSs and PowerAlert version 11.
    These objects are currently only used when
    tlEngineLegacySNMPSupport == true."
  ::= { tlV11Groups 1 }

tlDeprecatedV11NotificationsGroup NOTIFICATION-GROUP
  NOTIFICATIONS {
    tlV11upsCritical,
    tlV11upsWarning,
    tlV11upsInformation,
    tlV11upsAlarmCleared,
    tlV11upsAgentStarted,
    tlV11upsAgentStopped }
  STATUS obsolete
  DESCRIPTION
    "The tlDeprecatedV11NotificationsGroup defines PowerAlert version 11
    notifications.  These notifications are being deprecated, but may
    still be used when tlEngineLegacySNMPSupport = true."
  ::= { tlV11Groups 2 }

tlObsoleteV11Group OBJECT-GROUP
  OBJECTS {
    upsReceptaclesNumReceptacles,
    upsReceptacleIndex,
    upsReceptacleType,
    upsReceptacleStatus,
    upsReceptacleControl,
    upsEnvTemperature,
    upsEnvHumidity,
    upsContactIndex,
    upsContactName,
    upsContactStatus,
    upsContactConfig }
  STATUS obsolete
  DESCRIPTION
    "The tlObsoleteV11Group defines objects which were used by
    Sinetica SNMP cards on Tripplite UPSs.  Most of these objects are obsolete."
  ::= { tlV11Groups 3 }


-- tlUpsCompliances OBJECT IDENTIFIER ::= { tlCompliances 1 }
--
-- tlUpsSubsetCompliance MODULE-COMPLIANCE
--   STATUS current
--   DESCRIPTION
--     "Description"
--   MODULE == this module
--     MANDATORY-GROUPS {
--       groups}
--
--   OBJECT tlUpsOBJECT1
--   SYNTAX INTEGER {
--     enum1(1),
--     enum2(2)
--   }
--   DESCRIPTION
--     "Description"
--
--   OBJECT tlUpsOBJECT2
--   DESCRIPTION
--     "Description"
--
--   OBJECT tlUpsOBJECT3
--   MIN-ACCESS read-only
--   DESCRIPTION
--     "Description"
--   ::= { tlUpsCompliances 1 }
--
-- tlUpsBasicCompliance MODULE-COMPLIANCE
--   ...
--   ::= { tlUpsCompliances 2 }
--
-- tlUpsFullCompliance MODULE-COMPLIANCE
--   ...
--   ::= { tlUpsCompliances 3 }
--
-- units of conformance
--
-- summary at a glance:
--                                      subset  basic   full
--tlUpsIdentUPSSoftwareChecksum                         x
--tlUpsIdentSerialNum                                   x
--tlUpsIdentID                                          x
--
--tlUpsBatteryAge                                       x
--tlUpsBatteryTemperatureF                              x
--
--tlUpsAlarm
--
--tlUpsTestDate                                         x
--
--tlUpsWatchdogSupported                                x
--tlUpsWatchdogSecsBeforeReboot                         x
--
--tlUpsConfigBattReplDate                               x
--
--tlUpsLoadNumLoads                                     x
--
--tlUpsNotificationCode                                         x
--tlUpsNotificationDescription                                  x
--
--tlUpsCritical                                         x
--tlUpsWarning                                          x
--tlUpsInformation                                      x
--tlUpsAlarmCleared                                     x
--tlUpsAgentStarted                                     x
--tlUpsAgentStopped                                     x
--
--tlUpsSubsetGroups OBJECT IDENTIFIER   ::= { tlSubsetGroups 100 }
--
--tlUpsBasicGroups OBJECT IDENTIFIER  ::= { tlBasicGroups 100 }

tlUpsFullGroups OBJECT IDENTIFIER   ::= { tlFullGroups 100 }

tlUpsFullIdentGroup OBJECT-GROUP
  OBJECTS {
    tlUpsIdentUpsSoftwareChecksum,
    tlUpsIdentSerialNum,
    tlUpsIdentID }
  STATUS current
  DESCRIPTION
    "The tlUpsFullIdentGroup defines objects which are common to the Ident
    group of fully compliant Tripplite UPS's"
  ::= { tlUpsFullGroups 1 }

tlUpsFullBatteryGroup OBJECT-GROUP
  OBJECTS {
    tlUpsBatteryAge,
    tlUpsTemperatureF }
  STATUS current
  DESCRIPTION
    "The tlUpsFullBatteryGroup defines objects which are common to the Battery
    group of fully compliant Tripplite UPS's"
  ::= { tlUpsFullGroups 2 }

tlUpsFullAlarmGroup OBJECT IDENTIFIER   ::= { tlUpsFullGroups 6 }

tlUpsFullAlarmObjsGroup OBJECT-GROUP
  OBJECTS {
    tlUpsAlarmDevName,
    tlUpsAlarmDevLocation,
    tlUpsAlarmCategory }
  STATUS current
  DESCRIPTION
    "The tlUpsFullAlarmObjsGroup defines objects which are common to
    the Alarm group of fully compliant Tripplite UPS's"
  ::= { tlUpsFullAlarmGroup 1 }

--tlUpsFullAlarmsGroup NOTIFICATION-GROUP
--  NOTIFICATIONS { }
--  STATUS current
--  DESCRIPTION
--    "The tlUpsFullAlarmGroup defines notifications which are
--    common to the Alarm group of fully compliant Tripplite UPS's"
--  ::= { tlUpsFullAlarmGroup 2 }

tlUpsFullTestGroup OBJECT-GROUP
  OBJECTS {
    tlUpsTestDate,
    tlUpsTestResultsDetail }
  STATUS current
  DESCRIPTION
    "The tlUpsFullTestGroup defines objects which are common to the Test
    group of fully compliant Tripplite UPS's"
  ::= { tlUpsFullGroups 7 }

tlUpsFullControlGroup OBJECT-GROUP
  OBJECTS {
    tlUpsWatchdogSupported,
    tlUpsWatchdogSecsBeforeReboot }
  STATUS current
  DESCRIPTION
    "The tlUpsFullControlGroup defines objects which are common to the Control
    group of fully compliant Tripplite UPS's"
  ::= { tlUpsFullGroups 8 }

tlUpsFullConfigGroup OBJECT-GROUP
  OBJECTS {
    tlUpsConfigBattReplDate }
  STATUS current
  DESCRIPTION
    "The tlUpsFullConfigGroup defines objects which are common to the Config
    group of fully compliant Tripplite UPS's"
  ::= { tlUpsFullGroups 9 }

tlUpsFullOutletGroup OBJECT-GROUP
  OBJECTS {
    tlUpsOutletNumOutlets }
  STATUS current
  DESCRIPTION
    "The tlUpsFullOutletGroup defines objects which are common to the Outlet
    group of fully compliant Tripplite UPS's"
  ::= { tlUpsFullGroups 10 }

--------------------------------------------------------------------------
-- Legacy (PowerAlert version 11) objects
--
-- These objects have been published in previous Tripplite MIBs and are
-- no longer supported, except where otherwise indicated.
--------------------------------------------------------------------------

trippUPS OBJECT IDENTIFIER  ::= { tripplite 1 }

trippUpsReceptacles OBJECT IDENTIFIER   ::= { trippUPS 1 }

upsReceptaclesNumReceptacles OBJECT-TYPE
  SYNTAX NonNegativeInteger
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The number of available receptacles in this device.
    This variable indicates the number of rows in the
    receptacle table."
  ::= { trippUpsReceptacles 1 }


upsReceptacleTable OBJECT-TYPE
  SYNTAX SEQUENCE OF UpsReceptacleEntry
  MAX-ACCESS not-accessible
  STATUS obsolete
  DESCRIPTION
    "A list of receptacle table entries.  The number of entries
    is given by the value of upsReceptaclesNumReceptacles."
  ::= { trippUpsReceptacles 2 }


upsReceptacleEntry OBJECT-TYPE
  SYNTAX UpsReceptacleEntry
  MAX-ACCESS not-accessible
  STATUS obsolete
  DESCRIPTION
    "An entry containing information applicable to a
    particular receptacle."
  INDEX {
    upsReceptacleIndex }
  ::= { upsReceptacleTable 1 }


UpsReceptacleEntry ::= SEQUENCE {
  upsReceptacleIndex   PositiveInteger,
  upsReceptacleType    INTEGER,
  upsReceptacleStatus  INTEGER,
  upsReceptacleControl INTEGER }


upsReceptacleIndex OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The receptacle identifier."
  ::= { upsReceptacleEntry 1 }


upsReceptacleType OBJECT-TYPE
  SYNTAX INTEGER {
      surgeOnly(1),
      batteryProtected(2),
      controllableBatteryProtected(3) }
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The type of receptacle."
  ::= { upsReceptacleEntry 2 }


upsReceptacleStatus OBJECT-TYPE
  SYNTAX INTEGER {
      on(1),
      off(2),
      unknown(3) }
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The status of receptacle."
  ::= { upsReceptacleEntry 3 }


upsReceptacleControl OBJECT-TYPE
  SYNTAX INTEGER {
      on(1),
      off(2),
      cycle(3) }
  MAX-ACCESS read-write
  STATUS obsolete
  DESCRIPTION
    "Setting this object to 'on' will turn on the receptacle.
    Setting this object to 'off' will turn off the receptacle.
    Setting this object to 'cycle' will turn off and then turn
    on the receptacle.  This action will only take place if the
    receptacle is controllable
    (upsReceptacleType = controllableBatteryProtected(3))."
  ::= { upsReceptacleEntry 4 }


trippUpsTrapInfo OBJECT IDENTIFIER  ::= { trippUPS 2 }

upsTrapCode OBJECT-TYPE
  SYNTAX INTEGER (0..2147483647)
  MAX-ACCESS read-only
  STATUS deprecated
  DESCRIPTION
    "A numeric code identifiying the condition that caused the trap to be sent.
    If the trap number is 104 (upsAgentStarted) or 105 (upsAgentStopped), this
    code will indicate whether the SNMP agent is software (1) or hardware (2)."
  ::= { trippUpsTrapInfo 1 }


upsTrapDescription OBJECT-TYPE
  SYNTAX DisplayString (SIZE (0..63))
  MAX-ACCESS read-only
  STATUS deprecated
  DESCRIPTION
    "The description of the trap."
  ::= { trippUpsTrapInfo 2 }


trippUpsEnvironment OBJECT IDENTIFIER   ::= { trippUPS 3 }

upsEnvTemperature OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The ambient temperature of the EnviroSense unit (1/10 Deg C)."
  ::= { trippUpsEnvironment 1 }


upsEnvHumidity OBJECT-TYPE
  SYNTAX INTEGER (0..100)
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The ambient humidity of the EnviroSense unit (% Humidity)."
  ::= { trippUpsEnvironment 2 }


trippUpsContacts OBJECT IDENTIFIER  ::= { trippUPS 4 }

upsContactTable OBJECT-TYPE
  SYNTAX SEQUENCE OF UpsContactEntry
  MAX-ACCESS not-accessible
  STATUS obsolete
  DESCRIPTION
    "A table of contacts attached to the EnviroSense unit."
  ::= { trippUpsContacts 1 }


upsContactEntry OBJECT-TYPE
  SYNTAX UpsContactEntry
  MAX-ACCESS not-accessible
  STATUS obsolete
  DESCRIPTION
    "An entry containing information applicable to a
    particular contact."
  INDEX {
    upsContactIndex }
  ::= { upsContactTable 1 }


UpsContactEntry ::= SEQUENCE {
  upsContactIndex  PositiveInteger,
  upsContactName   DisplayString,
  upsContactStatus INTEGER,
  upsContactConfig INTEGER }


upsContactIndex OBJECT-TYPE
  SYNTAX PositiveInteger
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The contact identifier."
  ::= { upsContactEntry 1 }


upsContactName OBJECT-TYPE
  SYNTAX DisplayString (SIZE (0..15))
  MAX-ACCESS read-write
  STATUS obsolete
  DESCRIPTION
    "The contact name."
  ::= { upsContactEntry 2 }


upsContactStatus OBJECT-TYPE
  SYNTAX INTEGER {
      unknown(0),
      normal(1),
      alarm(2) }
  MAX-ACCESS read-only
  STATUS obsolete
  DESCRIPTION
    "The current status of the contact."
  ::= { upsContactEntry 3 }


upsContactConfig OBJECT-TYPE
  SYNTAX INTEGER {
      normallyClosed(0),
      normallyOpen(1) }
  MAX-ACCESS read-write
  STATUS obsolete
  DESCRIPTION
    "The default configuration of the contact."
  ::= { upsContactEntry 4 }


--------------------------------------------------------------------------
-- Legacy (PowerAlert version 11) traps, redefined as notifications.
--
-- These notifications define the traps used in previous Tripplite MIBs and
-- are only supported when legacy support is enabled, as indicated by
-- tlEngineLegacySNMPSupport
--------------------------------------------------------------------------

tlV11TrapsPrefix OBJECT IDENTIFIER  ::= { trippUPS 0 }

tlV11upsCritical NOTIFICATION-TYPE
  OBJECTS {
    upsTrapCode,
    upsTrapDescription }
  STATUS obsolete
  DESCRIPTION
    "UPS Critical Alarm."
  ::= { tlV11TrapsPrefix 100 }


tlV11upsWarning NOTIFICATION-TYPE
  OBJECTS {
    upsTrapCode,
    upsTrapDescription}
  STATUS obsolete
  DESCRIPTION
    "UPS Warning."
  ::= { tlV11TrapsPrefix 101 }


tlV11upsInformation NOTIFICATION-TYPE
  OBJECTS {
    upsTrapCode,
    upsTrapDescription}
  STATUS obsolete
  DESCRIPTION
    "UPS Information."
  ::= { tlV11TrapsPrefix 102 }


tlV11upsAlarmCleared NOTIFICATION-TYPE
  OBJECTS {
    upsTrapCode,
    upsTrapDescription}
  STATUS obsolete
  DESCRIPTION
    "UPS Alarm Cleared."
  ::= { tlV11TrapsPrefix 103 }


tlV11upsAgentStarted NOTIFICATION-TYPE
  OBJECTS {
    upsTrapCode,
    upsTrapDescription}
  STATUS obsolete
  DESCRIPTION
    "Agent started."
  ::= { tlV11TrapsPrefix 104 }


tlV11upsAgentStopped NOTIFICATION-TYPE
  OBJECTS {
    upsTrapCode,
    upsTrapDescription}
  STATUS obsolete
  DESCRIPTION
    "Agent stopped."
  ::= { tlV11TrapsPrefix 105 }


--------------------------------------------------------------------------
-- This is an excerpt from the TRIPPUPS-MIB used for Delta SNMP cards in
-- Tripplite UPSs.  It has major fundamental problems with OID collisions
-- and naming collosions, so it's commented out in its entirety.  It's
-- only included for historical documentation purposes.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- BEGIN Delta SNMP MIB
--------------------------------------------------------------------------
-- ups OBJECT IDENTIFIER   ::= { trippUPS 1 }
--
-- upsIdent OBJECT IDENTIFIER  ::= { ups 1 }
--
-- upsBattery OBJECT IDENTIFIER  ::= { ups 2 }
--
-- upsInput OBJECT IDENTIFIER  ::= { ups 3 }
--
-- upsOutput OBJECT IDENTIFIER   ::= { ups 4 }
--
-- upsAlarm OBJECT IDENTIFIER  ::= { ups 6 }
--
-- upsWellKnownAlarms OBJECT IDENTIFIER  ::= { ups 7 }
--
-- upsTest OBJECT IDENTIFIER   ::= { ups 8 }
--
-- upsControl OBJECT IDENTIFIER  ::= { ups 9 }
--
-- upsConfig OBJECT IDENTIFIER   ::= { ups 10 }
--
-- The Device Identification group.
-- All objects in this group are set at device initialization and remain static.
--
-- upsIdentManufacturer OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..31))
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The name of the UPS manufacturer."
--   ::= { upsIdent 1 }
--
--
-- upsIdentModel OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..63))
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The UPS Model designation."
--   ::= { upsIdent 2 }
--
--
-- upsIdentUPSSoftwareVersion OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..63))
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The UPS Firmware software version(s).  This variable
--     may or may not have the same value as
--     upsIdentAgentSoftwareVersion in some implementations."
--   ::= { upsIdent 3 }
--
--
-- upsIdentAgentSoftwareVersion OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..63))
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The UPS agent software version.  This variable may or
--     may not have the same value as
--     upsIdentUPSSoftwareVersion in some implementations."
--   ::= { upsIdent 4 }
--
--
-- upsIdentName OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..63))
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "A string identifying the UPS.  This object should be
--     set by the administrator."
--   ::= { upsIdent 5 }
--
--
-- upsIdentAttachedDevices OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..63))
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "A string identifying the devices attached to the
--     output(s) of the UPS.  This object should be set by
--     the administrator."
--   ::= { upsIdent 6 }
--
--
-- The Battery group.
-- Implementation of this group is mandatory for all systems.
--
-- upsBatteryStatus OBJECT-TYPE
--   SYNTAX INTEGER {
--       unknown(1),
--       batteryNormal(2),
--       batteryLow(3),
--       batteryDepleted(4) }
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The indication of the capacity remaining in the UPS
--     system's batteries.  A value of batteryNormal
--     indicates that the batteries are fully charged.  A
--     value of batteryLow indicates that the remaining battery
--     run-time is less than or equal to
--     upsConfigMinutesRemaining.  A value of batteryDepleted
--     indicates that the UPS will be unable to sustain the
--     present load when and if the utility power is lost."
--   ::= { upsBattery 1 }
--
--
-- upsSecondsOnBattery OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "If the unit is on battery power, the elapsed time
--     since the UPS last switched to battery power, or the
--     time since the network management subsystem was last
--     restarted, whichever is less.  Zero shall be returned
--     if the unit is not on battery power. UNITS - seconds"
--   ::= { upsBattery 2 }
--
--
-- upsEstimatedMinutesRemaining OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "An estimate of the time to battery charge depletion
--     under the present load conditions if the utility power
--     were to be lost and remain off. UNITS - minutes"
--   ::= { upsBattery 3 }
--
--
-- upsBatteryChargeRemaining OBJECT-TYPE
--   SYNTAX INTEGER (0..100)
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The estimate of the battery charge remaining expressed
--     as a percent of full charge."
--   ::= { upsBattery 4 }
--
--
-- upsBatteryVoltage OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The magnitude of the present battery voltage.   UNITS  0.1 Volt DC."
--   ::= { upsBattery 5 }
--
--
--------------------------------------------------------------------------
-- Note : upsBatteryCurrent MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB,  {upsBattery 6 }  is reserved.
--------------------------------------------------------------------------
--
-- upsBatteryTemperature OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The ambient temperature at or near the UPS Battery.
--     UNITS degrees Centigrade"
--   ::= { upsBattery 7 }
--
--
-- the table group has one attribute of its own - the number of rows in the
-- contained table.  It also contains the table of names.
-- The Input group.
-- Implementation of this group is mandatory for all systems.
--
-- upsInputFrequency OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The present input frequency.  UNITS  0.1 Hertz"
--   ::= { upsInput 1 }
--
--
-- upsInputLineBads OBJECT-TYPE
--   SYNTAX Counter
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A count of the number of times the input entered an
--     out-of-tolerance condition as defined by the manufacturer."
--   ::= { upsInput 2 }
--
--
-- upsInputNumLines OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The number of input lines utilized in this device.
--     This variable indicates the number of rows in the input table."
--   ::= { upsInput 3 }
--
--
-- upsInputVolt OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The magnitude of the present input voltage.
--     UNITS     RMS Volts"
--   ::= { upsInput 4 }
--
--
-- upsInputTable OBJECT-TYPE
--   SYNTAX SEQUENCE OF UpsInputEntry
--   ACCESS not-accessible
--   STATUS obsolete
--   DESCRIPTION
--     "A list of input table entries.  The number of entries
--     is given by the value of upsInputNumLines."
--   ::= { upsInput 5 }
--
--
-- upsInputEntry OBJECT-TYPE
--   SYNTAX UpsInputEntry
--   ACCESS not-accessible
--   STATUS obsolete
--   DESCRIPTION
--     "An entry containing information applicable to a
--     particular input line."
--   INDEX {
--     upsInputLineIndex }
--   ::= { upsInputTable 1 }
--
--
-- UpsInputEntry ::= SEQUENCE {
--   upsInputLineIndex INTEGER,
--   upsInputVoltage   INTEGER }
--
--
-- upsInputLineIndex OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The input line identifier."
--   ::= { upsInputEntry 1 }
--
--
-- upsInputVoltage OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The magnitude of the present input voltage.
--     UNITS     RMS Volts"
--   ::= { upsInputEntry 2 }
--
--
-- The Output group.
-- Implementation of this group is mandatory for all systems.
--
-- upsOutputSource OBJECT-TYPE
--   SYNTAX INTEGER {
--       other(1),
--       none(2),
--       normal(3),
--       bypass(4),
--       battery(5),
--       booster(6),
--       reducer(7) }
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The present source of output power."
--   ::= { upsOutput 1 }
--
--
-- upsOutputFrequency OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The present output frequency.
--     UNITS     0.1 Hertz"
--   ::= { upsOutput 2 }
--
--
-- upsOutputNumLines OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The number of output lines utilized in this device.
--     This variable indicates the number of rows in the output table."
--   ::= { upsOutput 3 }
--
--
-- upsOutputPercLoad OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The percentage of true power capacity presently being used.
--     UNITS     percent"
--   ::= { upsOutput 4 }
--
--
-- upsOutputTable OBJECT-TYPE
--   SYNTAX SEQUENCE OF UpsOutputEntry
--   ACCESS not-accessible
--   STATUS obsolete
--   DESCRIPTION
--     "A list of output table entries.  The number of
--     entries is given by the value of upsOutputNumLines."
--   ::= { upsOutput 5 }
--
--
-- upsOutputEntry OBJECT-TYPE
--   SYNTAX UpsOutputEntry
--   ACCESS not-accessible
--   STATUS obsolete
--   DESCRIPTION
--     "An entry containing information applicable to a
--     particular output line."
--   INDEX {
--     upsOutputLineIndex }
--   ::= { upsOutputTable 1 }
--
--
-- UpsOutputEntry ::= SEQUENCE {
--   upsOutputLineIndex   INTEGER,
--   upsOutputVoltage     INTEGER,
--   upsOutputCurrent     INTEGER,
--   upsOutputPower       INTEGER,
--   upsOutputPercentLoad INTEGER }
--
--
-- upsOutputLineIndex OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The output line identifier."
--   ::= { upsOutputEntry 1 }
--
--
-- upsOutputVoltage OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The present output voltage.
--     UNITS     RMS Volts"
--   ::= { upsOutputEntry 2 }
--
--
-- upsOutputCurrent OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The present output mandatory.
--     UNITS     0.1 Amp"
--   ::= { upsOutputEntry 3 }
--
--
-- upsOutputPower OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The present output true power.
--     UNITS     Watts"
--   ::= { upsOutputEntry 4 }
--
--
-- upsOutputPercentLoad OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The percentage of true power capacity presently being used.
--     UNITS     percent"
--   ::= { upsOutputEntry 5 }
--
--
-- Alarm Group
--
-- upsAlarmsPresent OBJECT-TYPE
--   SYNTAX Gauge
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The present number of active alarm conditions."
--   ::= { upsAlarm 1 }
--
--
-- upsAlarmID OBJECT-TYPE
--   SYNTAX INTEGER {
--       upsAlarmBatteryBad(1),
--       upsAlarmOnBattery(2),
--       upsAlarmLowBattery(3),
--       upsAlarmDepletedBattery(4),
--       upsAlarmTempBad(5),
--       upsAlarmOutputOverload(6),
--       upsAlarmOutputOffAsRequested(7),
--       upsAlarmOutputOff(8),
--       upsAlarmDiagnosticTestFailed(9),
--       upsAlarmCommunicationsLost(10),
--       upsAlarmShutdownPending(11),
--       upsAlarmShutdownImminent(12),
--       upsAlarmTestInProgress(13) }
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A unique identifier for an alarm condition.  This
--     value must remain constant."
--   ::= { upsAlarm 2 }
--
--
-- upsAlarmDESCR OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..31))
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A reference to an alarm description object.  The
--     object references should not be accessible, but rather
--     be used to provide a unique description of the alarm
--     condition."
--   ::= { upsAlarm 3 }
--
--
-- upsAlarmTable OBJECT-TYPE
--   SYNTAX SEQUENCE OF UpsAlarmEntry
--   ACCESS not-accessible
--   STATUS obsolete
--   DESCRIPTION
--     "A list of alarm table entries.  The table consists of
--     zero, one, or may rows at any moment, depending upon
--     the number of alarm conditions in effect.  The table
--     is initially empty at agent startup.  The agent
--     creates a row in the table each time a condition is
--     detected and deletes that row when that condition no
--     longer pertains.  The agent creates the first row with
--     upsAlarmId equal to 1, and increments the value fo
--     upsAlarmId each time a new row is created, wrapping to
--     the first free value greater than or equal to 1 when
--     the maximum value of upsAlarmId would otherwise be
--     exceeded.  Consequently, after multiple operations,
--     the table may become sparse, e.g., containing entries
--     for rows 95, 100, 101, and 203 and the entries are in
--     chronological order until upsAlarmId wraps.
--
--     Alarms are named by and OBJECT IDENTIFIER,
--     upsAlarmDescr, to allow a single table to reflect well
--     known alarms plus alarms defined by a particular
--     implementation, i.e., as documented in the private
--     enterprise MIB definition for the device.  No two rows
--     will have the same value of upsAlarmDescr, since
--     alarms define conditions.  In order to meet this
--     requirement, care should be take in the definition of
--     the number of active rows in the table at any given
--     time is reflected by the value fo upsAlarms."
--   ::= { upsAlarm 4 }
--
--
-- upsAlarmEntry OBJECT-TYPE
--   SYNTAX UpsAlarmEntry
--   ACCESS not-accessible
--   STATUS obsolete
--   DESCRIPTION
--     "An entry containing information applicable to a
--     particular alarm."
--   INDEX {
--     upsAlarmId }
--   ::= { upsAlarmTable 1 }
--
--
-- UpsAlarmEntry ::= SEQUENCE {
--   upsAlarmId    INTEGER,
--   upsAlarmDescr DisplayString,
--   upsAlarmTime  TimeTicks }
--
--
-- upsAlarmId OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A unique identifier for an alarm condition.  This
--     value must remain constant."
--   ::= { upsAlarmEntry 1 }
--
--
-- upsAlarmDescr OBJECT-TYPE
--   SYNTAX DisplayString (SIZE (0..31))
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A reference to an alarm description object.  The
--     object references should not be accessible, but rather
--     be used to provide a unique description of the alarm
--     condition."
--   ::= { upsAlarmEntry 2 }
--
--
-- upsAlarmTime OBJECT-TYPE
--   SYNTAX TimeTicks
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The value of sysUpTime when the alarm condition was
--     detected.  If the alarm condition was detected at the
--     time of agent startup and presumable existed before
--     agent startup, the value of upsAlarmTime shall equal
--     0."
--   ::= { upsAlarmEntry 3 }
--
--
-- upsAlarmBatteryBad OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "One or more batteries have been determined to require
--     replacement."
--   ::= { upsWellKnownAlarms 1 }
--
--
-- upsAlarmOnBattery OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The UPS is drawing power from the batteries."
--   ::= { upsWellKnownAlarms 2 }
--
--
-- upsAlarmLowBattery OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The remaining battery run-time is less than or equal
--     to upsConfigMinutesRemaining."
--   ::= { upsWellKnownAlarms 3 }
--
--
-- upsAlarmDepletedBattery OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The UPS will be unable to sustain the present load
--     when and if the utility power is lost."
--   ::= { upsWellKnownAlarms 4 }
--
--
-- upsAlarmTempBad OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A temperature is out of tolerance."
--   ::= { upsWellKnownAlarms 5 }
--
--
-- upsAlarmOutputOverload OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The output load exceeds the UPS output capacity."
--   ::= { upsWellKnownAlarms 6 }
--
--
-- upsAlarmOutputOffAsRequested OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The UPS has shutdown as commanded, i.e., the output is off."
--   ::= { upsWellKnownAlarms 7 }
--
--
-- upsAlarmUpsOutputOff OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The UPS is in the off state."
--   ::= { upsWellKnownAlarms 8 }
--
--
-- upsAlarmDiagnosticTestFailed OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The result of the last diagnostic test indicates a
--     failure."
--   ::= { upsWellKnownAlarms 9 }
--
--
-- upsAlarmCommunicationsLost OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A problem has been encountered in the
--     communications between the agent and the UPS."
--   ::= { upsWellKnownAlarms 10 }
--
--
-- upsAlarmShutdownPending OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A upsShutdownAfterDelay countdown is underway."
--   ::= { upsWellKnownAlarms 11 }
--
--
-- upsAlarmShutdownImminent OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A upsShutdownAfterDelay countdown is underway."
--   ::= { upsWellKnownAlarms 12 }
--
--
-- upsAlarmTestInProgress OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "A upsShutdownAfterDelay countdown is underway."
--   ::= { upsWellKnownAlarms 13 }
--
-- Test Group
--
-- upsTestId OBJECT-TYPE
--   SYNTAX INTEGER {
--       noTestsInitiated(1),
--       abortTestInProgress(2),
--       generalSystemsTest(3),
--       checkBatteryTest(4),
--       deepBatteryCalibration(5) }
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "The test named by an OBJECT IDENTIFIER which
--     allows a standard mechanism for the initiation of
--     test, including the well known tests identified in
--     this document as well as those introduced by a
--     particular implementation, i.e., as
--     documented in the private enterprise MIB definition
--     for the device.
--
--     Setting this variable initiates the named test.  Sets
--     to this variable require the presence of
--     upsTestSpinLock in the same SNMP message.
--
--     The set request will be rejected with an appropriate
--     error message if the requested test cannot be
--     performed, including attempts to start a test when
--     another test is already in progress.  Tests in
--     progress may be aborted by setting this variable to
--     upsTestAbortTestInProgress.
--
--     Read operations return the value of the name of the
--     test in progress if a test is in progress or the name
--     of the last test performed if no test is in progress,
--     unless no test has bee run, in which case the well
--     known value upsTestNoTestsInitiated is returned."
--   ::= { upsTest 1 }
--
--
-- upsTestResultsSummary OBJECT-TYPE
--   SYNTAX INTEGER {
--       donePass(1),
--       doneWarning(2),
--       doneError(3),
--       aborted(4),
--       inProgress(5),
--       noTestsInitiated(6) }
--   ACCESS read-only
--   STATUS obsolete
--   DESCRIPTION
--     "The results of the mandatory or last UPS diagnostics
--     test performed.  The values for donePass(1),
--     doneWarning(2), and doneError(3) are self-documenting.
--     The value aborted(4) is returned for tests which are
--     aborted by setting the value of upsTestId to
--     upsTestAbortTestInProgress.  Tests which have not yet
--     concluded are indicated by inProgress(5).  The value
--     noTestsInitiated(4) indicates that no previous test
--     results are available, such as in the case when no
--     tests have been run since the last reinitialization of
--     the network management subsystem and the system has no
--     provision for non-volatile storage of test results."
--   ::= { upsTest 2 }
--
--
--------------------------------------------------------------------------
-- Note : upsTestResultsDetail MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsTest 3 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsTestStartTime MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsTest 4 } is reserved.
--------------------------------------------------------------------------
-- Control Group
--
-- upsShutdownType OBJECT-TYPE
--   SYNTAX INTEGER {
--       output(1),
--       system(2) }
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "Setting this object will start the output after the
--     indicated number of seconds.  Setting this object to 0
--     will cause the UPS to start the output immediately.
--     If the output is already on at the time the delay has
--     counted down, nothing will happen."
--   ::= { upsControl 1 }
--
--
-- upsShutdownAfterDelay OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "Setting this object will shutdown (i.e., turn off)
--     either the UPS output or the UPS system (as determined
--     by the value of upsShhutdownType at the time of
--     shutdown) after the indicated number of seconds, or
--     less if the UPS batteries become depleted.  Setting
--     this object to 0 will cause the shutdown to occur
--     immediately.  Setting this object to -1 will abort the
--     countdown.  If the system is already in the desired
--     state at the time the countdown reaches 0, then
--     nothing will happen.  That is, there is no additional
--     action at that time if upsShutdownType = system and
--     the system is already off.  Similarly, there is no
--     additional action at that time if upsShutdownType =
--     output and the output is already off.  When read,
--     upsShutdownAfterDelay will return the number of
--     seconds remaining until shutdown, or -1 if no shutdown
--     countdown is in effect.  On some systems, if the agent
--     is restarted while a shutdown countdown is in effect,
--     the countdown may be aborted.  Sets to this object
--     override any upsShutdownAfterDelay already in effect.
--     UNITS seconds"
--   ::= { upsControl 2 }
--
--
-- upsStartupAfterDelay OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "Setting this object will start the output after the
--     indicated number of seconds, includeing starting the
--     UPS, if necessary.  Setting this object to 0 will
--     cause the start to occur immediately.  Setting this
--     object to -1 will abort the countdown.  If the output
--     is already on at the time the countdown reaches 0,
--     nothing will happen.  Sets to this object
--     override the effect of any upsStartupAfterDelay
--     countdown or upsRebootDuration countdown in progress.
--     When read, upsStartupAfterDelay will return the number
--     of seconds until start, or -1 if no startup
--     countdown is in effect.  If the countdown expires
--     during a utility failure, the startup shall depend
--     upon the value of upsAutoRestart at that time.  On
--     some systems, if the agent is restarted while a
--     startup countdown is in effect, the countdown is
--     aborted.
--     UNITS seconds"
--   ::= { upsControl 3 }
--
--
-- upsRebootDuration OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "Setting this object will immediately shutdown (i.e.,
--     turn off) either the UPS output or the UPS system (as
--     determined by the value of the upsShutdownType at the time
--     of shutdown)  for a period equal to the indicated
--     number of seconds, after which time the output will be
--     started, including starting the UPS, if necessary.  If
--     the number of seconds required to perform the request
--     is greater than the requested duration, then the
--     requested shutdown and startup cycle shall be
--     performed in the minimum time possible, but in no case
--     shall this require more than the requested duration
--     plus 60 seconds.  When read, upsRebootDuration shall
--     return the number of seconds remaining in the
--     countdown, or -1 if no countdown is in progress.  If
--     the startup should occur during a utility failure, the
--     startup shall depend on the value of upsAutoRestart
--     at that time.
--     UNITS seconds"
--   ::= { upsControl 4 }
--
--
-- upsAutoRestart OBJECT-TYPE
--   SYNTAX INTEGER {
--       on(1),
--       off(2) }
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "Setting this object to 'on' will cause the UPS system
--     to restart after a shutdown if/when utility power is present."
--   ::= { upsControl 5 }
--
--
-- upsConfig group
--------------------------------------------------------------------------
-- Note : upsConfigInputVoltage MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 1 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsInputFreq MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 2 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigOutputVoltage MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 3 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigOutputFreq MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 4 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigOutputVA MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 5 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigOutputPower MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 6 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigLowBattTime MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 7 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigAudibleStatus MIB variable removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, {upsConfig 8 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigLowVoltageTransferPoint MIB variable removed by Dave Cole (SEC) on
-- 4/24/95.  To conform with older versions of this MIB, {upsConfig 9 } is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsConfigHighVoltageTransferPoint MIB variable removed by Dave Cole (SEC) on
-- 4/24/95.  To conform with older versions of this MIB, {upsConfig 10 } is reserved.
--------------------------------------------------------------------------
-- upsConfigInputVoltageHigh OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "If the value of the input voltage (in Volts) exceeds this value, a
--     utilityVoltageHigh trap will be triggered."
--   ::= { upsConfig 11 }
--
--
-- upsConfigInputVoltageLow OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "If the value of the input voltage (in Volts) falls below this value, a
--     utilityVoltageLow trap will be triggered."
--   ::= { upsConfig 12 }
--
--
-- upsConfigOutputPercLoadHigh OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "If the value of the output percent load exceeds this value, a upsOverload trap
--     will be triggered."
--   ::= { upsConfig 13 }
--
--
-- upsConfigBatteryPercLow OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "If the value of the battery percent capacity falls below this value, a lowBattery
--     trap will be triggered."
--   ::= { upsConfig 14 }
--
--
-- upsConfigBatteryTemperatureHigh OBJECT-TYPE
--   SYNTAX INTEGER
--   ACCESS read-write
--   STATUS obsolete
--   DESCRIPTION
--     "If the value of the battery temperature exceeds this value, a
--     batteryTemperatureHigh trap will be triggered."
--   ::= { upsConfig 15 }
--
--
--
-- Traps
--------------------------------------------------------------------------
-- Note : upsOnBattery trap modified by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, trap 1 is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsTestCompleted trap removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, trap 2 is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsAlarmEntryAdded trap removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, trap 3 is reserved.
--------------------------------------------------------------------------
--------------------------------------------------------------------------
-- Note : upsAlarmEntryDeleted trap removed by Dave Cole (SEC) on 4/24/95
-- To conform with older versions of this MIB, trap 4 is reserved.
--------------------------------------------------------------------------
--
-- upsOnBattery TRAP-TYPE
--   ENTERPRISE tripplite
--   VARIABLES {
--     upsIdentAttachedDevices,
--     upsEstimatedMinutesRemaining}
--   DESCRIPTION
--     "The UPS is on battery."
--  ::= 5
--
--
-- powerRestored TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "Utility power has been restored."
--  ::= 6
--
--
-- lowBattery TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS batteries are low and will soon be exhausted."
--  ::= 7
--
--
-- returnFromLowBattery TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS has returned from a low battery condition."
--  ::= 8
--
--
-- communicationEstablished TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "Communication with the UPS has been established.  This trap will be sent
--     each time there is a transition from a power off condition to a power on condition."
--  ::= 9
--
--
-- communicationLost TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "Communication with the UPS has been lost."
--  ::= 10
--
--
-- upsOverload TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS has sensed a load greater than the value of the
--     upsConfigOutputPercLoadHigh MIB variable."
--  ::= 11
--
--
-- upsDiagnosticsFailed TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS failed its self-test."
--  ::= 12
--
--
-- upsDiagnosticsPassed TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS passed its internal self-test."
--  ::= 13
--
--
-- utilityVoltageHigh TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS input voltage greater than or equal to the value of
--     the upsConfigInputVoltageHigh MIB variable."
--  ::= 14
--
--
-- utilityVoltageLow TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS input voltage is less than or equal to the value of
--     the upsConfigInputVoltageLow MIB variable."
--  ::= 15
--
--
-- utilityVoltageReturnToNormal TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS has returned from a utility voltage high or low condition."
--  ::= 16
--
--
-- batteryTemperatureHigh TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS battery temperature has exceeded the value of the
--     upsConfigBatteryTemperatureHigh MIB variable."
--  ::= 17
--
--
-- shutdownPending TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "A UPS shutdown countdown is underway."
--  ::= 18
--
--
-- upsSleeping TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The output of the UPS has been turned off."
--  ::= 19
--
--
-- upsWokeup TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The output of the UPS has been turned on."
--  ::= 20
--
--
-- upsBatteryNeedsReplacement TRAP-TYPE
--   ENTERPRISE tripplite
--   DESCRIPTION
--     "The UPS battery needs to be replaced."
--  ::= 21
--------------------------------------------------------------------------
-- END Delta SNMP MIB
--------------------------------------------------------------------------


END
