-- =================================================================
-- Copyright (C) 2006 by HUAWEI TECHNOLOGIES. All rights reserved
-- 
-- Description: This MIB defines all the objects that containing PWE3 tunnel information.
-- Reference: rfc4001
-- Version: V1.00
-- History:
--         V1.0 Rengaofeng, 2008-12-11, publish
-- =================================================================


    HUAWEI-PWE3-TNL-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm            
                FROM HUAWEI-MIB            
            HWL2VpnVcEncapsType, HWEnableValue, HWL2VpnStateChangeReason            
                FROM HUAWEI-VPLS-EXT-MIB            
            InterfaceIndexOrZero            
                FROM IF-MIB            
            InetAddressType            
                FROM INET-ADDRESS-MIB            
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            sysUpTime            
                FROM SNMPv2-MIB            
            IpAddress, Integer32, Unsigned32, Counter64, BITS, 
            OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE            
                FROM SNMPv2-SMI            
            DisplayString, TruthValue, RowStatus            
                FROM SNMPv2-TC;
    
    
        hwL2VpnPwe3TnlExt MODULE-IDENTITY 
            LAST-UPDATED "200812151935Z"  --Dec 15, 2008 at 19:35 GMT
            ORGANIZATION 
                "Huawei Technologies Co., Ltd."
            CONTACT-INFO 
                "R&D BeiJing, Huawei Technologies co.,Ltd.
                Huawei Bld.,NO.3 Xinxi Rd., 
                Shang-Di Information Industry Base,
                Hai-Dian District Beijing P.R. China
                Zip:100085 
                Http://www.huawei.com                                       
                E-mail:support@huawei.com"
            DESCRIPTION 
                "Initial version 2008/12/11,L2VPN QOS OBJECT GROUP."
            ::= { hwL2Vpn 5 }
  
--
-- Node definitions
--
        hwL2Vpn OBJECT IDENTIFIER ::= { hwDatacomm 119 }

--          
-- The PWE3Tunnel Attribute Group
-- 
       hwPwe3TunnelMIBObjects OBJECT IDENTIFIER ::= { hwL2VpnPwe3TnlExt 1 }         

-- Textual Conventions.

      
   --  ============== hwPWE3TunnelTable  define beginning ==============  
   
   -- hwPwe3TunnelTable 
   hwPwe3TunnelTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwPwe3TunnelEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a tunnel table."
            ::= { hwPwe3TunnelMIBObjects 1 }
   
   hwPwe3TunnelEntry OBJECT-TYPE
            SYNTAX HwPwe3TunnelEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Provides the information of a VC entry."
            INDEX { hwPwVcId,hwPwVcType,hwPwe3PeerTnlId,hwPwe3PwInlabel}
            ::= { hwPwe3TunnelTable 1 }
   
-- HWPwe3TunnelEntry  
   HwPwe3TunnelEntry ::=              
    SEQUENCE { 
     hwPwVcId
      Unsigned32,
     hwPwVcType
      HWL2VpnVcEncapsType,   
    hwPwe3PwInlabel
      Unsigned32,                 
     hwPwe3PeerTnlId
      Unsigned32,
     hwPwe3TnlName
      OCTET STRING, -- GRE/TE tunnel name
     hwPwe3TnlType
      Integer32, --(or OCTET STRING type)
     hwPwe3TnlSrcAddress
      IpAddress,
     hwPwe3TnlDestAddress
      IpAddress,
     hwPwe3LspIndex 
       Integer32, 
     hwPwe3LspOutIf
      OCTET STRING,
     hwPwe3LspOutLabel
      Integer32,
     hwPwe3LspNextHop
       IpAddress,
     hwPwe3LspFec
      IpAddress, 
     hwPwe3LspFecPfxLen
      Integer32,
     hwPwe3LspIsBackup
      TruthValue,
     hwPwe3PwOutLabel
      Integer32,
     hwPwe3IsBalance
      TruthValue,
     hwPwe3TnlRowStatus
      RowStatus   
    }    


    hwPwVcId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Index for the conceptual row identifying a PW within  
                this PW Emulation table.Used in the outgoing PW ID field within the 'Virtual 
                Circuit FEC Element'."
            ::= { hwPwe3TunnelEntry 1 }


    hwPwVcType OBJECT-TYPE
            SYNTAX HWL2VpnVcEncapsType
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The type of the Virtual Circuit.This value indicate the service carried over 
                this PW."
            ::= { hwPwe3TunnelEntry 2 }


    hwPwe3PwInlabel OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The inlabel of SVC PW."
            ::= { hwPwe3TunnelEntry 3 }
                                    

    hwPwe3PeerTnlId OBJECT-TYPE
           SYNTAX Unsigned32
           MAX-ACCESS not-accessible
           STATUS current
           DESCRIPTION
            "The Tunnel ID."
           ::= { hwPwe3TunnelEntry 4 }  


    hwPwe3TnlName OBJECT-TYPE
         SYNTAX OCTET STRING
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
          "The name of this Tunnel."
           ::= { hwPwe3TunnelEntry 5 }
              

    hwPwe3TnlType OBJECT-TYPE
         SYNTAX Integer32 (0..255)
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
          "The type of this Tunnel. e.g. LSP/GRE/CR-LSP..."
           ::= { hwPwe3TunnelEntry 6}
          

    hwPwe3TnlSrcAddress OBJECT-TYPE
           SYNTAX IpAddress 
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The source ip address of this tunnel."   
           ::= { hwPwe3TunnelEntry 7 }


    hwPwe3TnlDestAddress OBJECT-TYPE
           SYNTAX IpAddress 
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The destination ip address of this tunnel."   
           ::= { hwPwe3TunnelEntry 8 } 
       

    hwPwe3LspIndex OBJECT-TYPE
           SYNTAX Integer32
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The index of lsp."
           ::= { hwPwe3TunnelEntry 9 } 
           
                   
    hwPwe3LspOutIf OBJECT-TYPE
           SYNTAX OCTET STRING
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The out-interface of lsp."
           ::= { hwPwe3TunnelEntry 10 }
           
    
    hwPwe3LspOutLabel OBJECT-TYPE
           SYNTAX Integer32 (0..2147483647)
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The out-label of lsp."
           ::= { hwPwe3TunnelEntry 11 }
           

    hwPwe3LspNextHop OBJECT-TYPE
           SYNTAX IpAddress
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The next-hop of lsp."
           ::= { hwPwe3TunnelEntry 12 }                       
           
         
    hwPwe3LspFec OBJECT-TYPE
           SYNTAX IpAddress 
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The FEC of lsp."   
           ::= { hwPwe3TunnelEntry 13 } 
           

    hwPwe3LspFecPfxLen OBJECT-TYPE
           SYNTAX Integer32
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The length of mask for hwVplsLspFec."   
           ::= { hwPwe3TunnelEntry 14 } 


    hwPwe3LspIsBackup OBJECT-TYPE
           SYNTAX TruthValue
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "Indicate whether the lsp is main."   
           ::= { hwPwe3TunnelEntry 15 } 


    hwPwe3PwOutLabel OBJECT-TYPE
           SYNTAX Integer32
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "the outlabel of pw£¬specified for SVC."   
           ::= { hwPwe3TunnelEntry 16 }


    hwPwe3IsBalance OBJECT-TYPE
           SYNTAX TruthValue
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "Property of Balance. Rerurn True if Tunnel-Policy is configed."   
           ::= { hwPwe3TunnelEntry 17 } 


    hwPwe3TnlRowStatus OBJECT-TYPE
           SYNTAX RowStatus
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
            "The operating state of the row."
           ::= { hwPwe3TunnelEntry 50}
              
   --  ============== hwTnlInfoTable  define end ==============    

--           
--  MIB Trap Definitions
-- 
        hwPwe3TunnelMIBTraps OBJECT IDENTIFIER ::= { hwL2VpnPwe3TnlExt 2 }
           
--    Conformance information
-- 
        hwPwe3TunnelMIBConformance OBJECT IDENTIFIER ::= { hwL2VpnPwe3TnlExt 3 }

        
        hwPwe3TunnelMIBCompliances OBJECT IDENTIFIER ::= { hwPwe3TunnelMIBConformance 1 }

        
--  MIB Compliance Definitions
        hwPwe3TunnelMIBCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "The compliance statement for systems supporting 
                the HUAWEI-PWE3-TNL-MIB."
            MODULE -- this module
                MANDATORY-GROUPS { hwPwe3TunnelGroup }
            ::= { hwPwe3TunnelMIBCompliances 1 }

--  MIB Group Definitions        
        hwPwe3TunnelMIBGroups OBJECT IDENTIFIER ::= { hwPwe3TunnelMIBConformance 2 }

        
        hwPwe3TunnelGroup OBJECT-GROUP
            OBJECTS { hwPwe3TnlName, hwPwe3TnlType, hwPwe3TnlSrcAddress, hwPwe3TnlDestAddress, hwPwe3LspIndex, hwPwe3LspOutIf,
            hwPwe3LspOutLabel, hwPwe3LspNextHop, hwPwe3LspFec, hwPwe3LspFecPfxLen, hwPwe3LspIsBackup, hwPwe3PwOutLabel, hwPwe3IsBalance, hwPwe3TnlRowStatus }
            STATUS current
            DESCRIPTION 
                "The PWE3 tunnel group."
            ::= { hwPwe3TunnelMIBGroups 1 }

   
    END 
