
-- *****************************************************************************
-- Juniper-ADDRESS-POOL-MIB
--
-- Juniper Networks Enterprise MIB
--   Address Pool MIB
--
-- Copyright (c) 1999 Redstone Communications, Inc.
-- Copyright (c) 2001, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002, 2003, 2004 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-ADDRESS-POOL-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, IpAddress, NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    RowStatus, TruthValue, DisplayString
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    juniRouterName
        FROM Juniper-ROUTER-MIB
    juniMibs
        FROM Juniper-MIBs;

juniAddressPoolMIB  MODULE-IDENTITY
    LAST-UPDATED "200502112135Z"  -- 11-Feb-05 04:35 PM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Road
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        E-mail: mib@Juniper.net"
    DESCRIPTION
        "The Address Pool MIB for the Juniper Networks enterprise."
    -- Revision History
    REVISION    "200502112135Z"  -- 11-Feb-05 04:35 PM EST  - JUNOSe 7.0
    DESCRIPTION
        "Added support for  juniAddressSharedPoolTable."
    REVISION    "200409172237Z"  -- 17-Sep-04 05:37 PM EST  - JUNOSe 6.0
    DESCRIPTION
        "Added support for next pool profile index.
        Changed the description of the juniAddressPoolRowStatus and 
        the juniAddressAliasRowStatus objects."
    REVISION    "200311032237Z"  -- 03-Nov-03 05:37 PM EST  - JUNOSe 5.3
    DESCRIPTION
        "Added support for address pool aliases."
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200205061838Z"  -- 06-May-02 02:38 PM EDT  - JUNOSe 3.3
    DESCRIPTION
        "Added juniAddressPoolProfileTable to support an address pool with
        multiple address ranges."
    REVISION    "200105021157Z"  -- 02-May-01 07:57 AM EDT  - JUNOSe 3.2
    DESCRIPTION
        "Added pool exhaustion variables and notifications for high pool
        utilization and pool exhaustion."
    REVISION    "200104271500Z"  -- 27-Apr-01 11:00 AM EDT  - JUNOSe 3.0
    DESCRIPTION
        "Fixed range on juniAddressPoolNextPoolIndex."
    REVISION      "9906010000Z"  -- 01-Jun-99               - JUNOSe 1.3
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 21 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed object groups
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniAddressPoolObjects  OBJECT IDENTIFIER ::= { juniAddressPoolMIB 1 }
juniAddressPool         OBJECT IDENTIFIER ::= { juniAddressPoolObjects 1 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects for Address Pools
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniAddressPoolTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniAddressPoolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of IP address pool configuration entries."
    ::= { juniAddressPool 1 }

juniAddressPoolEntry OBJECT-TYPE
    SYNTAX      JuniAddressPoolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry describing an IP address pool configuration."
    INDEX     { juniAddressPoolIndex }
    ::= { juniAddressPoolTable 1 }

JuniAddressPoolEntry ::= SEQUENCE {
    juniAddressPoolIndex                 Integer32,
    juniAddressPoolName                  OCTET STRING,
    juniAddressPoolRowStatus             RowStatus,
    juniAddressPoolStart                 IpAddress,
    juniAddressPoolEnd                   IpAddress,
    juniAddressPoolSize                  Integer32,
    juniAddressPoolInUse                 Integer32,
    juniAddressPoolHighUtilThreshold     Integer32,
    juniAddressPoolAbatedUtilThreshold   Integer32,
    juniAddressPoolUtilPct               Integer32,
    juniAddressPoolTrapEnable            TruthValue,
    juniAddressPoolNextPoolProfileIndex  Integer32 }

juniAddressPoolIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An arbitrary integer index that distinguishes this address pool."
    ::= { juniAddressPoolEntry 1 }

juniAddressPoolRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of address pools.
        
        Only value 'active' will be observed with GET.
        Only values 'createAndGo' and 'destroy' are supported for SET.

        To create an entry in this table, the following entry object MUST be
        explicitly configured:
            juniAddressPoolName

        Once created, the objects with current status can be modified with the
        exception of the juniAddressPoolName object.

        Deleting a row in this table will result in the removal of all rows in 
        the juniAddressPoolProfileTable with the same pool index."
    ::= { juniAddressPoolEntry 2 }

juniAddressPoolName OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1..16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of this address pool.  Represents textual information taken
        from the NVT ASCII graphics character set (codes 32 through 126)."
    REFERENCE
        "RFC 854: NVT ASCII character set."
    ::= { juniAddressPoolEntry 3 }

juniAddressPoolStart OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "The starting IP address for the range of addresses comprising the
        'first' pool profile entry.  This object is deprecated in favor of
        juniAddressPoolProfileStart because it applies to a single address range
        and can only show one of possibly many address ranges found in the newer
        juniAddressPoolProfileTable.  The value in this table maps to the value
        in the juniAddressPoolProfileTable for the entry with
        juniAddressPoolProfileIndex equal to 1."
    DEFVAL    { 0 }
    ::= { juniAddressPoolEntry 4 }

juniAddressPoolEnd OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "The ending IP address for the range of addresses comprising the 'first'
        pool profile entry.  This object is deprecated in favor of
        juniAddressPoolProfileEnd because it applies to a single address range
        and can only show one of possibly many address ranges found in the newer
        juniAddressPoolProfileTable.  The value in this table maps to the value
        in the juniAddressPoolProfileTable for the entry with
        juniAddressPoolProfileIndex equal to 1."
    DEFVAL    { 0 }
    ::= { juniAddressPoolEntry 5 }

juniAddressPoolSize OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "The number of addresses available in the 'first' pool profile entry.
        This object is deprecated in favor of juniAddressPoolProfileSize because
        it applies to a single address range and can only show one of possibly
        many address ranges found in the newer juniAddressPoolProfileTable.  The
        value in this table maps to the value in the juniAddressPoolProfileTable
        for the entry with juniAddressPoolProfileIndex equal to 1."
    ::= { juniAddressPoolEntry 6 }

juniAddressPoolInUse OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "The number of addresses currently allocated from the 'first' pool
        profile entry.  This object is deprecated in favor of
        juniAddressPoolProfileInUse because it applies to a single address range
        and can only show one of possibly many address ranges found in the newer
        juniAddressPoolProfileTable.  The value in this table maps to the value
        in the juniAddressPoolProfileTable for the entry with
        juniAddressPoolProfileIndex equal to 1."
    ::= { juniAddressPoolEntry 7 }

juniAddressPoolHighUtilThreshold  OBJECT-TYPE
    SYNTAX      Integer32 (1..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of address pool utilization, where if reached for the first
        time, will generate a high address pool utilization event to the
        management entity on this system.
 
        The value of this object must be greater than the value of
        juniAddressPoolAbatedUtilThreshold."
    DEFVAL    { 85 }
    ::= { juniAddressPoolEntry 8 }

juniAddressPoolAbatedUtilThreshold OBJECT-TYPE 
    SYNTAX      Integer32 (1..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of address pool utilization that is used to determine when to
        generate an abated address pool utilization event notification to the
        management entity on this system.

        The value of this object must be less than the value of the
        juniAddressPoolHighUtilThreshold.

        The abated address pool utilization event is sent once if the high
        address pool utilization threshold is reached and utilization falls to
        the value of this object."
    DEFVAL    { 75 }
    ::= { juniAddressPoolEntry 9 }

juniAddressPoolUtilPct OBJECT-TYPE
    SYNTAX      Integer32 (1..100)
    MAX-ACCESS  read-only
    STATUS      current 
    DESCRIPTION
        "The current address utilization for this pool."
    ::= { juniAddressPoolEntry 10 }
    
juniAddressPoolTrapEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The configuration setting for address pool notifications.  Setting this
        object to enable(1) will enable the sending of juniAddressPool event
        notifications to the management entity on this device.  Setting this
        object to false(2) will disable event notification reports."
    DEFVAL    { false }
    ::= { juniAddressPoolEntry 11 }
 
juniAddressPoolNextPoolProfileIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate juniAddressPoolProfileIndex value allocation for entries in
        juniAddressPoolProfileTable.

        A GET of this object returns the next available 
        juniAddressPoolProfileIndex value to be used to create an entry in the 
        associated juniAddressPoolProfileTable; or zero, if no valid 
        juniAddressPoolProfileIndex is available.  This object returns a value
        of zero when it is the lexicographic successor of a varbind presented 
        in an SNMP GETNEXT or GETBULK request, for which circumstance it is 
        assumed that a new index allocation is unintended."
    ::= { juniAddressPoolEntry 12 }

--
-- Address pool profile table.
--
juniAddressPoolProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniAddressPoolProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of IP address pool profile entries."
    ::= { juniAddressPool 3 }

juniAddressPoolProfileEntry OBJECT-TYPE
    SYNTAX      JuniAddressPoolProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An IP address pool profile entry.

        Deleting an entry in the juniAddressPoolProfileTable will result in the
        removal of all entries in this table that have the same pool index
        value."
    INDEX     { juniAddressPoolIndex,
                juniAddressPoolProfileIndex }
    ::= { juniAddressPoolProfileTable 1 }

JuniAddressPoolProfileEntry ::= SEQUENCE { 
    juniAddressPoolProfileIndex      Integer32,
    juniAddressPoolProfileRowStatus  RowStatus,
    juniAddressPoolProfileStart      IpAddress,
    juniAddressPoolProfileEnd        IpAddress,
    juniAddressPoolProfileSize       Integer32,
    juniAddressPoolProfileInUse      Integer32 }

juniAddressPoolProfileIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A monotonically increasing integer for the sole purpose of indexing
        entries within the named address pool."
    ::= { juniAddressPoolProfileEntry 1 }

juniAddressPoolProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of address pools.
        
        Only value 'active' will be observed with GET.
        Only values 'createAndGo' and 'destroy' are supported for SET.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniAddressPoolProfileStart
            juniAddressPoolProfileEnd

        Once created, entry content cannot be modified except by deleting and
        recreating an entry with the same index."
    ::= { juniAddressPoolProfileEntry 2 }

juniAddressPoolProfileStart OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The starting IP address for the range of addresses comprising this
        pool."
    ::= { juniAddressPoolProfileEntry 3 }

juniAddressPoolProfileEnd OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ending IP address for the range of addresses comprising this pool."
    ::= { juniAddressPoolProfileEntry 4 }

juniAddressPoolProfileSize OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of addresses available in this pool."
    ::= { juniAddressPoolProfileEntry 5 }

juniAddressPoolProfileInUse OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of addresses currently allocated from this pool."
    ::= { juniAddressPoolProfileEntry 6 }


--
-- Address alias table.
--
juniAddressAliasTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniAddressAliasEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of IP address alias entries.

        An alias is an alternate name for an existing local address pool within
        a virtual router.  It is comprised of an alias name and a pool name.
        Multiple aliases may be configured for each virtual router.  They will
        be stored in an alias table that will be managed by the virtual router's
        local address server.  A maximum number of 32 aliases may be configured
        per virtual router.

        When an AAA Server requests an IP address from a specific local address
        pool within a virtual router, the local address server will first search
        its alias table for a matching alias name.  If an alias exists, the IP
        address would be allocated from the pool specified by the alias.  If no
        alias exists, the IP address would be allocated from the pool specified
        in the request.  If a pool is not specified in the request, the local
        address server would disregard its alias table and allocate the first
        available IP address from its pools."
    ::= { juniAddressPool 4 }

juniAddressAliasEntry OBJECT-TYPE
    SYNTAX      JuniAddressAliasEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An IP address alias entry."
    INDEX     { IMPLIED juniAddressAliasName }
    ::= { juniAddressAliasTable 1 }

JuniAddressAliasEntry ::= SEQUENCE { 
    juniAddressAliasName       DisplayString,
    juniAddressAliasRowStatus  RowStatus,
    juniAddressAliasPoolName   DisplayString }

juniAddressAliasName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of this alias.  It should match a local address pool name that
        would appear in an IP address request from an AAA Server.

        Represents textual information taken from the NVT ASCII graphics
        character set (codes 32 through 126)."
    REFERENCE
        "RFC 854: NVT ASCII character set."
    ::= { juniAddressAliasEntry 1 }

juniAddressAliasRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of address aliases.
        
        Only value 'active' will be observed with GET, GETNEXT, and GETBULK.
        Only values 'createAndGo' and 'destroy' are supported for SET."
    ::= { juniAddressAliasEntry 2 }

juniAddressAliasPoolName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the address pool for this alias; corresponds to a
        juniAddressPoolName value in an existing juniAddressPoolTable entry.

        Represents textual information taken from the NVT ASCII graphics
        character set (codes 32 through 126)."
    REFERENCE
        "RFC 854: NVT ASCII character set."
    ::= { juniAddressAliasEntry 3 } 

--
-- Shared address pool table.
--

juniAddressSharedPoolTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniAddressSharedPoolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of shared address pool configuration entries.  These pools
         rely on DHCP for address allocations."
    ::= { juniAddressPool 5 }

juniAddressSharedPoolEntry OBJECT-TYPE
    SYNTAX      JuniAddressSharedPoolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry describing a shared address pool configuration."
    INDEX     { juniAddressSharedPoolIndex }
    ::= { juniAddressSharedPoolTable 1 }

JuniAddressSharedPoolEntry ::= SEQUENCE {
    juniAddressSharedPoolIndex            Integer32,
    juniAddressSharedPoolRowStatus        RowStatus,
    juniAddressSharedPoolName             OCTET STRING,
    juniAddressSharedPoolDhcpPoolName     OCTET STRING,
    juniAddressSharedPoolInUse            Integer32 }


juniAddressSharedPoolIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An arbitrary integer index that distinguishes this address pool."
    ::= { juniAddressSharedPoolEntry 1 }

juniAddressSharedPoolRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of address pools.
        
        Only value 'active' will be observed with GET.
        Only values 'createAndGo' and 'destroy' are supported for SET.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniAddressSharedPoolName, juniAddressSharedPoolDhcpPoolName.

        Once created, the objects in this table can not be modified."
    ::= { juniAddressSharedPoolEntry 2 }

juniAddressSharedPoolName OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1..16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of this address pool.  Represents textual information taken
        from the NVT ASCII graphics character set (codes 32 through 126). 
        Values for this object are mutually exclusive with juniAddressPoolName."
    REFERENCE
        "RFC 854: NVT ASCII character set."
    ::= { juniAddressSharedPoolEntry 3 }


juniAddressSharedPoolDhcpPoolName OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1..64))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the DHCP pool that allocates addresses for this
        pool.  Represents textual information taken
        from the NVT ASCII graphics character set (codes 32 through 126)."
    REFERENCE
        "RFC 854: NVT ASCII character set."
    ::= { juniAddressSharedPoolEntry 4 }

juniAddressSharedPoolInUse OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current number of address allocations for this entry."
      ::= { juniAddressSharedPoolEntry 5 }


--
-- juniAddressPoolIndex selection for creating new address pools 
--
juniAddressPoolNextPoolIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate values of juniAddressPoolIndex and juniAddressSharedPoolIndex
        for entries in juniAddressPoolTable and juniAddressSharedPoolTable.

        A GET of this object returns the next available index
        value to be used to create an entry in the associated
        juniAddressPoolTable or juniAddressSharedPoolTable or zero,
        if no valid index is available.

        This object returns a value of zero when it is the
        lexicographic successor of a varbind presented in an SNMP GETNEXT or
        GETBULK request, for which circumstance it is assumed that a new index
        allocation is unintended."
    ::= { juniAddressPool 2 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notification control objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholder follows.
-- juniAddressPoolTrapControl  OBJECT IDENTIFIER ::= { juniAddressPoolMIB 2 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The following two OBJECT IDENTIFIERS are used to define SNMPv2 
-- Notifications that are easily translated into SNMPv1 Traps.

juniAddressPoolTraps            OBJECT IDENTIFIER ::= { juniAddressPoolMIB 3 }
juniAddressPoolTrapPrefix       OBJECT IDENTIFIER ::= { juniAddressPoolTraps 0 }

juniAddressPoolHighAddrUtil NOTIFICATION-TYPE
    OBJECTS {
        juniRouterName,
        juniAddressPoolName,
        juniAddressPoolSize,
        juniAddressPoolInUse,
        juniAddressPoolUtilPct }
    STATUS      current
    DESCRIPTION
        "Reports address pool utilization has reached the configured high
        utilization threshold."
    ::= { juniAddressPoolTrapPrefix 1 }

juniAddressPoolAbatedAddrUtil NOTIFICATION-TYPE
    OBJECTS {
        juniRouterName,
        juniAddressPoolName,
        juniAddressPoolSize,
        juniAddressPoolInUse,
        juniAddressPoolUtilPct }
    STATUS      current
    DESCRIPTION
        "Reports address pool utilization has fallen to the configured abated
        threshold level."
    ::= { juniAddressPoolTrapPrefix 2 }

juniAddressPoolNoAddresses NOTIFICATION-TYPE
    OBJECTS {
        juniRouterName,
        juniAddressPoolName,
        juniAddressPoolSize }
    STATUS      current
    DESCRIPTION
        "Reports address pool has exhausted its supply of addresses.  This trap
        is issued every time a request is made to allocate an address from a
        fully utilized pool."
    ::= { juniAddressPoolTrapPrefix 3 }


-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniAddressPoolMIBConformance
             OBJECT IDENTIFIER ::= { juniAddressPoolMIB 4 }
juniAddressPoolMIBCompliances
             OBJECT IDENTIFIER ::= { juniAddressPoolMIBConformance 1 }
juniAddressPoolMIBGroups
             OBJECT IDENTIFIER ::= { juniAddressPoolMIBConformance 2 }

--
-- compliance statements
--
juniAddressPoolCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems providing local address
        pools.  This statement became obsolete when pool exhaustion variables
        and notifications were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniAddressPoolGroup }
    ::= { juniAddressPoolMIBCompliances 1 }                        -- JUNOSe 1.3

juniAddressPoolCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems providing local address
        pools.  This statement became obsolete when support was added for
        address pools with multiple address ranges."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniAddressPoolGroup2,
            juniAddressPoolTrapGroup }
    ::= { juniAddressPoolMIBCompliances 2 }                        -- JUNOSe 3.2

juniAddressPoolCompliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems providing local address
        pools.  This statement became obsolete when support was added for
        address aliases."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniAddressPoolGroup3,
            juniAddressPoolTrapGroup }
    ::= { juniAddressPoolMIBCompliances 3 }                        -- JUNOSe 3.3

juniAddressPoolCompliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems providing local address
        pools.  This statement became obsolete when support was added for
        next PoolProfile index."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniAddressPoolGroup3,
            juniAddressPoolTrapGroup,
            juniAddressAliasGroup }
    ::= { juniAddressPoolMIBCompliances 4 }                        -- JUNOSe 5.3  
    
juniAddressPoolCompliance5  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems providing local address
        pools.  This statement became obsolete when support was added for
        shared address pools."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniAddressPoolGroup4,
            juniAddressPoolTrapGroup,
            juniAddressAliasGroup }
    ::= { juniAddressPoolMIBCompliances 5 }                        -- JUNOSe 6.0

juniAddressPoolCompliance6  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for systems providing local address pools."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniAddressPoolGroup5,
            juniAddressPoolTrapGroup,
            juniAddressAliasGroup }
    ::= { juniAddressPoolMIBCompliances 6 }                        -- JUNOSe 7.0

--
-- units of conformance
--
juniAddressPoolGroup  OBJECT-GROUP
    OBJECTS {
        juniAddressPoolRowStatus,
        juniAddressPoolName,
        juniAddressPoolStart,
        juniAddressPoolEnd,
        juniAddressPoolSize,
        juniAddressPoolInUse,
        juniAddressPoolNextPoolIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of local address
        pools.  This group became obsolete when pool exhaustion variables and
        notifications were added."
    ::= { juniAddressPoolMIBGroups 1 }                             -- JUNOSe 1.3

juniAddressPoolGroup2  OBJECT-GROUP
    OBJECTS {
        juniAddressPoolRowStatus,
        juniAddressPoolName,
        juniAddressPoolStart,
        juniAddressPoolEnd,
        juniAddressPoolSize,
        juniAddressPoolInUse,
        juniAddressPoolNextPoolIndex,
        juniAddressPoolHighUtilThreshold,
        juniAddressPoolAbatedUtilThreshold,
        juniAddressPoolUtilPct,
        juniAddressPoolTrapEnable }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of local address
        pools.  This group became obsolete when support was added for address
        pools with multiple address ranges."
    ::= { juniAddressPoolMIBGroups 2 }                             -- JUNOSe 3.2

juniAddressPoolTrapGroup  NOTIFICATION-GROUP
    NOTIFICATIONS {
        juniAddressPoolHighAddrUtil,
        juniAddressPoolAbatedAddrUtil,
        juniAddressPoolNoAddresses }
    STATUS      current
    DESCRIPTION
        "The notifications providing alarms for high pool utilization and pool
        exhaustion of local address pools."
    ::= { juniAddressPoolMIBGroups 3 }                             -- JUNOSe 3.2

juniAddressPoolGroup3  OBJECT-GROUP
    OBJECTS {
        juniAddressPoolRowStatus,
        juniAddressPoolName,
        juniAddressPoolNextPoolIndex,
        juniAddressPoolHighUtilThreshold,
        juniAddressPoolAbatedUtilThreshold,
        juniAddressPoolUtilPct,
        juniAddressPoolTrapEnable,
        juniAddressPoolProfileRowStatus,
        juniAddressPoolProfileStart,
        juniAddressPoolProfileEnd,
        juniAddressPoolProfileSize,
        juniAddressPoolProfileInUse }
    STATUS      current
    DESCRIPTION
        "The basic collection of objects providing management of local address
        pools."
    ::= { juniAddressPoolMIBGroups 4 }                             -- JUNOSe 3.3

juniAddressPoolDeprecatedGroup  OBJECT-GROUP
    OBJECTS {
        juniAddressPoolStart,
        juniAddressPoolEnd,
        juniAddressPoolSize,
        juniAddressPoolInUse }
    STATUS      deprecated
    DESCRIPTION
        "A collection of deprecated objects providing management of local
        address pools.  This group became deprecated when support was added for
        address pools with multiple address ranges."
    ::= { juniAddressPoolMIBGroups 5 }                             -- JUNOSe 3.3

juniAddressAliasGroup OBJECT-GROUP
    OBJECTS {
        juniAddressAliasRowStatus,
        juniAddressAliasPoolName }
    STATUS      current
    DESCRIPTION
        "The basic collection of objects providing management of local address
        aliases."
    ::= { juniAddressPoolMIBGroups 6 }                             -- JUNOSe 5.3

juniAddressPoolGroup4  OBJECT-GROUP
    OBJECTS {
        juniAddressPoolRowStatus,
        juniAddressPoolName,
        juniAddressPoolNextPoolIndex,
        juniAddressPoolHighUtilThreshold,
        juniAddressPoolAbatedUtilThreshold,
        juniAddressPoolUtilPct,
        juniAddressPoolTrapEnable,
        juniAddressPoolProfileRowStatus,
        juniAddressPoolProfileStart,
        juniAddressPoolProfileEnd,
        juniAddressPoolProfileSize,
        juniAddressPoolProfileInUse,
        juniAddressPoolNextPoolProfileIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of local address
        pools."
    ::= { juniAddressPoolMIBGroups 7 }                             -- JUNOSe 6.0

juniAddressPoolGroup5  OBJECT-GROUP
    OBJECTS {
        juniAddressPoolRowStatus,
        juniAddressPoolName,
        juniAddressPoolNextPoolIndex,
        juniAddressPoolHighUtilThreshold,
        juniAddressPoolAbatedUtilThreshold,
        juniAddressPoolUtilPct,
        juniAddressPoolTrapEnable,
        juniAddressPoolProfileRowStatus,
        juniAddressPoolProfileStart,
        juniAddressPoolProfileEnd,
        juniAddressPoolProfileSize,
        juniAddressPoolProfileInUse,
        juniAddressPoolNextPoolProfileIndex,
        juniAddressSharedPoolRowStatus,
        juniAddressSharedPoolName,
        juniAddressSharedPoolDhcpPoolName,
        juniAddressSharedPoolInUse }
    STATUS      current
    DESCRIPTION
        "The basic collection of objects providing management of local address
        pools."
    ::= { juniAddressPoolMIBGroups 8 }                             -- JUNOSe 7.0

END
