ZYXEL-ZYWALL-ZLD-COMMON-MIB DEFINITIONS ::= BEGIN
	IMPORTS
		enterprises
			FROM RFC1155-SMI
		OBJECT-TYPE
			FROM RFC-1212
		TRAP-TYPE
			FROM RFC-1215
		zywallZLDCommon
			FROM ZYXEL-MIB;

	-- ZyWALL ZLD Key Groups
	zldSystem		OBJECT IDENTIFIER ::= { zywallZLDCommon 1 }
	zldIpSecVPN		OBJECT IDENTIFIER ::= { zywallZLDCommon 2 }

	-- ZyWALL ZLD System
	sysCPUUsage OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
			"Device CPU load."
		::= { zldSystem 1 }

	sysRAMUsage OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
			"Device RAM Usage."
		::= { zldSystem 2 }

	sysCPU5SecUsage OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
			"Average of past 5 secs cpu load."
		::= { zldSystem 3 }
		
	sysCPU1MinUsage OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
			"Average of past 1 min cpu load."
		::= { zldSystem 4 }
		
	sysCPU5MinUsage OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
			"Average of past 5 min cpu load."
		::= { zldSystem 5 }
		
	sysSessionNum OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS  mandatory
		DESCRIPTION
			"Device Session Num."
		::= { zldSystem 6 }
		
	-- ZyWALL ZLD IpSec VPN

	vpnIpSecTotalThroughput	OBJECT-TYPE
		SYNTAX	INTEGER
		MAX-ACCESS	read-only
		STATUS	mandatory
		DESCRIPTION
			"The VPN total throughput(B/s)."
		::= { zldIpSecVPN 1 }

END
