-- *****************************************************************
-- OLD-CISCO-CPU-MIB.my:  Old Cisco Cpu MIB file
--
-- May 1994, Jeffrey T. Johnson
--
-- Copyright (c) 1994 by cisco Systems, Inc.
-- All rights reserved.
-- 
-- *****************************************************************
--

               OLD-CISCO-CPU-MIB DEFINITIONS ::= BEGIN

               IMPORTS
			OBJECT-TYPE
				FROM RFC-1212
			local
				FROM CISCO-SMI;
          
-- lcpu is the same as lsystem
-- name changed to support separate compilation with mibcomp

               lcpu             OBJECT IDENTIFIER ::= { local 1 }

               busyPer OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "CPU busy percentage in the last 5 second
                           period. Not the last 5 realtime seconds but
                           the last 5 second period in the scheduler."
                   ::= { lcpu 56 }

               avgBusy1 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "1 minute exponentially-decayed moving
                           average of the CPU busy percentage."
                   ::= { lcpu 57 }

               avgBusy5 OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  mandatory
                   DESCRIPTION
                           "5 minute exponentially-decayed moving
                           average of the CPU busy percentage."
                   ::= { lcpu 58 }

               idleCount OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "cisco internal variable. not to be used"
                   ::= { lcpu 59 }

               idleWired OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  mandatory
                   DESCRIPTION
                           "cisco internal variable. not to be used"
                   ::= { lcpu 60 }

END

