
-- *****************************************************************************
-- Juniper-DNS-MIB
--
-- Juniper Networks Enterprise MIB
--   DNS MIB
--
-- Copyright (c) 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002, 2003 Juniper Networks, Inc.
-- Copyright (c) 2006, Juniper Networks Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-DNS-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, IpAddress, Integer32
        FROM SNMPv2-SMI
    RowStatus, TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    JuniEnable
        FROM Juniper-TC
    InetAddress, InetAddressType
        FROM INET-ADDRESS-MIB
    juniMibs
        FROM Juniper-MIBs;

juniDnsMIB  MODULE-IDENTITY
    LAST-UPDATED "200609150832Z"  -- 15-Sep-06 03:32 AM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The DNS MIB for the Juniper Networks, Inc. enterprise."
    -- Revision History
    REVISION    "200609150832Z"  -- 15-Sep-06 03:32 AM EST  - JUNOSe 6.1
    DESCRIPTION
        "Changed the maximum size of octet string for the object 
        juniDnsLocalDomainNameListName from 32 to 1025." 
    REVISION    "200309111550Z"  -- 11-Sep-03 11:50 AM EDT  - JUNOSe 5.2
    DESCRIPTION
        "Added IPv6 address support."
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200103221929Z"  -- 22-Mar-01 02:29 PM EST  - JUNOSe 3.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 47 }


-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- Type definitions
--
JuniNextServerListIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Coordinate index value allocation for entries in an associated table,
        by first reading an index value from this object, then creating an
        entry, having that index value, in the associated table.

        The DESCRIPTION clause for an object of this type must identify the
        associated table.

        A GET of this object returns the next available index value to be used
        to create an entry in the associated table; or zero, if no valid index
        value is available.  This object also returns a value of zero when it is
        the lexicographic successor of a varbind presented in an SNMP GETNEXT or
        GETBULK request, for which circumstance it is assumed that index
        allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously.

        Unless specified otherwise by its MAX-ACCESS and DESCRIPTION clauses, an
        object of this type is read-only, and a SET of such an object returns a
        notWritable error."
    SYNTAX      Integer32 (0..2147483647)

ServerListIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS       current
    DESCRIPTION
        "A unique value, greater than zero, for each DNS server in the managed
        system."
    SYNTAX       Integer32 (1..2147483647)

JuniNextLocalDomainNameListIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Coordinate index value allocation for entries in an associated table,
        by first reading an index value from this object, then creating an
        entry, having that index value, in the associated table.

        The DESCRIPTION clause for an object of this type must identify the
        associated table.

        A GET of this object returns the next available index value to be used
        to create an entry in the associated table; or zero, if no valid index
        value is available.  This object also returns a value of zero when it is
        the lexicographic successor of a varbind presented in an SNMP GETNEXT or
        GETBULK request, for which circumstance it is assumed that index
        allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously.

        Unless specified otherwise by its MAX-ACCESS and DESCRIPTION clauses, an
        object of this type is read-only, and a SET of such an object returns a
        notWritable error."
    SYNTAX      Integer32 (0..2147483647)

LocalDomainNameListIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS       current
    DESCRIPTION
        "A unique value, greater than zero, for each recognized domain name in
        the managed system."
    SYNTAX       Integer32 (1..2147483647)

LocalDomainName ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "1025a"
    STATUS       current
    DESCRIPTION
        "Local domain name.  Represents textual information taken from the NVT
        ASCII character set."
    REFERENCE
        "RFC 854: NVT ASCII character set.  See SNMPv2-TC.DisplayString
        DESCRIPTION for a summary."
    SYNTAX      OCTET STRING (SIZE (0..1025))


-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDnsObjects              OBJECT IDENTIFIER ::= { juniDnsMIB 1 }
juniDnsGeneral              OBJECT IDENTIFIER ::= { juniDnsObjects 1 }
juniDnsServerList           OBJECT IDENTIFIER ::= { juniDnsObjects 2 }
juniDnsLocalDomainNameList  OBJECT IDENTIFIER ::= { juniDnsObjects 3 }

--
-- General DNS Control Objects
--
juniDnsEnable OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Exerts administrative control to enable/disable DNS capability."
    ::= { juniDnsGeneral 1 }


--
-- The DNS Server List
--
juniDnsServerListNextIndex OBJECT-TYPE
    SYNTAX      JuniNextServerListIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate juniDnsServerListIndex value allocation for entries in
        juniDnsServerListTable.

        A GET of this object returns the next available index value to be used
        to create an entry in the associated table; or zero, if no valid index
        value is available.  This object also returns a value of zero when it is
        the lexicographic successor of a varbind presented in an SNMP GETNEXT or
        GETBULK request, for which circumstance it is assumed that index
        allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniDnsServerList 1 }

juniDnsServerListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDnsServerListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains an entry for each DNS server."
    ::= { juniDnsServerList 2 }

juniDnsServerListEntry OBJECT-TYPE
    SYNTAX      JuniDnsServerListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry corresponds to an associated DNS server."
    INDEX     { juniDnsServerListIndex }
    ::= { juniDnsServerListTable 1 }

JuniDnsServerListEntry ::= SEQUENCE {
    juniDnsServerListIndex      ServerListIndex,        
    juniDnsServerListAddress    IpAddress,   -- obsoleted
    juniDnsServerListRowStatus  RowStatus,
    juniDnsV4V6ServerListAddressType InetAddressType,
    juniDnsV4V6ServerListAddress     InetAddress }

juniDnsServerListIndex OBJECT-TYPE
    SYNTAX      ServerListIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of the DNS server.  When creating entries in this table,
        suitable values for this object are determined by reading
        juniDnsServerListNextIndex."
    ::= { juniDnsServerListEntry 1 }

juniDnsServerListAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The IP address of the DNS server.  This object has been replaced by
        juniDnsV4V6ServerListAddressType and juniDnsV4V6ServerListAddress."
    ::= { juniDnsServerListEntry 2 }

juniDnsServerListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy"
    ::= { juniDnsServerListEntry 3 }

juniDnsV4V6ServerListAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The type of IP address (IPv4 or IPv6) of the DNS server."
    ::= { juniDnsServerListEntry 4 }

juniDnsV4V6ServerListAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address of the DNS server.

         Note: Since this object is used to configure the IPv4 or IPv6 address 
               depending on juniDnsV4V6ServerListAddressType value, it is
               mandatory to provide the IPv4 or IPv6 address by specifying each
               octet's positional values explicitly.
               Example:
                     1. IPv4 -- 4  octets  --  0xFF 0xFF 0xFF 0xFF
                     2. IPv6 -- 16 octets  --  0xFF 0xFF 0xFF 0xFF
                                               0xFF 0xFF 0xFF 0xFF
                                               0xFF 0xFF 0xFF 0xFF
                                               0xFF 0xFF 0xFF 0xFF "
    ::= { juniDnsServerListEntry 5 }

--
-- The DNS Local Domain Name List
--
juniDnsLocalDomainNameListNextIndex OBJECT-TYPE
    SYNTAX      JuniNextLocalDomainNameListIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate juniDnsLocalDomainNameListIndex value allocation for entries
        in juniDnsLocalDomainNameListTable.

        A GET of this object returns the next available index value to be used
        to create an entry in the associated table; or zero, if no valid index
        value is available.  This object also returns a value of zero when it is
        the lexicographic successor of a varbind presented in an SNMP GETNEXT or
        GETBULK request, for which circumstance it is assumed that index
        allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniDnsLocalDomainNameList 1 }

juniDnsLocalDomainNameListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDnsLocalDomainNameListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains an entry for each recognized local domain name."
    ::= { juniDnsLocalDomainNameList 2 }

juniDnsLocalDomainNameListEntry OBJECT-TYPE
    SYNTAX      JuniDnsLocalDomainNameListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry corresponds to a recognized local domain name."
    INDEX     { juniDnsLocalDomainNameListIndex }
    ::= { juniDnsLocalDomainNameListTable 1 }

JuniDnsLocalDomainNameListEntry ::= SEQUENCE {
    juniDnsLocalDomainNameListIndex         LocalDomainNameListIndex,        
    juniDnsLocalDomainNameListName          LocalDomainName,
    juniDnsLocalDomainNameListRowStatus     RowStatus }

juniDnsLocalDomainNameListIndex OBJECT-TYPE
    SYNTAX      LocalDomainNameListIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of the domain name.  When creating entries in this table,
        suitable values for this object are determined by reading
        juniDnsLocalDomainNameListNextIndex."
    ::= { juniDnsLocalDomainNameListEntry 1 }

juniDnsLocalDomainNameListName OBJECT-TYPE
    SYNTAX      LocalDomainName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A recognized local domain name."
    ::= { juniDnsLocalDomainNameListEntry 2 }

juniDnsLocalDomainNameListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy"
    ::= { juniDnsLocalDomainNameListEntry 3 }


-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDnsConformance     OBJECT IDENTIFIER ::= { juniDnsMIB 2 }
juniDnsCompliances     OBJECT IDENTIFIER ::= { juniDnsConformance 1 }
juniDnsGroups          OBJECT IDENTIFIER ::= { juniDnsConformance 2 }

--
-- compliance statements
--
juniDnsCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper DNS
        MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDnsEnableGroup,
            juniDnsServerListGroup,
            juniDnsV4V6ServerListGroup,
            juniDnsLocalDomainNameListGroup }
    ::= { juniDnsCompliances 1 }                                   -- JUNOSe 3.0

--
-- units of conformance
--
juniDnsEnableGroup OBJECT-GROUP
    OBJECTS {
        juniDnsEnable }
    STATUS      current
    DESCRIPTION
        "A collection of objects for enabling/disabling DNS capabilities in a
        Juniper product."
    ::= { juniDnsGroups 1 }

juniDnsServerListGroup OBJECT-GROUP
    OBJECTS {
        juniDnsServerListNextIndex,

        juniDnsServerListAddress,
        juniDnsServerListRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing DNS server list
        capabilities in a Juniper product.  This group became obsolete when IPv2
        address support was added."
    ::= { juniDnsGroups 2 }

juniDnsLocalDomainNameListGroup OBJECT-GROUP
    OBJECTS {
        juniDnsLocalDomainNameListNextIndex,
        juniDnsLocalDomainNameListName,
        juniDnsLocalDomainNameListRowStatus }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing DNS local domain name list
        capabilities in a Juniper product."
    ::= { juniDnsGroups 3 }


juniDnsV4V6ServerListGroup OBJECT-GROUP
    OBJECTS {
        juniDnsServerListNextIndex,
        juniDnsServerListRowStatus,
        juniDnsV4V6ServerListAddress,
        juniDnsV4V6ServerListAddressType }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing DNS server list capabilities in a
        Juniper product."
    ::= { juniDnsGroups 4 }

END
