
-- *****************************************************************************
-- Juniper-DVMRP-MIB
--
-- Juniper Networks Enterprise MIB
--   DVMRP MIB
--
-- Copyright (c) 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002, 2003 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-DVMRP-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Unsigned32, NOTIFICATION-TYPE,
    IpAddress, TimeTicks
        FROM SNMPv2-SMI
    DisplayString, RowStatus, TruthValue
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    InterfaceIndex
        FROM IF-MIB
    junidDvmrpInterfaceEntry
        FROM DVMRP-STD-MIB-JUNI
    juniMibs
        FROM Juniper-MIBs;

juniDvmrpMIB  MODULE-IDENTITY
    LAST-UPDATED "200301162055Z"  -- 16-Jan-03 03:55 PM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The Enterprise MIB module for management of Juniper DVMRP routers."
    -- Revision History
    REVISION    "200301162055Z"  -- 16-Jan-03 03:55 PM EST  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         Added support for unicast routing and the interface announce list
         name."
    REVISION    "200111302124Z"  -- 30-Nov-01 04:24 PM EST  - JUNOSe 3.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 44 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDvmrpMIBObjects OBJECT IDENTIFIER ::= { juniDvmrpMIB 1 }
juniDvmrp           OBJECT IDENTIFIER ::= { juniDvmrpMIBObjects 1 }
juniDvmrpScalar     OBJECT IDENTIFIER ::= { juniDvmrp 1 }

--
-- Juniper DVMRP scalar objects.
--
juniDvmrpAdminState  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Controls whether DVMRP is enabled or not."
    ::= { juniDvmrpScalar 1 }

juniDvmrpMcastAdminState  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Whether multicast is enabled or not.  This is settable via the
        multicast component."
    ::= { juniDvmrpScalar 2 }

juniDvmrpRouteHogNotification  OBJECT-TYPE
    SYNTAX      Integer32 (0..134217727)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The number of routes allowed within a 1 minute interval before a trap
        is issued warning that there may be a route surge going on."
    ::= { juniDvmrpScalar 3 }

juniDvmrpRouteLimit  OBJECT-TYPE
    SYNTAX      Integer32 (0..134217727)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The limit on the number of routes that may be advertised on a DVMRP
        interface."
    ::= { juniDvmrpScalar 4 }

juniDvmrpS32PrunesOnly  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Identifies when DVMRP is sending prunes and grafts with only a 32 bit
        source masks."
    ::= { juniDvmrpScalar 5 }

juniDvmrpUnicastRouting  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable/disable the unicast routing portion of the DVMRP."
    ::= { juniDvmrpScalar 6 }


--
-- The Juniper DVMRP access list distance neighbor group.
--
juniDvmrpAclDistNbrTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDvmrpAclDistNbrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing the access lists distance for a list of
        neighbors."
    ::= { juniDvmrp 2 }

juniDvmrpAclDistNbrEntry  OBJECT-TYPE
    SYNTAX      JuniDvmrpAclDistNbrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniDvmrpAclDistNbrTable."
    INDEX     { juniDvmrpAclDistNbrIfIndex,
                juniDvmrpAclDistNbrAclListName }
    ::= { juniDvmrpAclDistNbrTable 1 }

JuniDvmrpAclDistNbrEntry ::= SEQUENCE {
    juniDvmrpAclDistNbrIfIndex              InterfaceIndex,
    juniDvmrpAclDistNbrAclListName          DisplayString,
    juniDvmrpAclDistNbrDistance             Integer32,
    juniDvmrpAclDistNbrNbrListName          DisplayString,
    juniDvmrpAclDistNbrStatus               RowStatus }

juniDvmrpAclDistNbrIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex value of the interface for which DVMRP is enabled."
    ::= { juniDvmrpAclDistNbrEntry 1 }

juniDvmrpAclDistNbrAclListName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..80))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the access list to be used in the filter."
    ::= { juniDvmrpAclDistNbrEntry 2 }

juniDvmrpAclDistNbrDistance  OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administritive distance metric that will be used"
    DEFVAL    { 1 }
    ::= { juniDvmrpAclDistNbrEntry 3 }

juniDvmrpAclDistNbrNbrListName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..80))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the access list of nbrs for this accept-filter to be applied,
        this field must be supplied when the row is created"
    ::= { juniDvmrpAclDistNbrEntry 4 }

juniDvmrpAclDistNbrStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this entry."
    ::= { juniDvmrpAclDistNbrEntry 5 }


--
-- The Juniper DVMRP Local Address table.
-- This is used to retrive all of the addresses configured
-- on a DVMRP interface.
--
juniDvmrpLocalAddrTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDvmrpLocalAddrTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing the local addresses.  This is used to
        retrive all of the addresses configured on a DVMRP interface."
    ::= { juniDvmrp 3 }

juniDvmrpLocalAddrTableEntry  OBJECT-TYPE
    SYNTAX      JuniDvmrpLocalAddrTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniDvmrpLocalAddrTable."
    INDEX     { juniDvmrpLocalAddrIfIndex,
                juniDvmrpLocalAddrAddrOrIfIndex }
    ::= { juniDvmrpLocalAddrTable 1 }

JuniDvmrpLocalAddrTableEntry ::= SEQUENCE {
    juniDvmrpLocalAddrIfIndex            InterfaceIndex,
    juniDvmrpLocalAddrAddrOrIfIndex      Unsigned32,
    juniDvmrpLocalAddrMask               IpAddress }

juniDvmrpLocalAddrIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex value of the interface for which DVMRP is enabled."
    ::= { juniDvmrpLocalAddrTableEntry 1 }

juniDvmrpLocalAddrAddrOrIfIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "For unnumbered interfaces, this takes on the value of the ifIndex.  For
        numbered interfaces, this is the address of one of the addresses
        associated with the interface."
    ::= { juniDvmrpLocalAddrTableEntry 2 }

juniDvmrpLocalAddrMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP Address mask associated with this entry."
    ::= { juniDvmrpLocalAddrTableEntry 3 }


--
-- The Juniper DVMRP Summary Address table.
-- This is used to retrive all of the summary address configured
-- on a DVMRP interface.
--
juniDvmrpSummaryAddrTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDvmrpSummaryAddrTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing the DVMRP summary addresses.  This is
        used to retrive all of the summary address configured on a DVMRP
        interface."
    ::= { juniDvmrp 4 }

juniDvmrpSummaryAddrTableEntry  OBJECT-TYPE
    SYNTAX      JuniDvmrpSummaryAddrTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniDvmrpSummaryAddrTable."
    INDEX     { juniDvmrpSummaryAddrIfIndex,
                juniDvmrpSummaryAddrAddress,
                juniDvmrpSummaryAddrMask }
    ::= { juniDvmrpSummaryAddrTable 1 }

JuniDvmrpSummaryAddrTableEntry ::= SEQUENCE {
    juniDvmrpSummaryAddrIfIndex          InterfaceIndex,
    juniDvmrpSummaryAddrAddress          IpAddress,
    juniDvmrpSummaryAddrMask             IpAddress,
    juniDvmrpSummaryAddrCost             Integer32,
    juniDvmrpSummaryAddrStatus           RowStatus }

juniDvmrpSummaryAddrIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex value of the interface for which DVMRP is enabled."
    ::= { juniDvmrpSummaryAddrTableEntry 1 }

juniDvmrpSummaryAddrAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the summary address that will be created."
    ::= { juniDvmrpSummaryAddrTableEntry 2 }

juniDvmrpSummaryAddrMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The mask of the summary address to be created."
    ::= { juniDvmrpSummaryAddrTableEntry 3 }

juniDvmrpSummaryAddrCost  OBJECT-TYPE
    SYNTAX      Integer32 (1..32)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administritive distance metric used to actually calculate distance
        vectors."
    DEFVAL    { 1 }
    ::= { juniDvmrpSummaryAddrTableEntry 4 }

juniDvmrpSummaryAddrStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this entry."
    ::= { juniDvmrpSummaryAddrTableEntry 5 }


--
-- The Juniper DVMRP Interface Table.
--
juniDvmrpInterfaceTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDvmrpInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing the router's multicast-capable
        interfaces.  This table augments the DvmrpInterfaceTable."
    ::= { juniDvmrp 5 }

juniDvmrpInterfaceEntry  OBJECT-TYPE
    SYNTAX      JuniDvmrpInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniDvmrpInterfaceTable.  This row
        extends ipMRouteInterfaceEntry in the IP Multicast MIB, where the
        threshold object resides."
    AUGMENTS  { junidDvmrpInterfaceEntry }
    ::= { juniDvmrpInterfaceTable 1 }

JuniDvmrpInterfaceEntry ::= SEQUENCE {
    juniDvmrpInterfaceAutoSummary           INTEGER,
    juniDvmrpInterfaceMetricOffsetOut       Integer32,
    juniDvmrpInterfaceMetricOffsetIn        Integer32,
    juniDvmrpInterfaceAdminState            INTEGER,
    juniDvmrpInterfaceAnnounceListName      DisplayString }

juniDvmrpInterfaceAutoSummary  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enables or disable auto-summarization on this interface."
    ::= { juniDvmrpInterfaceEntry 3 }

juniDvmrpInterfaceMetricOffsetOut  OBJECT-TYPE
    SYNTAX      Integer32 (0..31)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The distance metric for this interface which is used to calculate
        outbound distance vectors."
    DEFVAL    { 0 }
    ::= { juniDvmrpInterfaceEntry 4 }

juniDvmrpInterfaceMetricOffsetIn  OBJECT-TYPE
    SYNTAX      Integer32 (0..31)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The distance metric for this interface which is used to calculate
        inbound distance vectors."
    DEFVAL    { 1 }
    ::= { juniDvmrpInterfaceEntry 5 }

juniDvmrpInterfaceAdminState  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls whether DVMRP is enabled or not."
    ::= { juniDvmrpInterfaceEntry 6 }

juniDvmrpInterfaceAnnounceListName  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Configures the name of the acceptance announce filter for the IP access
        list."
    ::= { juniDvmrpInterfaceEntry 7 }


--
-- The Juniper DVMRP Prune Table
--
juniDvmrpPruneTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDvmrpPruneEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing the router's upstream prune state."
    ::= { juniDvmrp 6 }

juniDvmrpPruneEntry  OBJECT-TYPE
    SYNTAX      JuniDvmrpPruneEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniDvmrpPruneTable."
    INDEX     { juniDvmrpPruneGroup,
                juniDvmrpPruneSource,
                juniDvmrpPruneSourceMask }
    ::= { juniDvmrpPruneTable 1 }

JuniDvmrpPruneEntry ::= SEQUENCE {
    juniDvmrpPruneGroup              IpAddress,
    juniDvmrpPruneSource             IpAddress,
    juniDvmrpPruneSourceMask         IpAddress,
    juniDvmrpPruneIIFIfIndex         InterfaceIndex,
    juniDvmrpPruneUpTime             TimeTicks }

juniDvmrpPruneGroup  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The group address which has been pruned."
    ::= { juniDvmrpPruneEntry 1 }

juniDvmrpPruneSource  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The address of the source or source network which has been pruned."
    ::= { juniDvmrpPruneEntry 2 }

juniDvmrpPruneSourceMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The address of the source or source network which has been pruned.  The
        mask must either be all 1's, or else juniDvmrpPruneSource and
        juniDvmrpPruneSourceMask must match juniDvmrpRouteSource and
        juniDvmrpRouteSourceMask for some entry in the juniDvmrpRouteTable."
    ::= { juniDvmrpPruneEntry 3 }

juniDvmrpPruneIIFIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of the upstream interface for this source group entry."
    ::= { juniDvmrpPruneEntry 4 }

juniDvmrpPruneUpTime  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the amount of time that this prune has remained valid."
    ::= { juniDvmrpPruneEntry 5 }


--
-- The Juniper DVMRP source group OIF table
--
juniDvmrpSrcGrpOifTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDvmrpSrcGrpOifEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) OIFs for particular source group entries."
    ::= { juniDvmrp 7 }

juniDvmrpSrcGrpOifEntry  OBJECT-TYPE
    SYNTAX      JuniDvmrpSrcGrpOifEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniDvmrpSrcGrpOifTable."
    INDEX     { juniDvmrpSrcGrpOifGroup,
                juniDvmrpSrcGrpOifSource,
                juniDvmrpSrcGrpOifSourceMask,
                juniDvmrpSrcGrpOifOIFIfIndex }
    ::= { juniDvmrpSrcGrpOifTable 1 }

JuniDvmrpSrcGrpOifEntry ::= SEQUENCE {
    juniDvmrpSrcGrpOifGroup              IpAddress,
    juniDvmrpSrcGrpOifSource             IpAddress,
    juniDvmrpSrcGrpOifSourceMask         IpAddress,
    juniDvmrpSrcGrpOifOIFIfIndex         InterfaceIndex,
    juniDvmrpSrcGrpOifOIFPruned          INTEGER,
    juniDvmrpSrcGrpOifOIFDnTTL           TimeTicks }

juniDvmrpSrcGrpOifGroup  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The group address which has been pruned."
    ::= { juniDvmrpSrcGrpOifEntry 1 }

juniDvmrpSrcGrpOifSource  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The address of the source or source network which has been pruned."
    ::= { juniDvmrpSrcGrpOifEntry 2 }

juniDvmrpSrcGrpOifSourceMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The address of the source or source network which has been pruned.  The
        mask must either be all 1's, or else juniDvmrpPruneSource and
        juniDvmrpPruneSourceMask must match juniDvmrpRouteSource and
        juniDvmrpRouteSourceMask for some entry in the juniDvmrpRouteTable."
    ::= { juniDvmrpSrcGrpOifEntry 3 }

juniDvmrpSrcGrpOifOIFIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of one of the downstream interfaces for this source group
        entry."
    ::= { juniDvmrpSrcGrpOifEntry 4 }

juniDvmrpSrcGrpOifOIFPruned  OBJECT-TYPE
    SYNTAX      INTEGER {
                    false(0),
                    true(1) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "If true this OIF has been pruned."
    ::= { juniDvmrpSrcGrpOifEntry 5 }

juniDvmrpSrcGrpOifOIFDnTTL  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The timeout for this OIF.  If juniDvmrpSrcGrpOifOIFPruned is false
        then this is undefined."
    ::= { juniDvmrpSrcGrpOifEntry 6 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDvmrpTraps OBJECT IDENTIFIER ::= { juniDvmrp 0 }

juniDvmrpRouteHogNotificationTrap  NOTIFICATION-TYPE
    STATUS      current
    DESCRIPTION
        "This is an indication that the route hog notification limit has been
        exceeded during the past minute.  It may mean that a route surge is
        going on."
   ::= { juniDvmrpTraps 1 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDvmrpConformance OBJECT IDENTIFIER ::= { juniDvmrpMIB 4 }
juniDvmrpCompliances OBJECT IDENTIFIER ::= { juniDvmrpConformance 1 }
juniDvmrpGroups      OBJECT IDENTIFIER ::= { juniDvmrpConformance 2 }

--
-- compliance statements
--
juniDvmrpCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        DVMRP MIB.  This statement became obsolete when new objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDvmrpBaseGroup,
            juniDvmrpAclDistNbrGroup,
            juniDvmrpInterfaceGroup,
            juniDvmrpSourceGroup }
    ::= { juniDvmrpCompliances 1 }                                 -- JUNOSe 3.0

juniDvmrpCompliance2  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper DVMRP
        MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDvmrpBaseGroup2,
            juniDvmrpAclDistNbrGroup,
            juniDvmrpInterfaceGroup2,
            juniDvmrpSourceGroup }
    ::= { juniDvmrpCompliances 2 }                                 -- JUNOSe 5.0


--
-- units of conformance
--
juniDvmrpBaseGroup  OBJECT-GROUP
    OBJECTS {
        juniDvmrpAdminState,
        juniDvmrpMcastAdminState,
        juniDvmrpRouteHogNotification,
        juniDvmrpRouteLimit,
        juniDvmrpS32PrunesOnly }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing basic management of DVMRP in a
        Juniper product.  This group became obsolete when support was added for
        the DVMRP unicast routing object."
    ::= { juniDvmrpGroups 1 }

juniDvmrpAclDistNbrGroup  OBJECT-GROUP
    OBJECTS {
        juniDvmrpAclDistNbrDistance,
        juniDvmrpAclDistNbrNbrListName,
        juniDvmrpAclDistNbrStatus }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of DVMRP access list
        distance neighbors in a Juniper product."
    ::= { juniDvmrpGroups 2 }

juniDvmrpInterfaceGroup  OBJECT-GROUP
    OBJECTS {
        juniDvmrpLocalAddrMask,

        juniDvmrpSummaryAddrCost,
        juniDvmrpSummaryAddrStatus,

        juniDvmrpInterfaceAutoSummary,
        juniDvmrpInterfaceMetricOffsetOut,
        juniDvmrpInterfaceMetricOffsetIn,
        juniDvmrpInterfaceAdminState }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of a DVMRP
        interface in a Juniper product.  This group became obsolete when support
        for the DVMRP interface announce list name object was added."
    ::= { juniDvmrpGroups 3 }

juniDvmrpSourceGroup  OBJECT-GROUP
    OBJECTS {
        juniDvmrpPruneIIFIfIndex,
        juniDvmrpPruneUpTime,

        juniDvmrpSrcGrpOifOIFPruned,
        juniDvmrpSrcGrpOifOIFDnTTL }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of a DVMRP source group in
        a Juniper product."
    ::= { juniDvmrpGroups 4 }

juniDvmrpNotificationGroup  NOTIFICATION-GROUP
    NOTIFICATIONS {
        juniDvmrpRouteHogNotificationTrap }
    STATUS      current
    DESCRIPTION
        "A notification for signaling important DVMRP events."
    ::= { juniDvmrpGroups 5 }

juniDvmrpBaseGroup2  OBJECT-GROUP
    OBJECTS {
        juniDvmrpAdminState,
        juniDvmrpMcastAdminState,
        juniDvmrpRouteHogNotification,
        juniDvmrpRouteLimit,
        juniDvmrpS32PrunesOnly,
        juniDvmrpUnicastRouting  }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing basic management of DVMRP in a
        Juniper product."
    ::= { juniDvmrpGroups  6 }

juniDvmrpInterfaceGroup2  OBJECT-GROUP
    OBJECTS {
        juniDvmrpLocalAddrMask,

        juniDvmrpSummaryAddrCost,
        juniDvmrpSummaryAddrStatus,

        juniDvmrpInterfaceAutoSummary,
        juniDvmrpInterfaceMetricOffsetOut,
        juniDvmrpInterfaceMetricOffsetIn,
        juniDvmrpInterfaceAdminState ,
        juniDvmrpInterfaceAnnounceListName }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of a DVMRP interface in a
        Juniper product."
    ::= { juniDvmrpGroups 7 }

END
