
-- *****************************************************************************
-- Juniper Networks Data Products SNMP Experimental MIB Registry.
--
-- Copyright (c) 2000, 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002 Juniper Networks, Inc.
--   All rights reserved.
-- *****************************************************************************

Juniper-Experiment  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-IDENTITY
        FROM SNMPv2-SMI
    juniperUniExperiment
        FROM Juniper-UNI-SMI;

juniExperiment  MODULE-IDENTITY
    LAST-UPDATED "200211132058Z"  -- 13-Nov-02 03:58 PM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The object identifiers for experimental MIBs for the Juniper
        Networks, Inc. edge router products.  This is the top-level
        object identifier registry for SNMP modules containing experimental MIB
        definitions.  Experimental MIBs are defined as:

        1) IETF work-in-process MIBs which have not been assigned a permanent
           object identifier by the IANA.

        2) Juniper work-in-process MIBs that have not achieved final
           production quality or field experience.

        NOTE: Support for MIBs under the this OID subtree is temporary and
              changes to objects may occur without notice."
    -- Revision History
    REVISION    "200211132058Z"  -- 13-Nov-02 03:58 PM EST  - RX 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         Added OID for the Internet draft MPLS MIB."
    REVISION    "200106202036Z"  -- 20-Jun-01 04:36 PM EDT  - RX 4.0
    DESCRIPTION
        "Added OID for the Internet draft SONET APS-MIB."
    REVISION    "200010242100Z"  -- 24-Oct-00  5:00 PM EDT  - RX 3.0
    DESCRIPTION
        "The initial release of this management information module."
    ::= { juniperUniExperiment 2 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Experimental MIB OID assignments.
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDvmrpExperiment  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The object identifier used to anchor the experimental IETF draft for
        the Distance Vector Multicast Routing Protocol (DVMRP) MIB."
    REFERENCE
        "IETF Inter-Domain Multicast Routing (idmr) Working Group document:
        draft-ietf-idmr-dvmrp-mib-11.txt."
    ::= { juniExperiment 1 }

juniSonetApsExperiment  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The object identifier used to anchor the experimental IETF draft for
        the SONET linear Automatic Protection Switching (APS) MIB."
    REFERENCE
        "IETF AToM MIB (atommib) Working Group document:
        draft-ietf-atommib-sonetaps-mib-05.txt."
    ::= { juniExperiment 2 }

juniMplsExperiment  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The object identifier used to anchor the experimental IETF drafts for
        the Multiprotocol Label Switching (MPLS) set of MIBs."
    REFERENCE
        "IETF Multiprotocol Label Switching (MPLS) Working Group documents:
            draft-ietf-mpls-tc-mib-03.txt
            draft-ietf-mpls-lsr-mib-08.txt."
    ::= { juniExperiment 3 }

juniMplsVPNExperiment  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The object identifier used to anchor the experimental IETF drafts for
        the MPLS/BGP Layer 3 Virtual Private Network Management Information Base."
    REFERENCE
        "IETF Layer-3 Virtual Private Networks Working Group documents:
            draft-ietf-l3vpn-mpls-vpn-mib-07.txt."
    ::= { juniExperiment 4 }
    
juniBFDExperiment  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The object identifier used to anchor the experimental IETF drafts for
        BFD Management Information Base."
    REFERENCE
        "Bidirectional Forwarding Detection Management Information Base 
			draft-ietf-bfd-mib-02.txt "
    ::= { juniExperiment 5}

END
