-- This module defines enterprise MIBs DI Setting.
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-IDS-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenIDS
        FROM NETSCREEN-SMI
    Counter32, Integer32, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    ;

nsIdsProtect MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines NetScreen private MIBs DI Setting."
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200204260000Z" -- April 26, 2002
    DESCRIPTION
        "Screen option on zone setting, add new screen option (Zhong
         Wang)"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "No Comment"
    REVISION      "200101080000Z" -- January 08, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenIDS 1 }

NsIdsAttkMonEntry ::= SEQUENCE
{
    nsIdsAttkMonIfIdx       Integer32,
    nsIdsAttkMonVsys        Integer32,
    nsIdsAttkMonSynAttk     Counter32,
    nsIdsAttkMonTearDrop    Counter32,
    nsIdsAttkMonSrcRoute    Counter32,
    nsIdsAttkMonPingDeath   Counter32,
    nsIdsAttkMonAddrSpoof   Counter32,
    nsIdsAttkMonLand        Counter32,
    nsIdsAttkMonIcmpFlood   Counter32,
    nsIdsAttkMonUdpFlood    Counter32,
    nsIdsAttkMonWinnuke     Counter32,
    nsIdsAttkMonPortScan    Counter32,
    nsIdsAttkMonIpSweep     Counter32,
    nsAttkMonSynFrag        Counter32,
    nsAttkMonTcpNoFlag      Counter32,
    nsAttkMonIpUnknownProt  Counter32,
    nsAttkMonIpOptBad       Counter32,
    nsAttkMonIpOptRecord    Counter32,
    nsAttkMonIpOptTimestamp Counter32,
    nsAttkMonIpOptSCHT      Counter32,
    nsAttkMonIpOptLSR       Counter32,
    nsAttkMonIpOptSSR       Counter32,
    nsAttkMonIpOptStream    Counter32,
    nsAttkMonIcmpFrag       Counter32,
    nsAttkMonIcmpLarge      Counter32,
    nsAttkMonTcpSynFin      Counter32,
    nsAttkMonTcpFinNoAck    Counter32,
    nsAttkMonHttpMalUrl     Counter32,
    nsAttkMonSessMalNum     Counter32,
    nsAttkMonSynAckAck      Counter32,
    nsAttkMonIpFrag         Counter32,
    nsIdsAttkMonIfInfo      Integer32
}

NsIdsProtectSetEntry ::= SEQUENCE
{
    nsIdsProtectZoneIdx       Integer32,
    nsIdsDetectPingOfDeath    INTEGER,
    nsIdsDetectTearDrop       INTEGER,
    nsIdsDetectWinNuke        INTEGER,
    nsIdsFilterIpSrcRoute     INTEGER,
    nsIdsDetectPortScan       INTEGER,
    nsIdsDetectAddrSweep      INTEGER,
    nsIdsDetectLand           INTEGER,
    nsIdsBlockComponent       INTEGER,
    nsIdsDetectIpSpoof        INTEGER,
    nsIdsDetectSyn            INTEGER,
    nsIdsDetectIcmpFlood      INTEGER,
    nsIdsDetectUdpFlood       INTEGER,
    nsIdsDetectSynFrag        INTEGER,
    nsIdsDetectTcpNoFlag      INTEGER,
    nsIdsDetectIpUnknownProt  INTEGER,
    nsIdsDetectIpOptBad       INTEGER,
    nsIdsDetectIpOptRecord    INTEGER,
    nsIdsDetectIpOptTimestamp INTEGER,
    nsIdsDetectIpOptSCHT      INTEGER,
    nsIdsDetectIpOptLSR       INTEGER,
    nsIdsDetectIpOptSSR       INTEGER,
    nsIdsDetectIpOptStream    INTEGER,
    nsIdsDetectIcmpFrag       INTEGER,
    nsIdsDetectIcmpLarge      INTEGER,
    nsIdsDetectTcpSynFin      INTEGER,
    nsIdsDetectTcpFinNoAck    INTEGER,
    nsIdsHttpMalUrl           INTEGER,
    nsIdsSessMalNum           INTEGER,
    nsIdsDetectSynAckAck      INTEGER,
    nsIdsDetectIpFrag         INTEGER
}

NsIdsProtectThreshEntry ::= SEQUENCE
{
    nsIdsProtectThreshZoneIdx Integer32,
    nsIdsSynAttackThresh      Integer32,
    nsIdsSynAttackTimeout     Integer32,
    nsIdsSynAttackAlmTh       Integer32,
    nsIdsSynAttackQueSize     Integer32,
    nsIdsSynAttackAgeTime     Integer32,
    nsIdsIcmpFloodThresh      Integer32,
    nsIdsUdpFloodThresh       Integer32,
    nsIdsPortScanThresh       Integer32,
    nsIdsIpSweepThresh        Integer32,
    nsIdsSynAckAckThres       Integer32
}

nsIdsProtectSetTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsIdsProtectSetEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "NetScreen ScreenOS can allow DI protection on each of
         NetScreen device's physical interface. This table collects the
         DI protection configuration on each physical interface."
    ::= { nsIdsProtect 1 }

nsIdsProtectSetEntry OBJECT-TYPE
    SYNTAX        NsIdsProtectSetEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Hold the DI setting attribute."
    INDEX
        { nsIdsProtectZoneIdx }
    ::= { nsIdsProtectSetTable 1 }

nsIdsProtectZoneIdx OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "unique zone id."
    ::= { nsIdsProtectSetEntry 1 }

nsIdsDetectPingOfDeath OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Ping of Death."
    ::= { nsIdsProtectSetEntry 2 }

nsIdsDetectTearDrop OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Tear Drop Attack."
    ::= { nsIdsProtectSetEntry 3 }

nsIdsDetectWinNuke OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Win Nuke Attack."
    ::= { nsIdsProtectSetEntry 4 }

nsIdsFilterIpSrcRoute OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Filter IP Source Route Option attack."
    ::= { nsIdsProtectSetEntry 5 }

nsIdsDetectPortScan OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Port Scan Death attack."
    ::= { nsIdsProtectSetEntry 6 }

nsIdsDetectAddrSweep OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Address Sweep Attack."
    ::= { nsIdsProtectSetEntry 7 }

nsIdsDetectLand OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Land Attack."
    ::= { nsIdsProtectSetEntry 8 }

nsIdsBlockComponent OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Block Java/ActiveX/ZIP/EXE Component."
    ::= { nsIdsProtectSetEntry 9 }

nsIdsDetectIpSpoof OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP Spoofing attack."
    ::= { nsIdsProtectSetEntry 10 }

nsIdsDetectSyn OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect SYN attack."
    ::= { nsIdsProtectSetEntry 11 }

nsIdsDetectIcmpFlood OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect ICMP Flood attack."
    ::= { nsIdsProtectSetEntry 12 }

nsIdsDetectUdpFlood OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect UDP Flood attack."
    ::= { nsIdsProtectSetEntry 13 }

nsIdsDetectSynFrag OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect SYN fragment"
    ::= { nsIdsProtectSetEntry 14 }

nsIdsDetectTcpNoFlag OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect TCP without flag set."
    ::= { nsIdsProtectSetEntry 15 }

nsIdsDetectIpUnknownProt OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Unknown protocol IP packet."
    ::= { nsIdsProtectSetEntry 16 }

nsIdsDetectIpOptBad OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP bad option."
    ::= { nsIdsProtectSetEntry 17 }

nsIdsDetectIpOptRecord OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP record option."
    ::= { nsIdsProtectSetEntry 18 }

nsIdsDetectIpOptTimestamp OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP timestamp option."
    ::= { nsIdsProtectSetEntry 19 }

nsIdsDetectIpOptSCHT OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP security option."
    ::= { nsIdsProtectSetEntry 20 }

nsIdsDetectIpOptLSR OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Loose source route."
    ::= { nsIdsProtectSetEntry 21 }

nsIdsDetectIpOptSSR OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect strict source route."
    ::= { nsIdsProtectSetEntry 22 }

nsIdsDetectIpOptStream OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP stream option."
    ::= { nsIdsProtectSetEntry 23 }

nsIdsDetectIcmpFrag OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect ICMP fragment."
    ::= { nsIdsProtectSetEntry 24 }

nsIdsDetectIcmpLarge OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect large ICMP packet."
    ::= { nsIdsProtectSetEntry 25 }

nsIdsDetectTcpSynFin OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect TCP syn fin both set."
    ::= { nsIdsProtectSetEntry 26 }

nsIdsDetectTcpFinNoAck OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect TCP fin set without ack bit set."
    ::= { nsIdsProtectSetEntry 27 }

nsIdsHttpMalUrl OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect malicious URL."
    ::= { nsIdsProtectSetEntry 28 }

nsIdsSessMalNum OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect malicious session connection."
    ::= { nsIdsProtectSetEntry 29 }

nsIdsDetectSynAckAck OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect SYN ACK ACK DoS."
    ::= { nsIdsProtectSetEntry 30 }

nsIdsDetectIpFrag OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Block IP fragment packet."
    ::= { nsIdsProtectSetEntry 31 }

nsIdsProtectThreshTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsIdsProtectThreshEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "NetScreen ScreenOS can allow DI protection on each of
         NetScreen device's physical interface. This table collects the
         DI protection configuration on each physical interface."
    ::= { nsIdsProtect 2 }

nsIdsProtectThreshEntry OBJECT-TYPE
    SYNTAX        NsIdsProtectThreshEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Hold the DI setting attribute."
    INDEX
        { nsIdsProtectThreshZoneIdx }
    ::= { nsIdsProtectThreshTable 1 }

nsIdsProtectThreshZoneIdx OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "unique zone id."
    ::= { nsIdsProtectThreshEntry 1 }

nsIdsSynAttackThresh OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SYN attack threshold."
    ::= { nsIdsProtectThreshEntry 2 }

nsIdsSynAttackTimeout OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SYN attack timeout."
    ::= { nsIdsProtectThreshEntry 3 }

nsIdsSynAttackAlmTh OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SYN attack alarm threshold."
    ::= { nsIdsProtectThreshEntry 4 }

nsIdsSynAttackQueSize OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SYN attack queue size."
    ::= { nsIdsProtectThreshEntry 5 }

nsIdsSynAttackAgeTime OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SYN flood age time."
    ::= { nsIdsProtectThreshEntry 6 }

nsIdsIcmpFloodThresh OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ICMP attack alarm threshold."
    ::= { nsIdsProtectThreshEntry 7 }

nsIdsUdpFloodThresh OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "UDP attack alarm threshold."
    ::= { nsIdsProtectThreshEntry 8 }

nsIdsPortScanThresh OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ICMP attack alarm threshold."
    ::= { nsIdsProtectThreshEntry 9 }

nsIdsIpSweepThresh OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "UDP attack alarm threshold."
    ::= { nsIdsProtectThreshEntry 10 }

nsIdsSynAckAckThres OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "SYN ack ack alarm threshold."
    ::= { nsIdsProtectThreshEntry 11 }

nsIdsAttkMonTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsIdsAttkMonEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The table monitors the intrusion attack attemps amount to
         NetScreen Device."
    ::= { netscreenIDS 2 }

nsIdsAttkMonEntry OBJECT-TYPE
    SYNTAX        NsIdsAttkMonEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry containing intrusion attack couters."
    INDEX
        { nsIdsAttkMonIfIdx }
    ::= { nsIdsAttkMonTable 1 }

nsIdsAttkMonIfIdx OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "unique interface id."
    ::= { nsIdsAttkMonEntry 1 }

nsIdsAttkMonVsys OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "according NetScreen's concepts. each interface belongs to one
         virtual system. This attribute displays the virtual system name
         an interface belongs to."
    ::= { nsIdsAttkMonEntry 2 }

nsIdsAttkMonSynAttk OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "sync attack packet counter."
    ::= { nsIdsAttkMonEntry 3 }

nsIdsAttkMonTearDrop OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "tear drop attack packet counter."
    ::= { nsIdsAttkMonEntry 4 }

nsIdsAttkMonSrcRoute OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "source route option attack packet counter."
    ::= { nsIdsAttkMonEntry 5 }

nsIdsAttkMonPingDeath OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ping of death attack packet counter."
    ::= { nsIdsAttkMonEntry 6 }

nsIdsAttkMonAddrSpoof OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "address spoofing attack packet counter."
    ::= { nsIdsAttkMonEntry 7 }

nsIdsAttkMonLand OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "land attack packet counter."
    ::= { nsIdsAttkMonEntry 8 }

nsIdsAttkMonIcmpFlood OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ICMP flood attack packet counter."
    ::= { nsIdsAttkMonEntry 9 }

nsIdsAttkMonUdpFlood OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "udp flood attack packet counter."
    ::= { nsIdsAttkMonEntry 10 }

nsIdsAttkMonWinnuke OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "weired netbios attack packet counter."
    ::= { nsIdsAttkMonEntry 11 }

nsIdsAttkMonPortScan OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "port scan attempt attack packet counter."
    ::= { nsIdsAttkMonEntry 12 }

nsIdsAttkMonIpSweep OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "address sweep attemp attack packet counter."
    ::= { nsIdsAttkMonEntry 13 }

nsAttkMonSynFrag OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect SYN fragment"
    ::= { nsIdsAttkMonEntry 14 }

nsAttkMonTcpNoFlag OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect TCP without flag set."
    ::= { nsIdsAttkMonEntry 15 }

nsAttkMonIpUnknownProt OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Unknown protocol IP packet."
    ::= { nsIdsAttkMonEntry 16 }

nsAttkMonIpOptBad OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP bad option."
    ::= { nsIdsAttkMonEntry 17 }

nsAttkMonIpOptRecord OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP record option."
    ::= { nsIdsAttkMonEntry 18 }

nsAttkMonIpOptTimestamp OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP timestamp option."
    ::= { nsIdsAttkMonEntry 19 }

nsAttkMonIpOptSCHT OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP security option."
    ::= { nsIdsAttkMonEntry 20 }

nsAttkMonIpOptLSR OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect Loose source route."
    ::= { nsIdsAttkMonEntry 21 }

nsAttkMonIpOptSSR OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect strict source route."
    ::= { nsIdsAttkMonEntry 22 }

nsAttkMonIpOptStream OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect IP stream option."
    ::= { nsIdsAttkMonEntry 23 }

nsAttkMonIcmpFrag OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect ICMP fragment."
    ::= { nsIdsAttkMonEntry 24 }

nsAttkMonIcmpLarge OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect large ICMP packet."
    ::= { nsIdsAttkMonEntry 25 }

nsAttkMonTcpSynFin OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect TCP syn fin both set."
    ::= { nsIdsAttkMonEntry 26 }

nsAttkMonTcpFinNoAck OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect TCP fin set without ack bit set."
    ::= { nsIdsAttkMonEntry 27 }

nsAttkMonHttpMalUrl OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect malicious URL."
    ::= { nsIdsAttkMonEntry 28 }

nsAttkMonSessMalNum OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect malicious session connection."
    ::= { nsIdsAttkMonEntry 29 }

nsAttkMonSynAckAck OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Detect SYN ACK ACK attack."
    ::= { nsIdsAttkMonEntry 30 }

nsAttkMonIpFrag OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Block IP fragment packet."
    ::= { nsIdsAttkMonEntry 31 }

nsIdsAttkMonIfInfo OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Internal id assigned to this interface. Stays persistent across resets."
    ::= { nsIdsAttkMonEntry 32 }

END


