
-- *****************************************************************************
-- Juniper-SSC-CLIENT-MIB
--
-- Juniper Networks Enterprise MIB
--   Service Selection Center (SSC) Client
--
-- Copyright (c) 2000, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002, 2003 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-SSC-CLIENT-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, IpAddress, Counter32
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    JuniName
        FROM Juniper-TC
    juniMibs
        FROM Juniper-MIBs;

juniSscClientMIB  MODULE-IDENTITY
    LAST-UPDATED "200312181629Z"  -- 18-Dec-03 11:29 AM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The Service Selection Center (SSC) Client MIB for the Juniper Networks
        enterprise."
    -- Revision History
    REVISION    "200312181629Z"  -- 18-Dec-03 11:29 AM EST  - JUNOSe 5.3
    DESCRIPTION
        "Obsoleted token and added discover scalar statistics."
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200201142015Z"  -- 14-Jan-02 03:15 PM EST  - JUNOSe 4.0
    DESCRIPTION
        "Added version number, local address and transport router name objects."
    REVISION    "200101232130Z"  -- 23-Jan-01 04:30 PM EST  - JUNOSe 3.1
    DESCRIPTION
        "Added DHCP-LS, Web and SSC support."
    REVISION    "200002172310Z"  -- 17-Feb-00  6:10 PM EST  - JUNOSe 2.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 36 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniSscClientObjects      OBJECT IDENTIFIER ::= { juniSscClientMIB 1 }

juniSscClientCfg          OBJECT IDENTIFIER ::= { juniSscClientObjects 1 }
juniSscClientStatus       OBJECT IDENTIFIER ::= { juniSscClientObjects 2 }
juniSscClientStatistics   OBJECT IDENTIFIER ::= { juniSscClientObjects 3 }


--
-- Configuration scalars
--
juniSscClientCfgScalars   OBJECT IDENTIFIER ::= { juniSscClientCfg 1 }

juniSscClientServerSwitchoverTimeout  OBJECT-TYPE
    SYNTAX      Integer32 (5..300)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The server switchover timeout in seconds.  The SSC Client begins with
        the primary server and proceeds rotationally to secondary, tertiary,
        primary, etc. as timeouts occur."
    ::= { juniSscClientCfgScalars 1 }

juniSscClientPrimaryAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The IP address of the primary SSC server.  A value of 0.0.0.0 indicates
        the server address is unconfigured."
    ::= { juniSscClientCfgScalars 2 }

juniSscClientPrimaryPort  OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The TCP port number for the primary SSC server.  A value of zero
        indicates the port is unconfigured."
    ::= { juniSscClientCfgScalars 3 }

juniSscClientSecondaryAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The IP address of the secondary SSC server.  A value of 0.0.0.0
        indicates the server address is unconfigured."
    ::= { juniSscClientCfgScalars 4 }

juniSscClientSecondaryPort  OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The TCP port number of the secondary SSC server.  A value of zero
        indicates the port is unconfigured."
    ::= { juniSscClientCfgScalars 5 }

juniSscClientTertiaryAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The IP address of the tertiary SSC server.  A value of 0.0.0.0
        indicates the server address is unconfigured."
    ::= { juniSscClientCfgScalars 6 }

juniSscClientTertiaryPort  OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The TCP port number of the tertiary SSC server.  A value of zero
        indicates the port is unconfigured."
    ::= { juniSscClientCfgScalars 7 }

juniSscClientLocalAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The local IP address binding of the server connection.  A value of
        0.0.0.0 indicates the local address is unconfigured."
    ::= { juniSscClientCfgScalars 8 }

juniSscClientTransportRouterName  OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The name of the router to be used as the transport for the server
        connection."
    ::= { juniSscClientCfgScalars 9 }


--
-- Status objects
--
juniSscClientStatusScalars    OBJECT IDENTIFIER ::= { juniSscClientStatus 1 }

juniSscClientConnectionState  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disconnected(0),
                    trying(1),
                    connected(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The connection state of the SSC Client:
            disconnected    Not connected to a SSC server.
            trying          Attempting a connection to a server.
            connected       Connected to a server.

        When this object has the value 'connected', the active server address
        and TCP port are reported in juniSscClientActiveAddress and
        juniSscClientActivePort, respectively."
    ::= { juniSscClientStatusScalars 1 }

juniSscClientActiveAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address of the SSC server currently in use.  A value of 0.0.0.0
        indicates no server is in use."
    ::= { juniSscClientStatusScalars 2 }

juniSscClientActivePort  OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The TCP port number for the SSC server currently in use.  A value of
        zero indicates no server is in use."
    ::= { juniSscClientStatusScalars 3 }

juniSscClientVersion  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The version number for the SSC server currently in use."
    ::= { juniSscClientStatusScalars 4 }


--
-- Statistics Objects
--
juniSscClientStatisticsScalars  OBJECT IDENTIFIER
    ::= { juniSscClientStatistics 1 }

juniSscClientPolicyCommandsReceived  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of policy command packets received from the SSC."
    ::= { juniSscClientStatisticsScalars 1 }

juniSscClientPolicyCommandsListReceived  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of policy command packets received from the SSC with subtype
        LIST."
    ::= { juniSscClientStatisticsScalars 2 }

juniSscClientPolicyCommandsAcctReceived  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of policy command packets received from the SSC with subtype
        ACCOUTING."
    ::= { juniSscClientStatisticsScalars 3 }

juniSscClientBadPolicyCommandsReceived  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of policy command packets received from the SSC that
        included rules that were in error."
    ::= { juniSscClientStatisticsScalars 4 }

juniSscClientErrorPolicyCommandsReceived  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of policy command packets received from the SSC indicating
        an error from the SSC."
    ::= { juniSscClientStatisticsScalars 5 }

juniSscClientPolicyReportsSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of policy report packets sent to the SSC."
    ::= { juniSscClientStatisticsScalars 6 }

juniSscClientConnectionOpenRequests  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of connection open requests sent to the SSC."
    ::= { juniSscClientStatisticsScalars 7 }

juniSscClientConnectionOpenCompletes  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of connections to the SSC that open successfully."
    ::= { juniSscClientStatisticsScalars 8 }

juniSscClientConnectionClosedSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of connection close indications that were sent to the SSC."
    ::= { juniSscClientStatisticsScalars 9 }

juniSscClientConnectionClosedRemotely  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of connection close indications that were received from the
        SSC."
    ::= { juniSscClientStatisticsScalars 10 }

juniSscClientCreateInterfacesSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of interface creation indications that were sent to the SSC.
        This indicates the transition of an interface to an UP state."
    ::= { juniSscClientStatisticsScalars 11 }

juniSscClientDeleteInterfacesSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of delete interface indications that were sent to the SSC.
        This indicates the transition of an interface to an DOWN state."
    ::= { juniSscClientStatisticsScalars 12 }

juniSscClientActiveIpInterfaces  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of currently active IP interfaces that the SSC Client is
        aware of."
    ::= { juniSscClientStatisticsScalars 13 }

juniSscClientIpInterfaceTransitions  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of IP interface transitions that have been tracked by the
        SSC Client."
    ::= { juniSscClientStatisticsScalars 14 }

juniSscClientSynchronizesReceived  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of synchronization requests received from the SSC."
    ::= { juniSscClientStatisticsScalars 15 }

juniSscClientSynchronizeCompletesSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of synchronization complete packets sent to the SSC."
    ::= { juniSscClientStatisticsScalars 16 }

juniSscClientInternalErrors  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of internal errors tracked by the SSC Client."
    ::= { juniSscClientStatisticsScalars 17 }

juniSscClientCommunicationErrors  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of lower layer communication errors tracked by the SSC
        Client."
    ::= { juniSscClientStatisticsScalars 18 }

juniSscClientTokensSeen  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of tokens seen by the SSC client."
    ::= { juniSscClientStatisticsScalars 19 }

juniSscClientActiveTokens  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of tokens that the SSC client is currently aware of."
    ::= { juniSscClientStatisticsScalars 20 }

juniSscClientTokenTransitions  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of tokens transitions that have occurred."
    ::= { juniSscClientStatisticsScalars 21 }

juniSscClientCreateTokensSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of token creation indications that were sent to the SSC.
        This indicates the transition of a token to an UP state."
    ::= { juniSscClientStatisticsScalars 22 }

juniSscClientDeleteTokensSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of delete token indications that were sent to the SSC.  This
        indicates the transition of a token to an DOWN state."
    ::= { juniSscClientStatisticsScalars 23 }

juniSscClientActiveAddresses  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of addresses that the SSC client is currently aware of."
    ::= { juniSscClientStatisticsScalars 24 }

juniSscClientAddressTransitions  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of address transitions that have occurred."
    ::= { juniSscClientStatisticsScalars 25 }

juniSscClientCreateAddressesSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of address creation indications that were sent to the SSC.
        This indicates the transition of an address to an UP state."
    ::= { juniSscClientStatisticsScalars 26 }

juniSscClientDeleteAddressesSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of delete address indications that were sent to the SSC.
        This indicates the transition of an address to an DOWN state."
    ::= { juniSscClientStatisticsScalars 27 }

juniSscClientAuthenticationSuccesses  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of tokens which were authenticated successfully."
    ::= { juniSscClientStatisticsScalars 28 }

juniSscClientAuthenticationFailures  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of tokens which were not authenticated successfully."
    ::= { juniSscClientStatisticsScalars 29 }

juniSscClientDiscoversSeen  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of discovers seen by the SSC client."
    ::= { juniSscClientStatisticsScalars 30 }

juniSscClientActiveDiscovers  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of discovers that the SSC client is currently aware of."
    ::= { juniSscClientStatisticsScalars 31 }

juniSscClientDiscoverTransitions  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of discover transitions that have occurred."
    ::= { juniSscClientStatisticsScalars 32 }

juniSscClientCreateDiscoversSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of discover creation indications that were sent to the SSC."
    ::= { juniSscClientStatisticsScalars 33 }

juniSscClientDeleteDiscoversSent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of delete discover indications that were sent to the SSC."
    ::= { juniSscClientStatisticsScalars 34 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- juniSscClientTrapControl      OBJECT IDENTIFIER ::= { juniSscClientMIB 2 }
-- juniSscClientTraps            OBJECT IDENTIFIER ::= { juniSscClientMIB 3 }
-- juniSscClientTrapPrefix       OBJECT IDENTIFIER ::= { juniSscClientTraps 0 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniSscClientMIBConformance  OBJECT IDENTIFIER
    ::= { juniSscClientMIB 4 }
juniSscClientMIBCompliances  OBJECT IDENTIFIER
    ::= { juniSscClientMIBConformance 1 }
juniSscClientMIBGroups       OBJECT IDENTIFIER
    ::= { juniSscClientMIBConformance 2 }

--
-- compliance statements
--
juniSscClientAuthCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for authentication clients implementing
        the Juniper SSC Client MIB authentication functionality.  This statement
        became obsolete when DHCP-LS, Web and SSC support objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniSscClientGroup }
    ::= { juniSscClientMIBCompliances 1 }                          -- JUNOSe 2.0

juniSscClientAuthCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for authentication clients implementing
        the Juniper SSC Client MIB authentication functionality.  This statement
        became obsolete when the version number, local address and transport
        router name objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniSscClientGroup2 }
    ::= { juniSscClientMIBCompliances 2 }                          -- JUNOSe 3.1

juniSscClientAuthCompliance3 MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for clients implementing the Juniper SSC
        Client MIB functionality.  This statement became obsolete when token
        scalar statistics were obsoleted and discover scalar statistics were
        added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniSscClientGroup3 }
    ::= { juniSscClientMIBCompliances 3 }                          -- JUNOSe 4.0

juniSscClientAuthCompliance4 MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for clients implementing the Juniper SSC
        Client MIB functionality."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniSscClientGroup4 }
    ::= { juniSscClientMIBCompliances 4 }                          -- JUNOSe 5.3


--
-- units of conformance
--
juniSscClientGroup OBJECT-GROUP
    OBJECTS {
        juniSscClientServerSwitchoverTimeout,
        juniSscClientPrimaryAddress,
        juniSscClientPrimaryPort,
        juniSscClientSecondaryAddress,
        juniSscClientSecondaryPort,
        juniSscClientTertiaryAddress,
        juniSscClientTertiaryPort,
        juniSscClientActiveAddress,
        juniSscClientConnectionState,
        juniSscClientActivePort,
        juniSscClientPolicyCommandsReceived,
        juniSscClientPolicyCommandsListReceived,
        juniSscClientPolicyCommandsAcctReceived,
        juniSscClientBadPolicyCommandsReceived,
        juniSscClientErrorPolicyCommandsReceived,
        juniSscClientPolicyReportsSent,
        juniSscClientConnectionOpenRequests,
        juniSscClientConnectionOpenCompletes,
        juniSscClientConnectionClosedSent,
        juniSscClientConnectionClosedRemotely,
        juniSscClientCreateInterfacesSent,
        juniSscClientDeleteInterfacesSent,
        juniSscClientActiveIpInterfaces,
        juniSscClientIpInterfaceTransitions,
        juniSscClientSynchronizesReceived,
        juniSscClientSynchronizeCompletesSent,
        juniSscClientInternalErrors,
        juniSscClientCommunicationErrors }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of SSC Clients.
        This group became obsolete when DHCP-LS, Web and SSC support objects
        were added."
    ::= { juniSscClientMIBGroups 1 }                               -- JUNOSe 2.0

juniSscClientGroup2 OBJECT-GROUP
    OBJECTS {
        juniSscClientServerSwitchoverTimeout,
        juniSscClientPrimaryAddress,
        juniSscClientPrimaryPort,
        juniSscClientSecondaryAddress,
        juniSscClientSecondaryPort,
        juniSscClientTertiaryAddress,
        juniSscClientTertiaryPort,
        juniSscClientActiveAddress,
        juniSscClientConnectionState,
        juniSscClientActivePort,
        juniSscClientPolicyCommandsReceived,
        juniSscClientPolicyCommandsListReceived,
        juniSscClientPolicyCommandsAcctReceived,
        juniSscClientBadPolicyCommandsReceived,
        juniSscClientErrorPolicyCommandsReceived,
        juniSscClientPolicyReportsSent,
        juniSscClientConnectionOpenRequests,
        juniSscClientConnectionOpenCompletes,
        juniSscClientConnectionClosedSent,
        juniSscClientConnectionClosedRemotely,
        juniSscClientCreateInterfacesSent,
        juniSscClientDeleteInterfacesSent,
        juniSscClientActiveIpInterfaces,
        juniSscClientIpInterfaceTransitions,
        juniSscClientSynchronizesReceived,
        juniSscClientSynchronizeCompletesSent,
        juniSscClientInternalErrors,
        juniSscClientCommunicationErrors,
        juniSscClientTokensSeen,
        juniSscClientActiveTokens,
        juniSscClientTokenTransitions,
        juniSscClientCreateTokensSent,
        juniSscClientDeleteTokensSent,
        juniSscClientActiveAddresses,
        juniSscClientAddressTransitions,
        juniSscClientCreateAddressesSent,
        juniSscClientDeleteAddressesSent,
        juniSscClientAuthenticationSuccesses,
        juniSscClientAuthenticationFailures }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of SSC Clients.
        This group became obsolete when version number, local address and
        transport router name objects were added."
    ::= { juniSscClientMIBGroups 2 }                               -- JUNOSe 3.1

juniSscClientGroup3 OBJECT-GROUP
    OBJECTS {
        juniSscClientServerSwitchoverTimeout,
        juniSscClientPrimaryAddress,
        juniSscClientPrimaryPort,
        juniSscClientSecondaryAddress,
        juniSscClientSecondaryPort,
        juniSscClientTertiaryAddress,
        juniSscClientTertiaryPort,
        juniSscClientLocalAddress,
        juniSscClientTransportRouterName,
        juniSscClientActiveAddress,
        juniSscClientConnectionState,
        juniSscClientActivePort,
        juniSscClientVersion,
        juniSscClientPolicyCommandsReceived,
        juniSscClientPolicyCommandsListReceived,
        juniSscClientPolicyCommandsAcctReceived,
        juniSscClientBadPolicyCommandsReceived,
        juniSscClientErrorPolicyCommandsReceived,
        juniSscClientPolicyReportsSent,
        juniSscClientConnectionOpenRequests,
        juniSscClientConnectionOpenCompletes,
        juniSscClientConnectionClosedSent,
        juniSscClientConnectionClosedRemotely,
        juniSscClientCreateInterfacesSent,
        juniSscClientDeleteInterfacesSent,
        juniSscClientActiveIpInterfaces,
        juniSscClientIpInterfaceTransitions,
        juniSscClientSynchronizesReceived,
        juniSscClientSynchronizeCompletesSent,
        juniSscClientInternalErrors,
        juniSscClientCommunicationErrors,
        juniSscClientTokensSeen,
        juniSscClientActiveTokens,
        juniSscClientTokenTransitions,
        juniSscClientCreateTokensSent,
        juniSscClientDeleteTokensSent,
        juniSscClientActiveAddresses,
        juniSscClientAddressTransitions,
        juniSscClientCreateAddressesSent,
        juniSscClientDeleteAddressesSent,
        juniSscClientAuthenticationSuccesses,
        juniSscClientAuthenticationFailures }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of SSC Clients.
        This group became obsolete when token scalar statistics were obsoleted
        and discover scalar statistics were added."
    ::= { juniSscClientMIBGroups 3 }                               -- JUNOSe 4.0

juniSscClientGroup4 OBJECT-GROUP
    OBJECTS {
        juniSscClientServerSwitchoverTimeout,
        juniSscClientPrimaryAddress,
        juniSscClientPrimaryPort,
        juniSscClientSecondaryAddress,
        juniSscClientSecondaryPort,
        juniSscClientTertiaryAddress,
        juniSscClientTertiaryPort,
        juniSscClientLocalAddress,
        juniSscClientTransportRouterName,
        juniSscClientActiveAddress,
        juniSscClientConnectionState,
        juniSscClientActivePort,
        juniSscClientVersion,
        juniSscClientPolicyCommandsReceived,
        juniSscClientPolicyCommandsListReceived,
        juniSscClientPolicyCommandsAcctReceived,
        juniSscClientBadPolicyCommandsReceived,
        juniSscClientErrorPolicyCommandsReceived,
        juniSscClientPolicyReportsSent,
        juniSscClientConnectionOpenRequests,
        juniSscClientConnectionOpenCompletes,
        juniSscClientConnectionClosedSent,
        juniSscClientConnectionClosedRemotely,
        juniSscClientCreateInterfacesSent,
        juniSscClientDeleteInterfacesSent,
        juniSscClientActiveIpInterfaces,
        juniSscClientIpInterfaceTransitions,
        juniSscClientSynchronizesReceived,
        juniSscClientSynchronizeCompletesSent,
        juniSscClientInternalErrors,
        juniSscClientCommunicationErrors,
        juniSscClientActiveAddresses,
        juniSscClientAddressTransitions,
        juniSscClientCreateAddressesSent,
        juniSscClientDeleteAddressesSent,
        juniSscClientDiscoversSeen,
        juniSscClientActiveDiscovers,
        juniSscClientDiscoverTransitions,
        juniSscClientCreateDiscoversSent,
        juniSscClientDeleteDiscoversSent }
    STATUS      current
    DESCRIPTION
        "The basic collection of objects providing management of SSC Clients."
    ::= { juniSscClientMIBGroups 4 }                               -- JUNOSe 5.3

END
