-- This module defines enterprise MIBs for security zones
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-ZONE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenZone
        FROM NETSCREEN-SMI
    Integer32, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    ;

netscreenZoneMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines the object that are used to monitor all
         the security zones"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311130000Z" -- November 13, 2003
    DESCRIPTION
        "Correct spelling mistake"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "no comment"
    REVISION      "200005080000Z" -- May 08, 2000
    DESCRIPTION
        "Creation Date"
    ::= { netscreenZone 0 }

NsZoneCfgEntry ::= SEQUENCE
{
    nsZoneCfgId   Integer32,
    nsZoneCfgName DisplayString,
    nsZoneCfgType INTEGER,
    nsZoneCfgVsys Integer32
}

nsZoneCfg OBJECT IDENTIFIER ::= { netscreenZone 1 }

nsZoneCfgTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsZoneCfgEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "NetScreen device can have lots of secure zone. This table
         collects the zones exiting in NetScreen device."
    ::= { nsZoneCfg 1 }

nsZoneCfgEntry OBJECT-TYPE
    SYNTAX        NsZoneCfgEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each entry in the table holds a set of configuration
         parameters associated  with an instance of secure zone."
    INDEX
        { nsZoneCfgId }
    ::= { nsZoneCfgTable 1 }

nsZoneCfgId OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A unique value for zone table.  Its value ranges between 1 and
         65535 and may not be contiguous.  the index has no other
         meaning but a pure index"
    ::= { nsZoneCfgEntry 1 }

nsZoneCfgName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Secure zone name."
    ::= { nsZoneCfgEntry 2 }

nsZoneCfgType OBJECT-TYPE
    SYNTAX        INTEGER {
        regular(0),
        layer2(1),
        tunnel(2),
        null(3),
        func(4)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Secure zone type. Regular is sec(L3) and layer2 is sec(L2) type"
    ::= { nsZoneCfgEntry 3 }

nsZoneCfgVsys OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "VSYS this security zone belongs to."
    ::= { nsZoneCfgEntry 4 }
END


