FOUNDRY-SN-TRAP-MIB DEFINITIONS ::= BEGIN

-- Router Switch Trap MIB Release 1.0.0
-- Revision 06/02/97

-- Copyright 1996-1997 Foundry Networks, Inc.
-- All rights reserved.
-- This Foundry SNMP Management Information Base Specification
-- (Specification) embodies Foundry's confidential and
-- proprietary intellectual property. Foundry retains all
-- title and ownership in the Specification, including any
-- revisions.

-- This Specification is supplied "AS IS," and Foundry makes
-- no warranty, either express or implied, as to the use,
-- operation, condition, or performance of the Specification.

-- SECTION 1: Top Level Definitions


-- Imports


IMPORTS
   TRAP-TYPE              FROM RFC-1215
   foundry                FROM FOUNDRY-SN-ROOT-MIB
   snAgGblTrapMessage,
   snAgentBrdIndex,
   snChasPwrSupplyIndex,
   snChasPwrSupplyDescription,
   snChasFanIndex,
   snChasFanDescription   FROM FOUNDRY-SN-AGENT-MIB
   snL4TrapLinkName,
   snL4LinkVirtualInterface,
   snL4MaxSessionLimit,
   snL4TcpSynLimit,
   snL4TrapRealServerIP, 
   snL4TrapRealServerName,
   snL4TrapRealServerPort,
   snL4TrapRealServerCurConnections FROM FOUNDRY-SN-SW-L4-SWITCH-GROUP-MIB
   wgPnPIfIndex,
   wgPnPMacAddress,
   wgPnPStatus FROM FOUNDRY-SN-WIRELESS-GROUP-MIB;


-- Textual Conventions

-- Groups

-- SECTION 2: MIB Objects


-- Trap Information

-- These definitions use the TRAP-TYPE macro as defined in RFC 1215.

-- Foundry Networks, Inc. Specific Traps

-- Trap IDs 1 and 2 are not used now as they are obseleted.

-- Trap IDs from 3 through 18 are used by OSPF. See Router Trap mib for definitions.

snTrapL4MaxSessionLimitReached TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4MaxSessionLimit }
   DESCRIPTION
       "The SNMP trap that is generated when the maximum number
       of connections reached."
	--#TYPE "Foundry Trap: L4 Session Limit"
	--#SUMMARY "SLB maximum number of connections  %d has been reached."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 19


snTrapL4TcpSynLimitReached TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TcpSynLimit }
   DESCRIPTION
       "The SNMP trap that is generated when the number of TCP
       SYN limits reached."
	--#TYPE "Foundry Trap: L4 TCP Syn Limit"
	--#SUMMARY "SLB TCP Syn limits %d has been reached."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 20


snTrapL4RealServerUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TrapRealServerIP, snL4TrapRealServerName }
   DESCRIPTION
       "The SNMP trap that is generated when the load balancing
       real server is up."
	--#TYPE "Foundry Trap: L4 Real Server Up"
	--#SUMMARY "SLB real server %s %s is up."
	--#ARGUMENTS { 0, 1 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 21


snTrapL4RealServerDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TrapRealServerIP, snL4TrapRealServerName }
   DESCRIPTION
       "The SNMP trap that is generated when the load balancing
       real server is down."
	--#TYPE "Foundry Trap: L4 Real Server Down"
	--#SUMMARY "SLB real server %s %s is down."
	--#ARGUMENTS { 0, 1 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 22


snTrapL4RealServerPortUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TrapRealServerIP, snL4TrapRealServerName, snL4TrapRealServerPort }
   DESCRIPTION
       "The SNMP trap that is generated when the load balancing
       real server TCP port is up."
	--#TYPE "Foundry Trap: L4 Real Server Port Up"
	--#SUMMARY "SLB real server port %s %s %d is up."
	--#ARGUMENTS { 0, 1, 2 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 23


snTrapL4RealServerPortDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TrapRealServerIP, snL4TrapRealServerName, snL4TrapRealServerPort }
   DESCRIPTION
       "The SNMP trap that is generated when the load balancing
       real server TCP port is down."
	--#TYPE "Foundry Trap: L4 Real Server Port Down"
	--#SUMMARY "SLB real server port %s %s %d is down."
	--#ARGUMENTS { 0, 1, 2 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 24


snTrapL4RealServerMaxConnectionLimitReached TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TrapRealServerIP, snL4TrapRealServerName, snL4TrapRealServerCurConnections }
   DESCRIPTION
       "The SNMP trap that is generated when the real server reaches
       maximum number of connections."
	--#TYPE "Foundry Trap: L4 Real Server Max Connection Limit"
	--#SUMMARY "SLB real server %s %s maximum connection %d has been reached."
	--#ARGUMENTS { 0, 1, 2 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 25


snTrapL4BecomeStandby TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "The SNMP trap that is generated when the server load
       balancing switch changes state from active to standby."
	--#TYPE "Foundry Trap: L4 Server On Standby"
	--#SUMMARY "SLB changes state from active to standby."
	--#ARGUMENTS { }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 26


snTrapL4BecomeActive TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "The SNMP trap that is generated when the server load
       balancing switch changes state from standby to active."
	--#TYPE "Foundry Trap: L4 Server Active"
	--#SUMMARY "SLB changes state from standby to active."
	--#ARGUMENTS { }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 27


snTrapModuleInserted TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgentBrdIndex }
   DESCRIPTION
       "The SNMP trap that is generated when a module was inserted
       to the chassis during system running."
	--#TYPE "Foundry Trap: Module Inserted"
	--#SUMMARY "Module %d was inserted to the chassis during system running."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 28


snTrapModuleRemoved TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgentBrdIndex }
   DESCRIPTION
       "The SNMP trap that is generated when a module was removed
       from the chassis during system running."
	--#TYPE "Foundry Trap: Module Removed"
	--#SUMMARY "Module %d was removed from the chassis during system running."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 29


snTrapChasPwrSupplyFailed TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snChasPwrSupplyIndex, snChasPwrSupplyDescription }
   DESCRIPTION
       "The SNMP trap that is generated when a power supply fails
        to operate normally."
	--#TYPE "Foundry Trap: Power Supply Failure"
	--#SUMMARY "Power supply %d (%s)  failed."
	--#ARGUMENTS { 0, 1 }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 30


snTrapChasFanFailed TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snChasFanIndex, snChasFanDescription }
   DESCRIPTION
       "The SNMP trap that is generated when a fan fails
        to operate normally."
	--#TYPE "Foundry Trap: Fan Failure"
	--#SUMMARY "Fan  %d (%s)  failed."
	--#ARGUMENTS { 0, 1 }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 31


snTrapLockedAddressViolation2 TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when more source MAC addresses
        are received from a port than the maximum number of addresses
        configured to that port."
	--#TYPE "Foundry Trap: Lock Address Violation"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 32


snTrapFsrpIfStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a FSRP routing device
       changed state from active to standby or vice-versa."
	--#TYPE "Foundry Trap: FSRP Interface Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 33

snTrapVrrpIfStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a VRRP routing device
       changed state from master to backup or vice-versa."
	--#TYPE "Foundry Trap: VRRP Interface Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 34


snTrapMgmtModuleRedunStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the management module
       changes redundancy state."
	--#TYPE "Foundry Trap: Management Module Change State"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 35


snTrapTemperatureWarning TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the actual temperature
       reading is above the warning temperature threshold."
	--#TYPE "Foundry Trap: Temperature Warning"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY CRITICAL
	--#STATE OPERATIONAL
   ::= 36

snTrapAccessListDeny TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a packet was denied
       by an access list."
	--#TYPE "Foundry Trap: Deny from ACL"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 37

snTrapMacFilterDeny TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a packet was denied
       by a MAC address filter."
	--#TYPE "Foundry Trap: Deny from MAC Filter"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 38

snTrapL4GslbRemoteUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the connection to the remote SI is established."
	--#TYPE "Foundry Trap: Remote SI Up"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 39

snTrapL4GslbRemoteDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the connection to the remote SI is down."
	--#TYPE "Foundry Trap: Remote SI Down"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 40

snTrapL4GslbRemoteControllerUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the connection to the GSLB SI is established."
	--#TYPE "Foundry Trap: Remote GSLB SI Up"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 41

snTrapL4GslbRemoteControllerDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the connection to the GSLB SI is down."
	--#TYPE "Foundry Trap: Remote GSLB SI Down"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 42

snTrapL4GslbHealthCheckIpUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when GSLB health check for an address transitions
	   from down to active state."
	--#TYPE "Foundry Trap: GSLB HealtCheck Up"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 43

snTrapL4GslbHealthCheckIpDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when GSLB health check for an address transitions
	   from active to down state."
	--#TYPE "Foundry Trap: GSLB HealthCheck Down"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 44

snTrapL4GslbHealthCheckIpPortUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a given port for a health check address is up."
	--#TYPE "Foundry Trap: GSLB HealthCheck Port Up"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 45

snTrapL4GslbHealthCheckIpPortDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a given port for a health check address is down."
	--#TYPE "Foundry Trap: GSLB HealthCheck Port Down"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 46

snTrapL4FirewallBecomeStandby TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "The SNMP trap that is generated when the server load
       balancing switch Firewall changes state from active to standby."
	--#TYPE "Foundry Trap: Firewall Standby"
	--#SUMMARY "Firewall changes state from active to standby."
	--#ARGUMENTS { }
	--#SEVERITY MAJOR
	--#STATE OPERATIONAL
   ::= 47


snTrapL4FirewallBecomeActive TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "The SNMP trap that is generated when the server load
       balancing switch Firewall changes state from standby to active."
	--#TYPE "Foundry Trap: Firewall Active"
	--#SUMMARY "Firewall changes state from standby to active."
	--#ARGUMENTS { }
	--#SEVERITY MAJOR
	--#STATE OPERATIONAL
   ::= 48

snTrapL4FirewallPathUp TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "The SNMP trap that is generated when the server load
       balancing switch Firewall path is up."
	--#TYPE "Foundry Trap: Firewall Path Up"
	--#SUMMARY "Firewall path is up."
	--#ARGUMENTS { }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 49


snTrapL4FirewallPathDown TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "The SNMP trap that is generated when the server load
       balancing switch Firewall path is down."
	--#TYPE "Foundry Trap: Firewall Path Down"
	--#SUMMARY "Firewall path is down."
	--#ARGUMENTS { }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 50

snTrapIcmpLocalExceedBurst TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when incoming ICMP exceeds burst-MAX."
	--#TYPE "Foundry Trap: ICMP Burst Exceeded"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 51

snTrapIcmpTransitExceedBurst TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when transit ICMP exceeds burst-MAX."
	--#TYPE "Foundry Trap: Transit ICMP Burst Exceeded"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 52

snTrapTcpLocalExceedBurst TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when incoming TCP SYN exceeds burst-MAX."
	--#TYPE "Foundry Trap: TCP SYN Burst Exceeded"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 53

snTrapTcpTransitExceedBurst TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when transit TCP exceeds burst-MAX."
	--#TYPE "Foundry Trap: Transit TCP SYN Burst Exceeded"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 54

snTrapL4ContentVerification TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "The SNMP trap that is generated when the HTTP match-list pattern
       is found."
	--#TYPE "Foundry Trap: HTTP Match"
	--#SUMMARY "HTTP match-list pattern is found."
	--#ARGUMENTS { }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 55

snTrapDuplicateIp TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "Duplicate IP address detected."
	--#TYPE "Foundry Trap: Duplicate IP"
	--#SUMMARY "Duplicate IP address detect."
	--#ARGUMENTS { }
	--#SEVERITY MAJOR
	--#STATE OPERATIONAL
   ::= 56

snTrapMplsProblem TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "MPLS Problem Detected."
	--#TYPE "Foundry Trap: MPLS Problem"
	--#SUMMARY "MPLS Problem detect."
	--#ARGUMENTS { }
	--#SEVERITY MAJOR
	--#STATE OPERATIONAL
   ::= 57

snTrapMplsException TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "MPLS Exception Detected."
	--#TYPE "Foundry Trap: MPLS Exception"
	--#SUMMARY "MPLS Exception detect."
	--#ARGUMENTS { }
	--#SEVERITY MAJOR
	--#STATE OPERATIONAL
   ::= 58
   
snTrapMplsAudit TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "MPLS Audit Trap."
	--#TYPE "Foundry Trap: MPLS Audit"
	--#SUMMARY "MPLS Audit Trap."
	--#ARGUMENTS { }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 59
   
snTrapMplsDeveloper TRAP-TYPE
   ENTERPRISE foundry
   DESCRIPTION
       "MPLS Developer Trap."
	--#TYPE "Foundry Trap: MPLS Developer"
	--#SUMMARY "MPLS Developer Trap."
	--#ARGUMENTS { }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 60

snTrapNoBmFreeQueue TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when no free queue is available in buffer manager."
	--#TYPE "Foundry Trap: No BM Free Queue"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 61

snTrapSmcDmaDrop TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when SMC DMA packet is dropped."
	--#TYPE "Foundry Trap: SMC DMA Packet Dropped"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 62

snTrapSmcBpDrop TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when SMC BackPlane packet is dropped."
	--#TYPE "Foundry Trap: SMC BP Packet Dropped"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 63

snTrapBmWriteSeqDrop TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when BM write sequence packet is dropped."
	--#TYPE "Foundry Trap: BM Write Sequence Packet Dropped"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 64

snTrapBgpPeerUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the bgp peer is up."
	--#TYPE "Foundry Trap: BGP Peer Up"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 65

snTrapBgpPeerDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the bgp peer is down."
	--#TYPE "Foundry Trap: BGP Peer Down"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 66

snTrapL4RealServerResponseTimeLowerLimit TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the real server average response time exceeds lower threshold."
	--#TYPE "Foundry Trap: L4 Real Server Response Exceeds Lower Threshold"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 67

snTrapL4RealServerResponseTimeUpperLimit TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the real server average response time exceeds upper threshold."
	--#TYPE "Foundry Trap: L4 Real Server Response Exceeds Upper Threshold"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 68

snTrapL4TcpAttackRateExceedMax TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the TCP attack rate exceeds configured maximum."
	--#TYPE "Foundry Trap: L4 TCP Attack Rate Exceed Max"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY CRITICAL
	--#STATE OPERATIONAL
   ::= 69

snTrapL4TcpAttackRateExceedThreshold TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the TCP attack rate exceeds 80% of configured maximum."
	--#TYPE "Foundry Trap: L4 TCP Attack Rate Exceed Threshold"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 70

snTrapL4ConnectionRateExceedMax TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the L4 connection rate exceeds configured maximum."
	--#TYPE "Foundry Trap: L4 Connection Rate Exceed Max"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY CRITICAL
	--#STATE OPERATIONAL
   ::= 71

snTrapL4ConnectionRateExceedThreshold TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the L4 connection rate exceeds 80% of configured maximum"
	--#TYPE "Foundry Trap: L4 Connection Rate Exceed Threshold"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 72

snTrapRunningConfigChanged TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the running configuration
        was changed."
	--#TYPE "Foundry Trap: Running Configuration Changed"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 73

snTrapStartupConfigChanged TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the startup configuration
        was changed."
	--#TYPE "Foundry Trap: Startup Configuration Changed"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 74

snTrapUserLogin TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when user login."
	--#TYPE "Foundry Trap: User Login"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 75

snTrapUserLogout TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when user logout."
	--#TYPE "Foundry Trap: User Logout"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 76

snTrapPortSecurityViolation TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when insecure MAC addresses
        are received from a port with MAC security feature enabled."
	--#TYPE "Foundry Trap: Port Security Violation"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 77

snTrapPortSecurityShutdown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when insecure MAC addresses
        are received from a port caused the port to shutdown."
	--#TYPE "Foundry Trap: Port Security Violation Cause Shutdown"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 78

snTrapMrpStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a MRP switching and routing device
       changed state to  disabled, blocking, preforwarding, forwarding, uknown."
	--#TYPE "Foundry Trap: MRP Interface Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 79

snTrapMrpCamError TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a MRP Cam Error occurs."
	--#TYPE "Foundry Trap: MRP Cam Error"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 80

snTrapChasPwrSupplyOK TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snChasPwrSupplyIndex, snChasPwrSupplyDescription }
   DESCRIPTION
       "The SNMP trap that is generated when a power supply operational
        status changed from failure to normal."
	--#TYPE "Foundry Trap: Power Supply OK"
	--#SUMMARY "Power supply %d (%s)  OK."
	--#ARGUMENTS { 0, 1 }
	--#SEVERITY MINOR
	--#STATE OPERATIONAL
   ::= 81


snTrapVrrpeIfStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a VRRPE routing device
       switched between states master, backup, intialized or uknown."
	--#TYPE "Foundry Trap: VRRPE Interface Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 82

snTrapVsrpIfStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a VSRP switching and routing device
       switched between states master, backup, intialized or uknown."
	--#TYPE "Foundry Trap: VSRP Interface Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 83

snTrapSrcIpAddressViolation TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a rogue device spoofs source
       IP address for denial of service attack."
	--#TYPE "Foundry Trap: Intruder Source IP Address"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 84

snTrapMacAuthEnable TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when MAC-Authentication is enabled 
	    on an interface."
	--#TYPE "Foundry Trap: MAC-Authentication enabled"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 85

snTrapMacAuthDisable TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when MAC-Authentication is disabled 
	    on an interface."
	--#TYPE "Foundry Trap: MAC-Authentication disabled"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 86

snTrapMacAuthMACAccepted TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when MAC-Authentication is successful 
	    on an interface."
	--#TYPE "Foundry Trap: MAC-Authentication success"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 87

snTrapMacAuthMACRejected TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when MAC-Authentication is failed 
	    on an interface."
	--#TYPE "Foundry Trap: MAC-Authentication failure"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 88

snTrapMacAuthPortDisabled TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when an interface is disabled due to
	    MAC-Authentication detecting a DOS attack on that interface."
	--#TYPE "Foundry Trap: MAC-Authentication port disabled"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY CRITICAL
	--#STATE OPERATIONAL
   ::= 89

-- 90 through 103 are OSPFv3 traps

snTrapClientLoginReject TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a login attempt by a 
       telnet or SSH client fails."
	--#TYPE "Foundry Trap: Client Login Reject"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 110

snTrapLocalUserConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a local user configuration is changed."
	--#TYPE "Foundry Trap: Local User Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 111

snTrapVlanConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a vlan configuration is changed."
	--#TYPE "Foundry Trap: Vlan Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 112

snTrapAclConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a ACL configuration is changed."
	--#TYPE "Foundry Trap: ACL Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 113

snTrapMacFilterConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a MAC Filter configuration is changed."
	--#TYPE "Foundry Trap: MAC Filter Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 114

snTrapSNMPConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a SNMP configuration is changed."
	--#TYPE "Foundry Trap: SNMP Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 115

snTrapSyslogConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a Syslog configuration is changed."
	--#TYPE "Foundry Trap: Syslog Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 116

snTrapPasswordConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when enable or line password is changed."
	--#TYPE "Foundry Trap: Password Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 117

snTrapServerStatusChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a server is disabled or enabled."
	--#TYPE "Foundry Trap: Server Status Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 118

snTrapL4RealServerPortMaxConnectionLimitReached TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the real server's port reaches
       maximum number of connections."
	--#TYPE "Foundry Trap: L4 Real Server Port Max Connection Limit"
	--#SUMMARY "%s"
	--#ARGUMENTS { 0 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 119

snTrapL4LinkDown TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TrapLinkName, snL4LinkVirtualInterface }
   DESCRIPTION
       "The SNMP trap that is generated when the ISP link goes down."
	--#TYPE "Foundry Trap: L4 "
	--#SUMMARY "ISP Link %s bound to ve %d is down."
	--#ARGUMENTS { 0, 1 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 120

snTrapL4LinkUp TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snL4TrapLinkName, snL4LinkVirtualInterface }
   DESCRIPTION
       "The SNMP trap that is generated when the ISP link goes up."
	--#TYPE "Foundry Trap: L4 "
	--#SUMMARY "ISP Link %s bound to ve %d is up."
	--#ARGUMENTS { 0, 1 }
	--#SEVERITY WARNING
	--#STATE OPERATIONAL
   ::= 121

snTrapPortPriorityChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the priority of a port is changed."
	--#TYPE "Foundry Trap: Port Priority Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 122

snTrapAutoPortDisableTrigger TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when automatic port disable was triggered."
	--#TYPE "Foundry Trap: Automatic Port Disable Triggered "
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY ALERTS
	--#STATE OPERATIONAL
   ::= 123

snTrapAutoPortDisableRelease TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when automatic port disable was released."
	--#TYPE "Foundry Trap: Automatic Port Disable Released "
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY ALERTS
	--#STATE OPERATIONAL
   ::= 124

snTrapPnPStatusChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { wgPnPStatus, wgPnPStatus, snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when plug-and-play status change."
	--#TYPE "Foundry Trap: Plug-and-play Status Change "
	--#SUMMARY "Old Pnp status: %d, new Pnp status: %d, msg: %s."
	--#ARGUMENTS { 0, 1, 2 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 125

snTrapWirelessIsrpPeerStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when ISRP Peer changes state."
	--#TYPE "Foundry Trap: ISRP Peer's state has changed  "
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 126

snTrapWirelessStationStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a wireless station's state changes."
	--#TYPE "Foundry Trap: Wireless Station's state has changed."
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 127

snTrapWirelessStationRoamingEventTriggered TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when we received a MOVE request from
   the AP"
	--#TYPE "Foundry Trap: Station has roamed "
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 128

snTrapWirelessSappStateChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when SAPP between an AP and a FIPS
   changes state."
	--#TYPE "Foundry Trap: SAPP between AP and FIPS changes state. "
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 129

snTrapExternalPowerConnectionStatus TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when the external power supply
       connecting or disconnecting to a power over ethernet module."
	--#TYPE "Foundry Trap: External Power Supply Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY ALERTS
	--#STATE OPERATIONAL
   ::= 130

snTrapDot1xSecurityViolation TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a malicious mac
       address was detected."
	--#TYPE "Foundry Trap: 802.1x Security Violation"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY ALERTS
	--#STATE OPERATIONAL
   ::= 131

snTrapDot1xPortLinkChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when software port link status
       has changed to up or down."
	--#TYPE "Foundry Trap: 802.1x Port Link Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 132

snTrapDot1xPortControlChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when software port control status
       has changed to authorize or unauthorize."
	--#TYPE "Foundry Trap: 802.1x Port Control Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 133

snTrapDot1xVlanIdChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when VLAN ID of a port
       has changed."
	--#TYPE "Foundry Trap: 802.1x VLAN ID Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 134

snTrapDot1xFilterSetupFailure TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when software failed
       to setup a filter to a mac address of a port."
	--#TYPE "Foundry Trap: 802.1x Filter Setup Failure"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 135

snTrapDot1xError TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when software detected
       system error."
	--#TYPE "Foundry Trap: 802.1x Error"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY DEBUGGING
	--#STATE OPERATIONAL
   ::= 136

snTrapPortConfigChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when a port configuration is changed."
	--#TYPE "Foundry Trap: Port Config Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY INFORMATIONAL
	--#STATE OPERATIONAL
   ::= 137

snTrapMacAuthVlanIdChange TRAP-TYPE
   ENTERPRISE foundry
   VARIABLES { snAgGblTrapMessage }
   DESCRIPTION
       "The SNMP trap that is generated when VLAN ID of a port
       has changed."
	--#TYPE "Foundry Trap: MAC-Authentication VLAN ID Change"
	--#SUMMARY "%s."
	--#ARGUMENTS { 0 }
	--#SEVERITY NOTIFICATIONS
	--#STATE OPERATIONAL
   ::= 138

END