
-- *****************************************************************************
-- Juniper-Registry
--
-- Juniper Networks enterprise SNMP MIB.
--   Registry for the E-series edge router family of products.
--
-- Copyright (c) 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002-2004 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-Registry  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-IDENTITY
        FROM SNMPv2-SMI
    juniperUniAdmin
        FROM Juniper-UNI-SMI;

juniAdmin  MODULE-IDENTITY
    LAST-UPDATED "200412231158Z"  -- 23-Dec-04 06:58 AM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "Administratively assigned object identifiers for Juniper Networks
        E-series edge router products."
    -- Revision History
    REVISION    "200412231158Z"  -- 23-Dec-04 06:58 AM EST  - JUNOSe main
    DESCRIPTION
        "Updated for  the second generation E-series products."
    REVISION    "200312171925Z"  -- 17-Dec-03 02:25 PM EST  - JUNOSe 6.0
    DESCRIPTION
        "Added support for the second generation E-series products."
    REVISION    "200312171722Z"  -- 17-Dec-03 12:22 PM EST  - JUNOSe 5.3
    DESCRIPTION
        "Added 1G flash card."
    REVISION    "200211132038Z"  -- 13-Nov-02 03:38 PM EST  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         Added 512M flash card."
    REVISION    "200106012118Z"  -- 01-Jun-01 05:18 PM EDT  - JUNOSe 3.0
    DESCRIPTION
        "Initial version of this SNMP management information module."
    ::= { juniperUniAdmin 2 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Object identities for product family registries.
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniRegistry  OBJECT IDENTIFIER
--  STATUS      current
--  DESCRIPTION
--      "The root for administratively assigned object identifiers for Juniper
--      Networks cross-product objects."
    ::= { juniAdmin 1 }

juniErxRegistry  OBJECT IDENTIFIER
--  STATUS      current
--  DESCRIPTION
--      "The root for administratively assigned object identifiers for Juniper
--      Networks first generation E-series (ERX) edge router family products."
--  REFERENCE
--      "Actual values are defined in the Juniper-ERX-Registry module (in the
--      juniErxRegistry.mi2 file)."
    ::= { juniAdmin 2 }

juniES2Registry  OBJECT IDENTIFIER
--  STATUS      current
--  DESCRIPTION
--      "The root for administratively assigned object identifiers for Juniper
--      Networks second generation E-series edge router family products."
--  REFERENCE
--      "Actual values are defined in the Juniper-ES2-Registry module (in the
--      juniES2Registry.mi2 file)."
    ::= { juniAdmin 3 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--  Cross-product physical entity identifiers.
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniEntPhysicalType  OBJECT IDENTIFIER
--  STATUS      current
--  DESCRIPTION
--      "The OID values under juniEntPhysicalType are used by the SNMP agent in
--      the Juniper Networks edge router products as the AutonomousType values
--      for the entPhysicalVendorType varbinds for objects in the
--      entPhysicalTable."
    ::= { juniRegistry 1 }

--
-- PCMCIA Flash Cards
--
juniPcmciaFlashCard  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The vendor type ID for a standard PCMCIA flash card."
    ::= { juniEntPhysicalType 1 }

juni85MegT2FlashCard  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The vendor type ID for an 85 Megabyte Type II ATA PCMCIA flash card
        (Product Code: PCM-85)."
    ::= { juniPcmciaFlashCard 1 }

juni220MegT2FlashCard  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The vendor type ID for a 220 Megabyte Type II ATA PCMCIA flash card
        (Product Code: FLASH-220M)."
    ::= { juniPcmciaFlashCard 2 }

juni512MegT2FlashCard  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The vendor type ID for a 512 Megabyte Type II ATA PCMCIA flash card
        (Product Code: RX-FLASH512-FRU)."
    ::= { juniPcmciaFlashCard 3 }

juni1GigT2FlashCard  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The vendor type ID for a 1 Gigabyte Type II ATA PCMCIA flash card
        (Product Code: ERX-FLASH1GB-FRU)."
    ::= { juniPcmciaFlashCard 4 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--  Registration OIDs for Juniper Traceroute implementation types.
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniTraceRouteImplementationTypes  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The registration node (point) for Juniper Traceroute implementation
        types."
    REFERENCE
        "See DISMAN-TRACEROUTE-MIB.traceRouteCtlType (RFC2925) for how these
        objects are used."
    ::= { juniRegistry 2 }

juniTraceRouteUsingIcmpProbe  OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Indicates that an implementation is using ICMP probes to perform the
        trace-route operation."
    REFERENCE
        "DISMAN-TRACEROUTE-MIB.traceRouteCtlType (RFC2925)"
    ::= { juniTraceRouteImplementationTypes 1 }

END
