
-- *****************************************************************************
-- Juniper-IGMP-CONF
--
-- SNMP Agent Capabilities definitions for the IGMP MIBs.
--
-- Copyright (c) 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002-2006 Juniper Networks, Inc.
--   All rights reserved.
-- *****************************************************************************

Juniper-IGMP-CONF  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    juniAgents
        FROM Juniper-Agents;

juniIgmpAgent  MODULE-IDENTITY
    LAST-UPDATED "200608250540Z"  -- 25-Aug-06 12:40 AM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        E-mail: mib@Juniper.net"
    DESCRIPTION
        "The agent capabilities definitions for the Internet Group Management
        Protocol (IGMP) component of the SNMP agent in the Juniper E-series
        family of products."
    -- Revision History

    REVISION    "200608250540Z"  -- 25-Aug-06 12:40 AM EST  - JUNOSe 7.0
    DESCRIPTION
        "Added rsIgmpIfLocationType for support on REX platform and deprecated
         rsIgmpGroupsTable."
    REVISION    "200309291822Z"  -- 29-Sep-03 02:22 PM EDT  - JUNOSe 5.1
    DESCRIPTION
        "Juniper-IGMP-MIB:
         Added IGMP admin state support."
    REVISION    "200210281506Z"  -- 28-Oct-02 10:06 AM EST  - JUNOSe 5.0
    DESCRIPTION
        "Juniper-IGMP-MIB:
         Replaced Unisphere names with Juniper names.
         Added support for interface addresses and multicast group limits."
    REVISION    "200208292048Z"  -- 29-Aug-02 04:48 PM EDT  - JUNOSe 4.1
    DESCRIPTION
        "IGMP-STD-MIB:
         Added support for the IETF IGMP MIB (RFC 2933)."
    REVISION    "200103281720Z"  -- 28-Mar-01 12:20 PM EST  - JUNOSe 3.2
    DESCRIPTION
        "The initial release of this management information module."
    ::= { juniAgents 19 }


-- *****************************************************************************
-- IGMP SNMP Agent Capabilities definitions
-- *****************************************************************************
juniIgmpAgentV1  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 1 of the IGMP component of the JUNOSe SNMP agent.  This version
        of the IGMP component was supported in JUNOSe 3.0 thru 4.0 system
        releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIB supported by the SNMP agent for the IGMP application in JUNOSe.
        These capabilities became obsolete when support was added for the
        IGMP-STD-MIB (RFC 2933)."
    SUPPORTS    Juniper-IGMP-MIB
        INCLUDES {
            juniIgmpProxyInterfaceGroup,
            juniIgmpProxyCacheGroup }
    ::= { juniIgmpAgent 1 }

juniIgmpAgentV2  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 2 of the IGMP component of the JUNOSe SNMP agent.  This version
        of the IGMP component was supported in JUNOSe 4.1 and subsequent 4.x
        system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the IGMP application in
        JUNOSe.  These capabilities became obsolete when support was added to
        Juniper-IGMP-MIB for interface addresses and multicast group limits."
    SUPPORTS    IGMP-STD-MIB
        INCLUDES {
            igmpBaseMIBGroup,
            igmpRouterMIBGroup,
            igmpV2HostMIBGroup,
            igmpHostOptMIBGroup,
            igmpV2RouterMIBGroup,
            igmpV2ProxyMIBGroup }
        VARIATION   igmpCacheSelf
            ACCESS      read-only
            DESCRIPTION
                "This attribute is not supported on the JUNOSe system.  It will
                always get created with a value of false and can be read only.
                JUNOSe currently has no applications which join multicast
                groups."
    SUPPORTS    Juniper-IGMP-MIB
        INCLUDES {
            juniIgmpProxyInterfaceGroup,
            juniIgmpProxyCacheGroup }
    ::= { juniIgmpAgent 2 }

juniIgmpAgentV3  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 3 of the IGMP component of the JUNOSe SNMP agent.  This version
        of the IGMP component was supported in JUNOSe 5.0 system releases."
    STATUS      obsolete
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the IGMP application in
        JUNOSe.  These capabilities became obsolete when support was added to
        Juniper-IGMP-MIB for the administrative state object."
    SUPPORTS    IGMP-STD-MIB
        INCLUDES {
            igmpBaseMIBGroup,
            igmpRouterMIBGroup,
            igmpV2HostMIBGroup,
            igmpHostOptMIBGroup,
            igmpV2RouterMIBGroup,
            igmpV2ProxyMIBGroup }
        VARIATION   igmpCacheSelf
            ACCESS      read-only
            DESCRIPTION
                "This attribute is not supported on the JUNOSe system.  It will
                always get created with a value of false and can be read only.
                JUNOSe currently has no applications which join multicast
                groups."
    SUPPORTS    Juniper-IGMP-MIB
        INCLUDES {
            juniIgmpProxyInterfaceGroup,
            juniIgmpProxyCacheGroup,
            juniIgmpInterfaceGroup,
            juniIgmpGroupsGroup }
    ::= { juniIgmpAgent 3 }

juniIgmpAgentV4  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 4 of the IGMP component of the JUNOSe SNMP agent.  This version
        of the IGMP component is supported in JUNOSe 5.1 and subsequent system
        releases."
    STATUS      deprecated
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the IGMP application in
        JUNOSe."
    SUPPORTS    IGMP-STD-MIB
        INCLUDES {
            igmpBaseMIBGroup,
            igmpRouterMIBGroup,
            igmpV2HostMIBGroup,
            igmpHostOptMIBGroup,
            igmpV2RouterMIBGroup,
            igmpV2ProxyMIBGroup }
        VARIATION   igmpCacheSelf
            ACCESS      read-only
            DESCRIPTION
                "This attribute is not supported on the JUNOSe system.  It will
                always get created with a value of false and can be read only.
                JUNOSe currently has no applications which join multicast
                groups."
    SUPPORTS    Juniper-IGMP-MIB
        INCLUDES {
            juniIgmpProxyInterfaceGroup,
            juniIgmpProxyCacheGroup,
            juniIgmpInterfaceGroup2,
            juniIgmpGroupsGroup }
    ::= { juniIgmpAgent 4 }


juniIgmpAgentV5  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 5 of the IGMP component of the JUNOSe SNMP agent.  This version
        of the IGMP component is supported in JUNOSe 7.0 and subsequent system
        releases."
    STATUS      current
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the IGMP application in
        JUNOSe."
    SUPPORTS    IGMP-STD-MIB
        INCLUDES {
            igmpBaseMIBGroup,
            igmpRouterMIBGroup,
            igmpV2HostMIBGroup,
            igmpHostOptMIBGroup,
            igmpV2RouterMIBGroup,
            igmpV2ProxyMIBGroup }
        VARIATION   igmpCacheSelf
            ACCESS      read-only
            DESCRIPTION
                "This attribute is not supported on the JUNOSe system.  It will
                always get created with a value of false and can be read only.
                JUNOSe currently has no applications which join multicast
                groups."
    SUPPORTS    Juniper-IGMP-MIB
        INCLUDES {
            juniIgmpProxyInterfaceGroup,
            juniIgmpProxyCacheGroup,
            juniIgmpInterfaceGroup2,
            juniIgmpGroupsGroup2 }
    ::= { juniIgmpAgent 5 }

END
